0       RakeshRao
1       January
2       February
3       March
4       April
5       May
6       June
7       July
8       August
9       September
10      October
11      November
12      December
13      Successfully read GeoTools registration information...
14      The trial or subscription period for registering GeoTools was from
15      to
16      of
17      You have reached the maximum number of
18      times this command can be
19      used in a single CAD session before it needs to be registered.
20      GeoTools notification
21      GeoTools Registration Notice
22      Thank you for your interest in GeoTools software.
23      This is a 30-day evaluation copy of GeoTools.
24      All users are required to register GeoTools within 30 days
25      of purchase to receive the required registration files
26      needed to run the software beyond the 30-day period.
27      Please refer to your documentation 'Register_GeoTools.Txt' on how
28      to register GeoTools.
29      be used before it needs to be registered and this program has expired.
30      or you can run this program for
31      times from now whichever is earlier.
32      Thank you for downloading this evaluation copy of GeoTools
33      You may run this evaluation copy for 30 days or
34      whichever happens earlier. If you have not finished the evaluation
35      and would like to extend it, please let us know and we can
36      provide you with an extended period evaluation license.
37      GeoTools can be purchased online through our website at
38      the following URL:
39      Once you purchase GeoTools, your order will be shipped to
40      you by airmail within 2 working days.
41      is
42      done.
43      and

;; Generic messages and prompts
5000    Enter Layers to process(or . to select):
5001    Processing objects
5002    objects stored in active [previous] selection set
5003    objects processed, NOT placed in active selection, exceeds
5004    objects ignored.
5005    objects processed.
5006    3dfaces ignored.
5007    objects found matching selection criteria.
5008    3dfaces processed.
5009    Invalid citerion.
5010    Block attribute
5011    not found in block
5012    Processing block objects...
5013    polylines ignored
5014    polylines processed.
5015    Processing
5016    Program
5017    Loading
5018    application
5019    frozen
5020    locked
5021    turned off
5022    turned on
5023    Extracted
5024    Height
5025    Layer
5026    Field Name
5027    with
5028    Displaying
5029    on layer
5030    Save
5031    Restore
5032    removed
5033    ignored
5034    drawings selected.
5035    Select DWG files
5036    Error:
5037    failed.
5038    successful
5039    not successful
5040    Select objects [or ENTER to type layer name(s)]:
5041    Enter Layer-name(s) to process(separated by commas):

10000   Convert 0 length LINEs and POLYLINEs to POINTs.
10001   All linear objects shorter than
10002   will be converted to point objects.
10003   objects processed and new points created.
10004   Converts 3DFACE to a 3D polyface mesh with elevations of each 3DFACE vertex.
10005   Building 3DFACE points list...
10006   Defining polyface points...
10007   Defining polyface connectivity relationships...
10008   Converts 3DFACE to a 3D Polyline with elevations of each 3DFACE vertex.
10009   Converting 3DFACEs to 3D polylines
10010   newly created polylines stored in active [previous] selection set
10011   new polylines created, NOT placed in active selection, exceeds
10012   Filter 3DFACE objects based on their perimeter/area values
10013   Select filter criteria:
10014   Horizontal [projected] area      : HArea
10015   Inclined   [slope]     area      : IArea
10016   Horizontal [projected] perimeter : HPerimeter
10017   Inclined   [slope]     perimeter : IPerimeter
10018   Redundant  [duplicate] vertex    : RedVertex
10019   Filter what property?
10020   Enter value condition to check
10021   Improper syntax. Must be in the format like
10022   Checking 3dfaces,
10023   Do you want to turn into one? <Y>:
10024   Select 3Dpolyline:
10025   Object selected is not a 3D polyline.
10026   Select objects to join.
10027   segment
10028   added to polyline
10029   Compute the horizontal angle between two lines.
10030   Select first line:
10031   Select second line:
10032   The two angles [acute & obtuse] between the line segments are
10033   Cannot compute angle between the two lines.
10034   Selected object is not a line or polyline.
10035   Select objects for assigning properties:(POINTs/SHAPEs/BLOCKs/CIRCLEs):
10036   Specify search distance around insertion point:
10037   Assign What property?
10038   Inherit property from:
10039   Enter attribute tag name to inherit property value:
10040   Performing a ZOOM EXTENTS for full view.
10041   Pick reference contour:
10042   Enter Reference Elevation:
10043   Reference elevation
10044   Enter contour interval with sign
10045   Pick adjoining contour in order
10046   This contour has already been picked.
10047   Only 2d polylines can be picked as contours
10048   Only polylines can be picked as contours.
10049   Only 2d polylines can be selected as reference contours.
10050   Transfer Block Attributes to AutoCAD Map Object table data.
10051   Enter block name to transfer attributes from:
10052   Enter object table name to populate:
10053   Blocks transfer mode
10054   Perform automatic transfer of identical attribute and object data fields?
10055   Type the AOD command to manually transfer block attribute data.
10056   There are no Object Data Tables in this drawing.
10057   There are no blocks with attributes in this drawing.
10058   This command can be run only within AutoCAD Map.
10059   Transferring Block Attributes to Object Table Data
10060   1 Object ignored. Block does not contain required attributes
10061   Object table records transferred.
10062   [Block with Attribute]:Select object:
10063   [Target Object Data]:Select object:
10064   Attribute data transfer was successful.
10065   Attribute data transfer was not successful.
10066   Only
10067   blocks can be selected to export attribute data.
10068   Selected object is not a block.
10069   Please run the ATT2OD command first to set the transfer parameters.
10070   Multiple association of Attribute->Object Table is not allowed.
10071   is already linked.
10072   Please select an attribute and an Object Table first.
10073   is not linked.
10074   Registered to
10075   There are no similar Attribute->Field names
10076   You have not made any Attribute->Object table mapping
10077   Transfer block attributes between objects.
10078   Enter name of source attribute tag to transfer (or . for none)
10079   Enter name of target attribute tag to transfer to (or . for none)
10080   Perform automatic transfer of common attributes?
10081   Type GT_AX to start the attribute transfer command directly.
10082   Select source block:
10083   Selected block:
10084   This block has no attributes.
10085   Layer name:
10086   You picked the same block twice.
10087   does not exist
10088   Source Block:
10089   Target Block:
10090   transferred to
10091   Error: Attribute could not be transferred. Layer may be locked.
10092   Common attributes between source and target blocks:
10093   There are no common attributes in source and target blocks.
10094   Select target block:
10095   Create automatic dimensions at all intersections with lines.
10096   From point:
10097   To point:
10098   Pick dimension line location:
10099   No intersections with LINE objects found.
10100   Convert object properties from 'BYLAYER' to 'BYENTITY'
10101   Converting object properties...
10102   does not contain any attributes.
10103   Current block: (none)
10104   No block selected
10105   Edit Block graphics and attribute properties independently
10106   Create a POINT at every BLOCK/SHAPE/TEXT location.
10107   Select INSERTs/SHAPEs/TEXTs to convert:
10108   Deleting original SHAPEs/INSERTs/TEXTs...
10109   Cannot open GeoTools online user-manual
10110   Cannot find 'GeoTools.VLX' file to determine installation folder
10111   Last GeoTools selection is empty.
10112   GeoTools is a product of DesignSense Software Technologies Pvt. Ltd..
10113   GeoTools Version
10114   Contact:
10115   About GeoTools
10116   cannot be found.
10117   GeoTools Readme & installation instructions
10118   Select contour polyline:
10119   Pick insertion point:
10120   Pick insertion point to insert
10121   Please select a block first.
10122   Checking line ends...
10123   [Ignored - More than one crossing object]
10124   Osnap cover could not be set.
10125   Select a polyline:
10126   Bulge at vertex
10127   and Radius is
10128   Bulge not found at Vertex #
10129   Select POLYLINEs,SPLINEs,CIRCLEs to compute total areas:
10130   Totaling areas, please wait...
10131   The total cumulative area of
10132   processed objects is
10133   Digitize Road Center Lines from Rights-Of-Way
10134   Pick Start point of line:
10135   First zig-zag point:
10136   Intersection Solver Failed.
10137   Fence is empty
10138   Manual mode entered: Next digitized point WILL be used as a CENTERLINE point.
10139   Manual mode exited: Next digitized point WILL NOT be used as a CENTERLINE point.
10140   Next point WILL be used for boundary calculation.
10141   Next point WILL NOT be used for boundary calculation.
10142   No solution [Distance from point too short]
10143   All segments already undone.
10144   Compute centroid of a polygon area[must be closed POLYLINEs, REGION or 3DSOLID]
10145   Select a POLYLINE, REGION or 3DSOLID:
10146   Select 2D POLYLINEs to convert to 3D polylines.
10147   Converting POLYLINEs from 2d to 3d...
10148   1 Polyline with ARC segments found and ignored
10149   Select 3D POLYLINEs and/or 3D Lines to convert to 2D.
10150   Set target elevation with:
10151   Store original vertex elevations in 2d polylines?
10152   ** WARNING **
10153   The converted 2D polylines created will acquire new handles but will retain any existing Xdata and object table data.
10154   Select 3d polylines for creating cross-sectional profiles:
10155   Error: This is a 3D mesh polyline. This cannot be used for cross-section profiling.
10156   Error: This is a 3D polyface polyline. This cannot be used for cross-section profiling.
10157   Error: This is a fitted polyline. This cannot be used for cross-section profiling. Please decurve it first.
10158   Error: This is a splined polyline. This cannot be used for cross-section profiling. Please decurve it first.
10159   Warning: This is a 2D Polyline. You will get a flat profile.
10160   Do you wish to continue?
10161   Error: Selected object is not a Polyline.
10162   Error: Profile Interval cannot be greater than annotation interval.
10163   Error: Annotation Interval cannot be less than profile interval.
10164   Save profile parameters as ASCII file
10165   Restore profile parameters from ASCII file
10166   Computing statistics, please wait...
10167            P O L Y L I N E   S T A T I S T I C S
10168   Number of vertices   :
10169   Minimum X coordinate :
10170   Minimum Y coordinate :
10171   Minimum Z coordinate :
10172   Maximum X coordinate :
10173   Maximum Y coordinate :
10174   Maximum Z coordinate :
10175   Slope Length         :
10176   Horizontal Length    :
10177   Profile polyline statistics
10178   Select layer for TIN triangles
10179   Pick insertion point of profile
10180   Chainages and elevation written into file:
10181   Profile creation terminated.
10182   Creating Interpolated profile...
10183   Reference Height :
10184   Profile Sampling interval :
10185   Profile Annotation interval :
10186   Chainages printed are slope distances
10187   Chainages printed are horizontally projected distances
10188   Route Name
10189   Vertical Exaggeration Factor
10190   Creating Interpolated profile...
10191   This POLYLINE is too short for profiling.
10192   Creating source points profile...
10193   Error: Cannot open output file:
10194   Polylines crossing profile is not implemented yet.
10195   Unsupported entity type for crossing.
10196   Cross
10197   Point features include points, blocks and shape objects.
10198   Linear features include lines, polylines and spline objects.
10199   Program Operation Mode:
10200   Object type to process:
10201   Enter extract file name:
10202   Delimiter to use between fields (type . to use SPACE as delimiter)
10203   Add point numbering for the coordinate records?
10204   Begin new point numbering for each new linear record?
10205   Exporting objects...
10206   Writing output file
10207   for export
10208   Scanning input file...
10209   Error: Unable to read import file
10210   Processing...
10211   Attribute transfer successful.
10212   Attribute transfer failed.
10213   Object Data transfer successful.
10214   Object Data transfer NOT successful.
10215   Created output file
10216   Input string:
10217   does not match the
10218   format
10219   Error: Attribute tag
10220   could not be read from block
10221   Enter
10222   data file
10223   Please select an object table field name.
10224   Please select an object table name.
10225   Please enter an attribute tag name
10226   Select PolyLine for chainage annotation:
10227   Error: This is a 3D mesh polyline. This cannot be used for chainage annotation.
10228   Error: This is a 3D polyface polyline. This cannot be used for chainage annotation.
10229   Error: This is a fitted polyline. This cannot be used for chainage annotation. Please decurve it first.
10230   Error: This is a splined polyline. This cannot be used for chainage annotation. Please decurve it first.
10231   Pre-processing polyline for annotation...
10232   Reading chainage description file...
10233   Creating chainage descriptions
10234   Import chainage descriptions ASCII file
10235   Save annotation parameters as ASCII file
10236   Restore annotation parameters from ASCII file
10237   Chainage polyline statistics
10238   Compute Layer Statistics
10239   Compute Object [entity] Statistics
10240   Compute Block Statistics
10241   Compute Symbol Table Statistics
10242   Select objects to compute statistics:
10243   Enter drawing statistics filename:
10244   Drawing Statistics of
10245   --------------------Objects [entity] Information----------------------
10246   Selection criteria used
10247   Object Names
10248   Layer Names
10249   Block Names
10250   Number of
10251   objects
10252   Lowest Z value of
10253   Highest Z value of
10254   Total number of vertices in all POLYLINEs
10255   The following objects were not found in this drawing
10256   --------------------Symbol Table Information----------------------
10257   Drawing Statistics written to file :
10258   Cannot open output report file
10259   for writing.
10260   Please check your file permissions.
10261   Custom AutoCAD Objects
10262   -------------------Detailed Layer Information---------------------
10263   Layer Name                Visibility      Lock/Unlock     Color     Linetype    Lineweight      Transperancy     PlotStyle   Plot   Num-of-Objects
10264   NOT COMPUTED
10265   -------Detailed BLOCKs(INSERTs) Information (includes dynamic blocks, if present)-------
10266   BLOCK Name                                       Number
10267   -----------------------Detailed Text Style information------------------
10268   Text STYLE Names defined in this drawing
10269   Define CADPower macros.
10270   Define CADPower command macros (will overwrite any existing macro definitions)?
10271   objects deleted from GeoTools temporary layer
10272   GeoTools temporary layer
10273   is empty or has not yet been created.
10274   VBA application to unload(or ? to browse)
10275   Select VBA application to unload
10276   BLIPS turned on.
10277   BLIPS turned off.
10278   Enter Autolisp function for which you need help:
10279   Move UCS Origin.
10280   Pick new origin of UCS:
10281   Object snap mode set to NONe.
10282   Object snap mode set to END.
10283   Object snap mode set to INTersection.
10284   Object snap mode set to MIDpoint.
10285   Object snap mode set to NEArest.
10286   Object snap mode set to PERpendicular.
10287   Object snap mode set to QUADrant.
10288   Object snap mode set to CENter.
10289   File already exists. Overwrite?
10290   WBLOCKing into
10291   Enter Block or drawing name:
10292   Insert BLOCK or DWG at 0,0,0 with Scl=1
10293   WBLOCK part of DWG with Insertion @ 0,0,0
10294   Enter drawing name:
10295   Create drawing file
10296   Horizontal & Slope distance with dX and dY components.
10297   First point:
10298   Second point:
10299   Slope (actual) distance =
10300   Horiz.Projected dist =
10301   Length along X & Y axes, dX =
10302   Delete contents of a layer.
10303   Layer name to delete (RETURN to select):
10304   Select object on layer to delete [ENTER to select layer]:
10305   is locked.
10306   Cannot delete objects from locked layers.
10307   objects deleted from layer:
10308   is already empty.
10309   does not exist.
10310   Select object to query:
10311   Object Type=
10312   Pick first corner:
10313   Specify Length & Rotation:
10314   Specify breadth:
10315   Enter new value for SURFTAB1
10316   Enter new value for SURFTAB2
10317   Enter new value for SURFU
10318   Enter new value for SURFV
10319   Easy create 3D point objects
10320   Pick X,Y location of point:
10321   Enter point elevation
10322   Pick point on curve to draw perpendicular from:
10323   Draw a rectangle with diagonals.
10324   Pick other corner:
10325   Select object to set current layer (ENTER to select from list):
10326   Current layer set to:
10327   Select polyline:
10328   Temporarily setting Osnap mode set to ENDpoint.
10329   Pick vertex to delete [ (U)ndo / e(X)it ]:
10330   deleted.
10331   Picked point does not fall on a polyline vertex.\nUse OSNAP for accurate snapping.
10332   Pick a position to insert vertex [ (U)ndo / e(X)it ]:
10333   Vertex at :
10334   added.
10335   CADPower command shortcut macros defined.
10336   not found in current search path.
10337   Select AutoLisp application to load
10338   Select ARX application to load
10339   Select VBA application to load
10340   Snap criteria application
10341   Snap Mode
10342   Vertical tolerance for source-target Z snap
10343   Snap to target object in existing selection only?
10344   Select objects to process:
10345   GT_NODELINESNAP - Snaps (joins) all loose ends of lines and nearby points.
10346   For correct results, please keep ONLY required layers on and visible.
10347   Snapping linear objects....
10348   Snapping node objects....
10349   ** GT_NODELINESNAP ** statistics
10350   Maximum Vertex shift:
10351   Minimum Vertex shift:
10352   Average Vertex shift:
10353   Osnap Object box could not be set. Please call technical support with this drawing details.
10354   Select [LINE,POLYLINE,ARC,3DFACE] objects.
10355   Label with
10356   Select bearing format
10357   Label position with ref. to segments
10358   Label position with ref. to reading direction. Always
10359   Pre-processing polylines...
10360   Enter a BLOCK name to edit
10361   Attribute Tag names in this block.
10362   Specify attribute [tag] names to extract separated by commas
10363   Current Block:
10364   Select a BLOCK object:
10365   No attribute has been selected for editing.
10366   GeoTools discontinued command. Please use 'GT_ModTxt' command instead.
10367   GeoTools discontinued command. Please use the 'GT_MRedefine' command instead.
10368   GeoTools discontinued command. Please use the 'GT_NodeLineSnap' command instead.
10369   GeoTools discontinued command. Please use the 'GT_TanCurve' command instead.
10370   This command is not yet implemented in the current version.
10371   Select what type?
10372   Enter filter criteria for
10373   Invalid
10374   filter citeria.
10375   Only polylines which are actually closed with a CLOSED flag will be identified.
10376   3D Polylines with different Z will be projected to 0.0.
10377   All polylines with at-least one vertex Z value matching the criteria will be selected.
10378   Only polylines whose first segment width matches the given value will be identified.
10379   Offset and remove original object.
10380   Select object to offset:
10381   Pick side to offset:
10382   Offset closed polyline objects INwards or OUTwards.
10383   Offset direction:
10384   Horizontal Offset distance:
10385   1 3d polyline cannot be offset and has been ignored.
10386   Offsetting polylines,
10387   Start and/or End Date/time markers are not set.
10388   There are a total of
10389   objects in this selection.
10390   Split selection mode
10391   Enter number of objects to place in each selection
10392   Enter number of equal divisions to make
10393   Highlight a layer[turns all others off]
10394   Select layer [ENTER to select from a list]:
10395   Select first object:
10396   Select second object:
10397   Join all segments together?
10398   Object must be either line,polyline,arc or spline.
10399   Select an object [A to set xdata Application names]:
10400   Enter XData application names separated by commas
10401   XData of application
10402   is empty.
10403   Select object at break point:
10404   Break object at picked point.
10405   Copy from Source to Destination layer
10406   Enter source layer name
10407   Enter destination layer name
10408   objects copied to layer:
10409   Source Layer:
10410   Change selected objects to current layer.
10411   Change to current layer.
10412   Copy to current layer.
10413   Copy and Rotate.
10414   Move and Rotate.
10415   <Base point or displacement>:
10416   <Second point of displacement>:
10417   Enter base point of rotation
10418   Create ARC ASCII DEM files from AutoCAD data.
10419   Enter source coordinate system identification string
10420   Source coordinate system successfully set to
10421   Enter destination coordinate system identification string
10422   Source destination system successfully set to
10423   Error: Source coordinate system could not be set to
10424   Error: Destination coordinate system could not be set to
10425   Enter DEM resolution
10426   Enter nodata value
10427   Enter DEM ASCII file name:
10428   Enter rubber-sheeting script file name
10429   Enter minimum elevation
10430   Enter maximum elevation
10431   Pick lower left corner [must be a POINT/AECC_POINT object]:
10432   Pick upper right corner [must be a POINT/AECC_POINT object]:
10433   Lower Left corner point not found
10434   Upper Right corner point not found
10435   Do you want to include the header info in the output file?
10436   Total number of rows    :
10437   Total number of columns :
10438   Enter starting row number
10439   Starting row RESET to 1.
10440   AutoLISP program to Load(~ or ? to browse)
10441   ARX application to Load(~ or ? to browse)
10442   VBA application to Load(~ or ? to browse)
10443   New thickness:
10444   Change thickness of selected objects.
10445   New elevation:
10446   Change elevation of selected objects.
10447   New Linetype[must be loaded already]:
10448   Change linetype of selected objects.
10449   New Color:<ENTER to select from color pallete>:
10450   Change color of selected objects.
10451   objects changed to layer:
10452   Do you want to create it?
10453   Enter target layer name:
10454   Select object on desired layer[or ENTER to type layer name]:
10455   Change selected objects to another layer.
10456   Enter New Layer name:
10457   Thawing all the layers...
10458   Turning on all the layers...
10459   Freezing all the layers except current layer...
10460   Turning off all layers except current layer...
10461   is the current layer and cannot be frozen.
10462   [current layer] is already thawed & on.
10463   thawed & turned on.
10464   is the current layer and cannot be locked.
10465   Number of Used styles =
10466   Number of UnUsed styles =
10467   Report of all fonts used in this drawing created in
10468   Select TEXT [from top to bottom sequence]:
10469   Pick Insertion point of MTEXT:
10470   Pick new start point of the polyline:
10471   The new start point picked does not lie on an existing polyline vertex.
10472   Selected polyline contains ARC segments. Only linear polylines can be used here.
10473   Selected polyline is not a closed polyline. Only closed polylines can have their start point changed.
10474   Selected object is not a polyline.
10475   Determine polyline direction.
10476   This is a clockwise polyline.
10477   This is a counter clockwise polyline.
10478   Error: Direction cannot be determined.
10479   is the current layer and cannot be turned off.
10480   is the current layer and already on.
10481   Enter layer names separated by commas[wildcards accepted]:
10482   Select layer to freeze [ENTER to type name(s)]:
10483   Select layer(s) to thaw [ENTER to type name(s)]:
10484   Select layer to turn on [ENTER to type name(s)]:
10485   Select layer to turn off [ENTER to type name(s)]:
10486   Select layer to lock [ENTER to type name(s)]:
10487   Join two lines by extension to their intersection.
10488   Enter Pan Factor as % of screen
10489   Pan RightWards
10490   Pan Leftwards
10491   Pan Downwards
10492   Pan Upwards
10493   Set SURFU and SURFV
10494   Set SURFTAB1 and SURFTAB2
10495   Query an object
10496   There is a current selection set of
10497   No current selection set exists.
10498   objects appended to existing selection set of
10499   New current selection set has
10500   Scanning TEXT objects...
10501   Erasing
10502   null TEXT objects...
10503   There are no null text objects in this drawing.
10504   There are no TEXT objects in this drawing.
10505   objects removed from existing selection set of
10506   New current selection set has
10507   There are no objects in current selection set.
10508   Scanning drawing file...
10509   Current selection filter will be applied to this selection.
10510   Current Object selection: 
10511   Current Layer selection: 
10512   is not a valid object type for this selection
10513   is not a valid layer name for this selection
10514   is not a valid block name for this selection
10515   Block name:
10516   Current Object selection :
10517   Current Layer selection :
10518   Select 2D POLYLINEs/LINEs/ARCs to join [or ENTER to select by layers]:
10519   Objects have to be touching each other in order to be joined successfully.
10520   Height
10521   Relative Rotate (degrees)
10522   Absolute Rotate (degrees)
10523   Style
10524   Justification
10525   Value Increment
10526   Value Decrement
10527   Value Set
10528   Add prefix.
10529   Add Suffix
10530   Trim characters from start.
10531   Trim characters from end.
10532   Specify option:
10533   Enter new text height
10534   Enter angle by which to rotate relative selected objects(ccw +ve / cw -ve)
10535   New rotation angle for selected objects(ccw +ve / cw -ve)
10536   Select a TEXT style to set for selected objects
10537   Enter Text justification to set
10538   Enter numeric amount to increment
10539   Enter numeric amount to decrement
10540   Enter text string value to set for all text
10541   Enter prefix to add
10542   Enter suffix to add
10543   Enter number of characters to trim from start
10544   Enter number of characters to trim from end
10545   Select TEXT/MTEXTs to modify:
10546   Processing selected text objects
10547   Operation Mode?
10548   Horizontal distance to search for ENDpoints
10549   Horizontal distance to search for NEArest points
10550   Horizontal distance to search for NODe points
10551   Enter last row number
10552   Ending row cannot be less than starting row. RESET to
10553   Ending row cannot be more than total rows =
10554   RESET to max limit
10555   Do you want to export the selection as a WBLOCKed drawing?
10556   Enter WBLOCK drawing name
10557   WriteDEM will now exit.
10558   new point objects were created.
10559   Skipping row #
10560   Creating points on row #
10561   Reading row #
10562   Enter DEM ASCII file name to read:
10563   Read an ARC ASCII DEM files and create AutoCAD points.
10564   This command can be run only within AutoCAD Map / Land Development Desktop.
10565   Error: Cannot open
10566   for writing.
10567   Writing DEM data, Row #
10568   Error: Invalid Z range
10569   Process Text based on text matching properties.
10570   Text Filter Mode:
10571   Enter Text Filter criteria [wildcards accepted]
10572   filter criteria operator
10573   filter criteria value
10574   Enter text justification to filter
10575   Current selection:
10576   Current selection: [none]
10577   Polyline Intersections Explorer.
10578   Enter object break options:
10579   Enter vertex add options:
10580   Enter target objects selection options:
10581   Select source objects to process:
10582   Select target objects to process:
10583   Processing source objects....
10584   1 polyline with arc found and ignored.
10585   Traversing segments...
10586   Checking for intersections...
10587   Pick point which you want to resolve:
10588   Global Object Data editor.
10589   There are no object tables in this drawing.
10590   This command can be run only within Autodesk Map.
10591   Processing object data...
10592   Please select a field name to edit.
10593   Please select an object table to edit.
10594   This command has not been implemented yet. Wait for the next update.
10595   Run current query with 'Alter Properties' and format label placements.
10596   There are no 'TextObject' settings in the current 'Alter properties' settings.
10597   There is no 'Alter properties' setting in the current query.
10598   There are no current queries in this drawing.
10599   Error: It appears that the graphic objects have already been queried\n\nPlease clear any previously queried objects before running this command.
10600   Processing text labels...
10601   Transfer AutoCAD Map Object table data into block attribute data.
10602   Enter object table name to transfer
10603   Enter block name to tranfer the data to
10604   Select objects manually or automatic blocks transfer
10605   Type the ODA command to manually transfer object table data.
10606   [Source Object Data]:Select object:
10607   [Target Block]:Select block:
10608   blocks can be selected to receive the object data.
10609   Selected object does not contain any object data belonging to table:
10610   Please run the OD2ATT command first to set the transfer parameters.
10611   1 Object ignored. Does not contain Object table data belonging to table
10612   Transferring Object table data to Block Attributes...
10613   Number of entities ignored:
10614   Number of Object table records transferred:
10615   Number of entities processed:
10616   Please select an Object Table and an attribute first.
10617   There are no similar Field->Attribute names
10618   You have not made any object table > attribute transfer mapping.
10619   Cannot locate first mirror point on source polyline.
10620   Cannot locate second mirror point on source polyline.
10621   Error: Polyline segments could not be determined.\nPlease make sure your polyline type is valid for the command you are running.
10622   1 polyline with
10623   vertices extracted.
10624   Pick base point for rotation:
10625   Enter rotation angle:
10626   Error: Second connection point could not be determined.
10627   Error: First connection point could not be determined.
10628   Pick destination point of new segment:
10629   Select first point on polyline:
10630   Select second point on polyline:
10631   The two points must be on the same polyline.
10632   Error: Fitted or Splined polylines cannot be used by this command.
10633   Enter a BLOCK name to extract
10634   No tags selected for extraction. No attributes will be extracted.
10635   does not exist or does not contain any attributes.
10636   Include Block Name?
10637   Include Insertion Point?
10638   Include XY Scale Factors?
10639   Include Rotation Angle?
10640   Include Object Handle?
10641   Extracting block attributes into text file...
10642   Attribute Tag names in this block.
10643   Specify attribute [tag] names to extract separated by commas
10644   Search and/or replace object table data
10645   Rename Object data fields.
10646   Retrieving object table information...
10647   Modifying object table...
10648   Writing back revised object table data...
10649   already exists in object table
10650   Please enter a new object field name
10651   Define object table from block attributes
10652   Object Table
10653   created successfully.
10654   could not be created.
10655   already exists
10656   You must specify a name for target object table.
10657   You must specify a name for source block with attributes.
10658   Copy Object table definition
10659   You must specify a name for source object table.
10660   Select ARC/CIRCLE/POLYLINE objects:
10661   Enter sampling type
10662   Enter angular interval for sampling(degrees)
10663   Enter maximum chord length between sampled points
10664   Enter maximum chord offset between sampled points
10665   Create polylines in
10666   Delete original objects?
10667   Change Case to:
10668   Use translation dictionary for special text handling?
10669   Translation dictionary file to use
10670   Enter delimiter character used in translation dictionary
10671   What to process?
10672   Select TEXT,MTEXT,INSERT objects.
10673   Enter a BLOCK name:
10674   Read
10675   translation strings from file:
10676   No translation strings found in
10677   Enter dictionary file name
10678   Please select an attribute name
10679   for reading.
10680   Create counter with
10681   Enter search distance around picked point for underlying text/block
10682   Enter name of the block to use (must be already defined)
10683   Enter attribute name to fill with counter value(must be already defined)
10684   Next String Value =
10685   Enter new current layer:
10686   Please select a block name to use and an attribute name to fill.
10687   Block names must be already defined in the current drawing document
10688   Blocks which do not contain attributes will not appear in this list.
10689   Select Block & Attribute name to use
10690   Multiple TEXT placements
10691   Pick TEXT insertion point:
10692   Enter TEXT string:
10693   Select polylines/3dfaces to label:
10694   Annotate with:
10695   Enter first point number
10696   Enter first point distance
10697   Prefix to use before co-ordinates
10698   Enter horizontal offset from vertex for text insertion
10699   Enter vertical offset from vertex for text insertion
10700   Annotate first and last points only?
10701   Processing polyline/3dfaces...
10702   Select POLYLINEs to flip [reverse direction]:
10703   Flip polylines to:
10704   Retain object handle where possible [arc polylines will be ignored]?
10705   Processing polylines...
10706   Cannot FLIP 2 vertex polylines with the 'Cw' or 'CCw' option.
10707   leader polylines displaying polyline direction stored in active [previous] selection set
10708   CounterClockwise polylines flipped into Clockwise direction.
10709   Clockwise polylines flipped into CounterClockwise direction.
10710   polyline directions reversed.
10711   polyline directions displayed.
10712   Turning on the 'Retain same object handles' option will result in slower execution and ARC'ed polylines will NOT be processed.
10713   Please select a property to transfer.
10714   Error: Invalid field type: Expected 'Integer', Found
10715   Error: Invalid field type: Expected 'Real', Found
10716   Error: Invalid field type: Expected 'Character', Found
10717   Error: Invalid field type: Expected 'Point', Found
10718   Error: Invalid field type: Expected 'Integer/Real', Found
10719   Error : No Visit Selection set is defined.
10720   Visit Selection set already exists. Redefine it?
10721   -------
10722   Current Visit Selection Set closed.
10723   Error: Visit Selection set not defined.
10724   Include linear objects also for 'Visit'?
10725   Display error messages in dialog box?
10726   Color for cross-mark used for highlighting:
10727   This operation will reset the current pointer. Ok to continue?
10728   Visit pointer reset to object # :
10729   Visit selection set unchanged.
10730   Currently showing object # :
10731   Press any key to continue.
10732   Current object # :
10733   is a line feature and not shown
10734   Number of segments
10735   Start point:
10736   End point:
10737   Points must be distinct.
10738   Try again:
10739   Visit Selection Set is empty.
10740   Current View Center :
10741   There is no entity currently being visited
10742   The current entity in Visit selection is dead.
10743   Create virtual segment to point:
10744   Invalid index to GoTo:
10745   Unknown object type.
10746   End of Visit Selection Set reached.
10747   Start of Visit Selection Set reached.
10748   Select POLYLINEs to edit.
10749   Select an option
10750   New width of all polylines
10751   Changing Widths,please wait....
10752   Processing lines...
10753   Select [LINE,POLYLINE,LWPOLYLINE,ARC,SPLINE] objects.
10754   Placing contour labels...
10755   Select LINE,ARC,POLYLINE,LWPOLYLINE,SPLINE to label:
10756   Please select a LINE, POLYLINE, LWPOLYLINE, ARC or SPLINE object.
10757   WIPEOUT objects have been created on layer
10758   Scanning selected TEXT/BLOCK objects...
10759   ---Unused--
10760   Replace
10761   Zooming to searched text...
10762   ENTER to contine or Escape to cancel.
10763   Sort ASCII files in a user-defined format.
10764   Enter input file name to sort
10765   Enter output file name to create
10766   Sort Type:
10767   Sort Data By:
10768   Enter field position to sort data by
10769   Enter delimiter string between fields
10770   Enter start column for sort data
10771   Enter end column for sort data
10772   Reading input file...
10773   Tokenizing input file...
10774   Sorting input file...
10775   Input ASCII text file to sort
10776   Output ASCII text file (sorted) to create
10777   Warning: Input file will be overwritten with sorted data file.
10778   Start Column cannot be greater than end column.
10779   End Column cannot be lesser than start column.
10780   Enter linear unit of measurement
10781   Enter default Text height for new text creations
10782   Enter default TEXT justification
10783   Enter default Block and Text rotation angle in degrees
10784   Enter default X Scale factor for block insertions
10785   Enter default Y Scale factor for block insertions
10786   Enter precision for X (Eastings) annotations and output
10787   Enter precision for Y (Northings) annotations and output
10788   Enter precision for Z (Elevations) annotations and output
10789   Enter precision for distance annotations and output
10790   Enter precision for angular measurements and output
10791   Maximum number of selection set objects to store
10792   Display Command line options?
10793   working parameters to text file
10794   working parameters from text file
10795   Select rounding method
10796   Precision to apply:
10797   Round Off to nearest mulitple of
10798   Apply round-off computations on
10799   Rounding off objects...
10800   Draw graded lines:
10801   Next graded point [U to Undo last segment]:
10802   All segments already undone.
10803   Enter point elevation[or (G)rade percent/(D)egrees slope]
10804   Target Grade can be entered in the following formats:
10805   Enter target grade for this segment
10806   Export Object Table Data to ASCII files.
10807   Enter object table names to extract(* for all)
10808   Exporting Object table data to ASCII file
10809   **Start of Object data listing** for object of handle
10810   **End of Object listing**
10811   Number of distinct Object table records written:
10812   Object Table data export file name
10813   Relative Scale
10814   Scale Factor
10815   Enter new Scale factor
10816   Enter Scale factor by which to scale selected objects
10817   Highlight 3D POLYLINEs with vertices of zero elevation.
10818   vertices have 0 elevation.
10819   There are no vertices with 0 elevation.
10820   Redefine properties of multiple block definitions
10821   Enter Block name(s) to redefine(seperated by commas):
10822   is not an normal block in this drawing.
10823   External references or anonymous blocks cannot be used.
10824   Enter property to redefine
10825   Enter layer-name to set for block entities
10826   Enter color value to set for block entities
10827   Enter elevation value to set for block entities
10828   Enter thickness value to set for block entities
10829   redefined to
10830   Please select the block name(s) to process.
10831   Select vertex on polyline:
10832   Express Pedit.
10833   Warning: Vertex position not in current viewport.
10834   Enter new location:
10835   New location not in current viewport.
10836   Z elevations of vertices cannot be set for light weight and 2D polylines.
10837   Polyline broken at vertex #
10838   Cannot break the polyline at this vertex.
10839   Inherit current vertex Z during 'Move' and 'Insert' options?
10840   Projected horizontal length:
10841   Enter minimum distance weeding tolerance
10842   Specify weed criteria
10843   Create a marker point at every weeded vertex location?
10844   Weeding polylines...
10845   vertices weeded from
10846   Compute Polyline statistics.
10847   Polyline properties:
10848   Polyline is Open.
10849   Polyline is Closed.
10850   Polyline is 3D.
10851   Polyline is 2D.
10852   Polyline contains arc segments.
10853   Polyline does not contain arc segments.
10854   Polyline is curve fitted.
10855   Polyline is splined.
10856   Polyline is a light weight polyline.
10857   Polyline is a heavy weight polyline.
10858   The picked point is at vertex #
10859   The coordinates of the picked point is:
10860   The elevation at the picked point is:
10861   Detailed polyline vertex listing:::
10862   Segment lengths shown are distances from the current point to the next point.
10863   Draw linear polylines from arced polylines.
10864   Pick start point of table:
10865   Select objects to chop [ polyline,line,arc,circle,spline,ellipse ]
10866   Enter number of equally divided segments to create
10867   Enter or pick length of each chop
10868   1 object skipped. Not long enough for this operation.
10869   chopped segments created.
10870   Chopping polylines...
10871   Control the direction of 3DFACE face normals.
10872   How do you want to control face normals?
10873   Enter length of face normal to draw
10874   Enter reference elevation to point to
10875   Enter or pick point to align face normals:
10876   Enter contour interval #
10877   Enter layer for contour interval #
10878   AECC_CONTOUR objects not yet implemented.
10879   No contour intervals have been specified for classifying contours.
10880   is already selected.
10881   Enter or pick spacing between hatch lines
10882   Enter percentage length for alternate hatch lines
10883   Double hatch this area?
10884   Select first side of embankment:
10885   Select second side of embankment:
10886   Select middle path between embankment sides [ENTER to use first side]:
10887   Object has already been picked as an embankment side.
10888   Select middle side of embankment:
10889   Processing polylines and/or arcs...
10890   Processing intersections...
10891   Processing contour objects...
10892   Select source object:
10893   Select destination object for property match:
10894   Elevation of Destination object cannot not be determined.\nElevation match will not be done.
10895   Elevation and thickness match will be done only for those objects allowed by AutoCAD.
10896   Target properties:
10897   Source object has no style property.
10898   Create text labels from object data / extended entity data / database data.
10899   You can now use the GT_ODLA command to label the objects directly using the current settings.
10900   Select object to label:
10901   Pick insertion point of label:
10902   Specify rotation angle:
10903   Required program parameters have not been set yet. Please run the GT_OD_XD_LABEL command first.
10904   No Object Data field selected.
10905   does not exist in the list of selected fields.
10906   'Minimum' Radius value should be less than 'Maximum' radius value
10907   'Maximum' Radius value should be greater than 'Minimum' radius value
10908   Include Closed polylines?
10909   polylines corrected.
10910   polylines flipped and corrected.
10911   polylines ignored
10912   vertices have errors.
10913   Merge fields from two object tables within the same object
10914   Merging field data from source table
10915   to target table
10916   does not exist in target table
10917   You have not selected the data fields to transfer.
10918   You have not selected the target object table.
10919   You have not selected the source object table.
10920   Select a curve [ARC / POLYLINE / SPLINE]:
10921   Pick point on curve to draw tangent from:
10922   Pick second point of tangent:
10923   Error: No tangent possible to this point.
10924   Selection Error: Polylines must be fitted, splined or arced and must be 2d only.
10925   Selection Error: Only polylines, arcs and splines can be selected.
10926   Select a line or polyline:
10927   Enter measured distance from start (Press RETURN to exit):
10928   Enter the next segment distance, as measured from the last point (Press RETURN to exit):
10929   No point is possible at this distance.
10930   This point will fall outside the line.
10931   This command works only under AutoCAD 2000 or higher.
10932   There are no blocks in this drawing.
10933   Pick object to extract:
10934   extracted.
10935   Cannot extract entity type
10936   Extracting from XREF...
10937   This command works only partially in BricsCAD. Please be aware that some functions or options in this command may not work correctly.
10938   This command is not yet implemented in BricsCAD. Please contact 'rakesh.rao@thedesignsense.com' for more info.
10939   There are no referenced blocks in this drawing.
10940   Cannot extract from an unequally scaled or rotated block.
10941   Extracting POLYLINE,Please wait...
10942   Creating vertex #
10943   Skipping CurveFit Vertex #:
10944   Create  a Block or Shape at the location of every POINT object.
10945   Convert to what?
10946   Select POINT objects to convert:
10947   Deleting original POINT objects.
10948   Select SPLINEs or ELLIPSEs to convert to polylines.
10949   Select type of spline conversion:
10950   There are no FIT points available in this spline.
10951   There are no CONTROL points available in this spline.
10952   Processing SPLINEs/ELLIPSEs...
10953   The DXF method re-creates the exact geometry of a spline but can\nsometimes crash your AutoCAD on long splines.\n\nPlease save your work before using this option.
10954   ------
10955   Already reached first segment of polyline. Use 'Next' to go forward or 'eXit' to finish.
10956   Already reached last segment of polyline. Use 'Previous' to go back or 'eXit' to finish.
10957   Select boundary objects:
10958   Select by:
10959   Creation method:
10960   Current selection will be added to active ESelect selection set.
10961   Current selection will be removed from active ESelect selection set.
10962   Current selection will form new active ESelect selection set.
10963   No objects in active ESelect selection set.
10964   Nothing selected.
10965   Remove duplicate or additional object data attached to the same object.
10966   Enter object table names to check(* for all)
10967   Checking Object table data for duplicated records...
10968   object records were deleted.
10969   You have not selected any object tables.
10970   Select TEXT objects to align:
10971   Pick point to align text
10972   Pick first point of alignment:
10973   Pick second point of alignment:
10974   Error: UCS could not be set.
10975   Aligning TEXT...
10976   Select a LINE object to align text:
10977   Processing text objects...
10978   Selected object is not a line
10979   Please select a reference entity before exiting the dialog box.
10980   Select reference object for alignment:
10981   Aligning objects...
10982   Converts polyface mesh objects to polylines.
10983   Converting polyface meshes to polylines...
10984   1 non-polyface polyline ignored.
10985   Transfer AutoCAD Map Object table data into extended entity data.
10986   Enter object table names to transfer(* for all)
10987   Transferring Object table data to Xdata...
10988   Replace one block with another.
10989   ** WARNING ** : This will change the handle of the block.
10990   Applications relying on handle beware.
10991   Enter source Block name:
10992   Enter target Block name:
10993   Perform external block synchronization with DWG file?
10994   Reading
10995   Please select a source block.
10996   Please select a target block.
10997   object records were transferred
10998   Transfer Text Strings as Object Table Data values.
10999   Select entity to receive object table data:
11000   data attached to object.
11001   Select text string for object field [or ENTER to key in a value]:
11002   successfully updated.
11003   was not updated.
11004   Please select at-least one object field name to transfer to.
11005   Please select an object table to transfer to.
11006   Annotate with what?
11007   Prefix to use before co-ordinates
11008   Select point objects to annotate or ENTER to pick individual points:
11009   Converting attributes to TEXTs...
11010   Note: Unequally Scaled BLOCKs cannot be EXPLODEd.
11011         You can turn off their attribute displays, if desired.
11012   Exploding BLOCKs...
11013   Converting attribute definitions to TEXTs...
11014   Deleting attribute definitions....
11015   Explodes polylines with width, recreate geometry
11016   Type the GT_XO command to start the transfer of object table data.
11017   There are no Object tables defined for transfer. Please run the 'GT_Xfer_Od_Xd' command first.
11018   Select target object:
11019   The following object table data are attached to this object:
11020   Overwrite existing object table data?
11021   Source object does not contain any object data attached to it.
11022   What to place?
11023   BLOCKs will be placed with a scale factor of
11024   and rotation angle of
11025   Enter a BLOCK name to insert:
11026   Which layer to place?
11027   Placing points on polylines...
11028   Placing blocks on lines,polylines...
11029   Scale Z values of selected objects.
11030   Enter conversion factor for Z values:
11031   Scaling Z coordinates...
11032   Enter Lower bound Value for search
11033   Enter Upper bound Value for search
11034   Select objects to filter from.
11035   No objects found in the specified Z range.
11036   Add/Remove redundant closing vertex in polylines.
11037   Closing vertex control
11038   Enter start-end closing tolerance
11039   Checking polylines...
11040   Convert lines, arcs and circles to polylines.
11041   Select LINEs, ARCs,CIRCLEs objects
11042   Output polyline type?
11043   Filtering Selected objects...
11044   Select CIRCLE:
11045   The object you picked is not a circle.
11046   Select 3D POLYLINEs to set Z values.
11047   Enter minimum vertex elevation to be allowed:
11048   Error: Polyline has no vertex which is higher than the minimum specified Z.
11049   2D Polyline(s) were ignored.
11050   Polyline(s) were ignored because of 'out-of-range' Z values.
11051   Transfer Text Strings as Block Attributes.
11052   Select block object to receive attribute data:
11053   Select text string for block attribute [or ENTER to key in a value]:
11054   (or type a value)
11055   Selected object is not a TEXT entity.
11056   Selected block is not a
11057   Please select at-least one attribute to transfer to
11058   Please select a block name to process.
11059   Enter segment length (X to exit):
11060   Enter number of segments
11061   Densifying vertices....
11062   additional vertices added to
11063   Flowing linetypes flow across polyline segments.
11064   Broken linetypes start at each segment.
11065   Convert object linetype to:
11066   polylines have been updated from
11067   non-flowing to flowing linetype mode
11068   flowing to non-flowing linetype mode
11069   No objects found matching selection criteria.
11070   Enter or pick width of the right-of-way
11071   Creating Rights-Of-Way from polylines...
11072   polylines were created.
11073   Slide [move] text in a direction relative to its rotation angle.
11074   Enter relative angle to slide through
11075   Enter distance to slide text through
11076   Select first object[ARC or LINE]:
11077   Select second object[ARC or LINE]:
11078   Selected object is a
11079   Error: ARC's and/or LINEs are not touching each other at their ends.
11080   Same object picked twice.
11081   Please pick only a LINE or ARC object.
11082   Select text objects to write to ACSII file.
11083   Select first polyline:
11084   Select second polyline:
11085   ----
11086   ----
11087   ----
11088   Sort Order:
11089   Creating TEXT list...
11090   Writing selected text objects to...
11091   Select lines and/or polylines:
11092   Change widths of LINEs, POLYLINEs, CIRCLEs and ARCs.
11093   Enter or pick new width:
11094   Changing Widths,please wait....
11095   Select objects to delete(move) duplicates:
11096   A non-zero value for tolerance will significantly increase processing time.
11097   Enter tolerance for duplicate recognition
11098   Check for Xdata equality also?
11099   Check for Layer equality also?
11100   There are
11101   duplicate object(s)
11102   Duplicate objects moved to $DUPLICATE$ layer and placed in 'previous' selection set...
11103   There are no duplicate objects in the selection.
11104   The enclosed area of the picked points is
11105   The cumulative area so far is :
11106   Really want to reset the cumulative perimeter counter
11107   Select LINE,[LW]POLYLINE,ARC or CIRCLE to add to perimeter count:
11108   Really want to reset the cumulative area counter
11109   Fitted polyline ignored.
11110   Unsupported object type.
11111   Select text objects to edit inside a text editor.
11112   Reading text from temporary file...
11113   Updating Text objects...
11114   Select LINEs,POLYLINEs,SPLINEs,ARCs and/or CIRCLEs to add length:
11115   Adding up lengths...
11116   Select object to list data:
11117   There is no object data belonging to the object table:
11118   Hit ENTER to continue.
11119   Please select an object table to list data from.
11120   Hightlight polylines,lines,splines,3dfaces with specified vertex elevation differences.
11121   Select polylines/3dfaces to check for vertex elevation difference:
11122   Enter vertex difference to identify
11123   Identifying elevation differences...
11124   There are no objects that match the specified vertex elevation drop.
11125   Control visibility of polyface edges.
11126   Select edge on polyline:
11127   The containing edges are:
11128   Explode Splined polylines and convert to decurved polylines.
11129   Select splined or fitted POLYLINEs:
11130   The new polylines will acquire new handles but any existing Xdata will be transferred.
11131   Exploding and assembling fitted/splined POLYLINEs...
11132   Draw 3d polyline with elevation prompts.
11133   Enter vertex elevation
11134   Cannot close a 3d polyline with less than three points.
11135   Enable Automatic elevation increment/decrement?
11136   Enter increment[+]/decrement[-] value
11137   From point:
11138   Boundary edge orientation?
11139   Pick point through which
11140   Pick first point of boundary edge:
11141   Pick second point of boundary edge:
11142   Line from point:
11143   SegOffset command is designed to function on linear segments only
11144   On arc segments, the straight line joining the points will be used.
11145   Select a polyline segment to offset:
11146   Point picked does fall on polyline\nYour picked point may have been on an arc segment.
11147   Add or remove TEXT underlining.
11148   The Text String
11149   is found in the following blocks:
11150   There are no blocks containing the text string
11151   Select TEXT objects for enclosing:
11152   Select Objects to remove Xdata.
11153   Registered Extended entity data applications
11154   Enter Xdata application name(s) to delete
11155   Insert multiple drawing files.
11156   Draw 3DFACE with elevation prompts.
11157   Third point:
11158   Fourth point: <create three-sided face>:
11159   Enter elevation of point
11160   Create a DWG each for selected layers in current drawing.
11161   Include layer
11162   is empty. 0 objects exported.
11163   objects exported.
11164   Select a line or polyline:
11165   block intersections were trimmed.
11166   Convert polylines to splines.
11167   Select 3D POLYLINEs to interpolate.
11168   [Interpolated]
11169   [No change]
11170   Error : Number of points in updated polyline is not the same as original polyline
11171   Interpolating polylines...
11172   Pick Center point:
11173   Pick Starting angle:
11174   Specify Outside radius:
11175   Specify Radius pitch:
11176   Specify Coil width:
11177   Specify Pitch:
11178   Enter Number of rotations:
11179   Enter Resolution:
11180   Drawing Helix...
11181   Offset type?
11182   Offset distance must be positive and non-zero.
11183   Select TEXT object to set current style [ENTER to select from list]:
11184   Current TEXT style set to:
11185   Maximum Spread Length along segment
11186   Maximum Spread Length across segment
11187   self-intersections in
11188   Their locations have been marked as points on the layer
11189   There are no self-intersections in these polylines.
11190   Explode only nested block objects [block within a block].
11191   Scanning blocks...
11192   Exploding nested blocks...
11193   nested blocks exploded.
11194   blocks ignored.
11195   List Object Table data in text mode.
11196   Your trial or subscription period for registering GeoTools has passed.
11197   Refer to your documentation 'Register_GeoTools.Txt' for instructions
11198   on how to register your GeoTools
11199   - or -
11200   Please contact your GeoTools distributor from whom you bought
11201   this product or the developer at the following address
11202   Meanwhile, you can register your evaluation copy online
11203   at the following URL:
11204   You can also purchase GeoTools using several other methods
11205   More information on purchase options and pricing can be obtained from
11206   the file GeoToolsOrderForm.Txt located in your installation folder
11207   You may also contact our office directly for queries:
11208   *This notice does not appear once GeoTools has been registered*
11209   GeoTools is a product of DesignSense Software Technologies Pvt. Ltd., Bengaluru-INDIA
11210   Your grace period during which you can run without
11211   registering is from
11212   Waiting for GeoToolsUser Registration file...
11213   GeoTools User Registration file 'GeoToolsUser25_??_??.RGS' is in incorrect format.
11214   Please make sure you are using the correct file.
11215   Could not open GeoTools User Registration file.
11216   Internal Error: GeoTools temporary file could not be created.
11217   Please verify that you have write permissions available for your
11218   Windows TEMP directory.
11219   Fatal Error - GeoTools aborting
11220   Your windows TEMP directory has not been set. Please ensure
11221   that you have defined your TEMP directory before resuming
11222   GeoTools User Registration file not found.
11223   GeoTools license information
11224   GeoTools Notification
11225   The GeoToolsUser25_??_??.RGS file that you are using has been retired and is no longer in use.
11226   You are probably trying to use GeoTools on a computer that has been indicated
11227   not to be for GeoTools use.
11228   Please obtain a valid user registration file for this computer from your GeoTools
11229   dealer or from DesignSense Software Technologies Pvt. Ltd.: rakesh.rao@thedesignsense.com
11230   You will need to send us your application key to authorize your use of GeoTools
11231   on this computer. This can be obtained now by typing 'GT_AppKey' on the command line
11232   Please see 'Register_GeoTools.Txt' for further instructions on how to obtain a valid user registration
11233   is not licensed to run on this copy of AutoCAD.
11234   Please obtain a registration for the copy of AutoCAD you are using.
11235   Refer to the file
11236   Error: Your FIXED hard disk identification could not be obtained.
11237   Error: GeoTools cannot continue. Your computer does not have a FIXED hard disk.
11238   Application key cannot be generated unless GeoTools is initialized.
11239   Please select any GeoTools command from 'GeoTools' pull-down menu
11240   and then rerun the 'GT_AppKey' command.
11241   Display GeoTools/CADPower Application Key for this computer.
11242   The disk-based GeoTools/CADPower application key for this computer is
11243   Show all GeoTools Toolbars.
11244   Hide all GeoTools Toolbars.
11245   This point has already been measured.
11246   Number of column values to write on each row [0=All values]
11247   Perform co-ordinate transformation before exporting DEM data?
11248   Enter object table name to process:
11249   Enter object table field name to rename:
11250   Enter new field name:
11251   Select [LINE,POLYLINE,SPLINE] objects.
11252   Pick object to annotate at annotation position(ESC to end):
11253   Invalid object type: Only LINE,POLYLINE,LWPOLYLINE and SPLINEs can be selected.
11254   Nothing selected. Please pick again.
11255   There are more than one object table records. 'GT_Pl_DataLbl' will use the first data record.
11256   No links found attached to this object.
11257   Please select an object table and atleast one field name to use for labeling.
11258   Connected to ADO database.
11259   Database connection
11260   Please select a link template and atleast one field name to use for labeling.
11261   To remove a selected field, choose one of the selected fields first.
11262   Please select a database field.
11263   Select 3d polyline to offset:
11264   Message deleted
11265   Only 3d polylines can be ofsetted by this command. Use AutoCAD Offset command for 2d polylines.
11266   Selected object is not a polyline (must be 3d polylines only)
11267   collinear vertices removed.
11268   Pick chainage point on polyline:
11269   overlapping objects deleted.
11270   attached and placed on layer
11271   Select DWG files to Xref
11272   Select DWG folder
11273   Measure distances in
11274   Create a DWG each for selected blocks in current drawing.
11275   Include block
11276   Select POLYLINEs and/or ARCs
11277   Enter name of tag export file
11278   Vertex #    X-Coord       Y-Coord       Z-Coord       SegmentLength  SegmentSlope(%)  SegmentSlope(degs)  Azimuth(Bearing)
11279   Define object table from linked database table.
11280   There are no link templates defined in this drawing.
11281   Please enter an object table name to create.
11282   Please select a link template to define database connection
11283   Transfer database linked data to object table data.
11284   Transferring data from database to object table
11285   ---------
11286   Error: Database fields could not be transferred. Data links may not exist.
11287   and object data field
11288   are not of the same types.
11289   Error: Point data type object fields are not supported by this command.
11290   Multiple association of Database->Object Table is not allowed.
11291   Please select a database and object table field first
11292   There are no similar database->object table names.
11293   You have not made any database->object data mapping.
11294   Join multiple 3d polyline segments.
11295   Select 3d polylines/lines to join (or ENTER to select by layer):
11296   Do you want to export the interpolation statistics to an ASCII text file?
11297   Selected object is not a line, polyline or spline.
11298   Select HATCH objects to create outline.
11299   Error: Hatch object is not in WCS.
11300   Select polylines:
11301   objects created
11302   Calculate surface area of the 3DFACE entities
11303   Select 3DFACE objects:
11304   Processing 3DFACE/SOLIDs,
11305   Skipping 3DFACE/SOLIDs,
11306   The total calculated surface area of
11307   objects is
11308   Reset registry information of
11309   commands
11310   command
11311   Clearing registry entries for
11312   Fillet between two polylines.
11313   Fillet multiple polylines.
11314   3dpolylines or lines cannot be processed and are ignored.
11315   DEM Export format:
11316   DEM Import format:
11317   Drawing:
11318   Polylines containing ARC segments will be weeded based on their inter-vertex
11319   straight line lengths and NOT the actual arc distances. ARC segments will
11320   be replaced with straight line segments
11321   (You can copy-paste this appkey from the text window after exiting this message box)
11322   CADPower Layer Manager
11323   Layer Name
11324   renamed to
11325   Error:Cannot rename layer
11326   destination layer
11327   already exists.
11328   lower-cased to
11329   upper-cased to
11330   upper-cased to
11331   Please select some layer name(s) first.
11332   is of insufficient length.
11333   Select slope format
11334   Precision for grade value
11335   1 zero-length line was found and ignored.
11336   Cannot join arcs at differing elevations
11337   Cannot join since one of the objects is a SPLINE
11338   Sends all images back using the DRAWORDER command.
11339   images sent to 'Back' of drawing using DrawOrder command.
11340   Enter area unit of measurement
11341   Attach linear and area units strings as suffixes to values?
11342   Pick start point of area annotation:
11343   Extracting tag names from block:
11344   Attribute tag names extract file
11345   Please select some blocks to export tags.
11346   Extract block attribute tag-names into ASCII file.
11347   Drawing Name:
11348   Pick first point of cutting line [or ENTER to select existing lines]:
11349   Pick second point of cutting line:
11350   Select lines/polylines as cutting edges:
11351   Polylines must contain exactly two vertices to qualify as cutting line.
11352   Select point to annotate:
11353   new point objects created and place in active selection set.
11354   This command will operate in command-line mode for the rest of this CAD session.
11355   If you want to see the dialog box again, please start a new CAD session.
11356   ASCII output file to create
11357   Enter names of blocks to extract seperated by commas
11358   Create polygonal centroid points / labels
11359   The centroidal point, if falling outside the polygon, will be moved to a location physically inside the polygon
11360   There are no object tables attached to this object.
11361   Breaks object but retains object data
11362   Select object to break:
11363   Specify second break point or [First point]:
11364   Specify first break point:
11365   Specify second break point:
11366   Convert 3 or 4 segment polylines to 3dface objects.
11367   1 polyline ignored: This command requires only a 3 or 4 segment polyline
11368   Create auto-incrementing object table data.
11369   Select object to auto-increment object data:
11370   This object did not contain object table data. New object record created.
11371   This object does not contain object data and has been skipped.
11372   Export 3dface objects to SMS 2DM file format.
11373   2DM output file name to create
11374   Create polygonal centroid points / labels...
11375   List total areas of polylines in selected layers.
11376   1 object was in non-parallel UCS and has been ignored.
11377   Transferring object data as elevations... 
11378   Error: Custom block named:
11379   does not exist in the current drawing.
11380   Number of vertices in source and ofsetted polyline are the same.
11381   Warning: Number of vertices in source and ofsetted polyline are not the same.
11382   Any extended entity data and object data found in source objects will be transferred to the target objects.
11383   Error: Acreage will be displayed with area annotation only if linear unit is either 'ft' or 'feet'. Please run 'GT_GenSet' command.
11384   1 ellipse object ignored. 'GT_Spl2Pl' can process ellipses only if the 'Interpolate' option is chosen
11385   Insert geo-referenced images (accompanied with World files only)
11386   Error in file name structure: The dot character [.] is missing in file:
11387   Invalid file extension
11388   Cannot find World file:
11389   Progress Indicator interval (in 'number of objects' processed)
11390   Select image files to import
11391   Select text objects to split.
11392   Exploding objects...
11393   Blocks with unequal scale factors cannot be exploded.1 block ignored
11394   Specify next point
11395   Specify start point of polyline
11396   Requires atleast 3 vertices to close.
11397   Updating 3d polylines...
11398   Rename block tag names and update all inserted blocks
11399   Trim before first occurence of marker character
11400   Trim after last occurence of marker character
11401   Trim marker character also
11402   Enter marker character to check (all characters BEFORE this will be trimmed)
11403   Enter marker character to check (all characters AFTER this will be trimmed)
11404   You have picked the start point of the polyline. This operation does not change anything.
11405   Multiple vertex position editor [for polylines, lines, arcs]
11406   Picked points must be visible on screen.
11407   points picked], Pick point to move: [ENTER to finish]:
11408   Pick insertion point of table:
11409   Table can be created only in AutoCAD versions 2005 and above.
11410   Reposition target block attribute locations to match source attribute locations?
11411   This attribute tag already exists in the source block.
11412   Error: The source and target attribute tags are the same. Please choose a differnt name for the target attribute.
11413   Please select a 'new attribute' tag name before exiting this dialog box.
11414   Please select a block name to process before exiting this dialog box.
11415   ----un-used---
11416   Please select a tag to rename before exiting this dialog box.
11417   Check for objects with no extended entity data or Object Table data.
11418   Create a [mathematical] polyline offset relative to another polyline
11419   GeoTools is in Script Mode. All commands will now display a non-dialog box interface.
11420   GeoTools is in dialog box mode. All commands will now display a dialog box interface.
11421   Square (right angle) the edges of a polyline representing a digitized building.
11422   Select text object to acquire height from:
11423   1 polyline height changed to 
11424   Selected object is not a TEXT or MTEXT object.
11425   does not exist in this drawing -or- cannot be found in the search path.
11426   Exploding polylines
11427   Processing objects
11428   is already selected.
11429   Import an SMS 2DM file as 3dfaces
11430   Select 2DM file to import
11431   Processing 2DM file
11432   Processing 3dfaces...
11433   Building mesh information...
11434   Building points information...
11435   Object data for table:
11436   No LINEs,POLYLINEs,ARCs or CIRCLE objects found in selection area.
11437   objects at point.
11438   Enter ending row
11439   Number of rows = 
11440   Number of columns = 
11441   Reading DEM points, row # 
11442   Enter lower bound Z range value
11443   Enter upper bound Z range value
11444   Check first and last vertices also?
11445   Processing polylines...
11446   Warning: 1 2d polyline in selection ignored.
11447   Enter fillet radius
11448   Attribute field
11449   successfully updated with value =
11450   Data field
11451   unchanged.
11452   Select polyline to trace:
11453   Select polylines:
11454   ASCII text file to create
11455   New object created.
11456   New object NOT created.
11457   Polyline boundary is not implemented.
11458   Select HATCH object:
11459   Number of boundary paths
11460   Select HATCH object:
11461   from point
11462   Enter point elevation
11463   ASCII output file to create
11464   Offset segment
11465   Selected object is a 
11466   Color    :
11467   Linetype : 
11468   Style    :
11469   Elevation:
11470   Thickness:
11471   Processing 3DFACE objects...
11472   Processing boundaries...
11473   'DwgSplit' cannot continue. Number of objects is each selection > than total number of objects selected.
11474   Scanning objects...
11475   Select output drawings folder
11476   Select polyline to label:
11477   Selected object is not a polyline.
11478   Writing
11479   Visit selection set contains : 
11480   Select text objects to re-position [un-clutter].
11481   Re-positioning text objects...
11482   Selection Method?
11483   Point(s) moved in X direction by: 
11484   Point(s) moved in Y direction by: 
11485   Point(s) moved in Z direction by: 
11486   Pick base point:
11487   Pick target point:
11488   Drape 3d polylines over an existing set of intersecting lines,polylines,arcs,splines
11489   Select [source] polylines to be draped.
11490   Select [target] objects to get the elevations from.
11491   Processing 3d polylines...
11492   Batch process multiple drawings for script processing.
11493   Please select some drawing files before pressing 'Ok' button
11494   Select drawing files to use
11495   Please select a drawing file to remove.
11496   Error: Please select a script file to use
11497   Error: Please select/specify a BATch file to create
11498   Search embedded text?
11499   Case Sensitive search?
11500   Search Block Attributes also?
11501   Replace searched TEXT?
11502   Interactive Replace (confirm each replace)?
11503   Search Text:
11504   Replace Text:
11505   Error: Cannot find script file:
11506   Display extended entity data from selected object.
11507   Select object to view extended entity data (xdata):
11508   Xdata from application:
11509   This entity does not contain xdata belonging to application:
11510   Search and replace extended entity data values.
11511   There are no registered extended entity data applications in this drawing.
11512   Densify Method
11513   For technical support
11514   1 Open polyline cannot be offset and has been ignored.
11515   1 2d polyline was ignored by this command
11516   Profile parameters file:
11517   saved successfully
11518   restored successfully
11519   Inherit property from one object only once?
11520   Delete inherited property object from drawing?
11521   Specify block/SHAPE XY scale factor:
11522   Specify block/SHAPE rotation angle:
11523   Select objects to flatten:
11524   A generic 'flatten' procedure was applied on all selected objects.
11525   Please verify if the results are accurate.
11526   Enter segment slope in degrees
11527   Specify block XY scale factor:
11528   Specify block rotation angle:
11529   Error: This is a 3d polyline. Only 2d polylines can be offsetted by this command.
11530   Selection Error: Only lines, 2d polylines, arcs and splines can be selected.
11531   Enter Text height
11532   Enter Text rotation angle
11533   A closed polyline rectangle was drawn at the screen extents.
11534   Select object(s) to enclose with bounding box:
11535   A closed polyline rectangle was drawn covering the extent of the selected objects.
11536   Select object(s) to zoom to:
11537   Enter layer name to isolate:
11538   is current, all other layers frozen.
11539   Select object(s) on layer(s) to isolate [ENTER to select from a list]:
11540   Layers selected:
11541   Over-write existing layer state named
11542   Current layer settings saved as
11543   Layer setting name:
11544   This command works only under AutoCAD 2006 or higher.
11545   Longest segment in polyline        :
11546   Shortest segment in polyline       :
11547   Average segment length in polyline :
11548   Apply elevation value check before labeling?
11549   From (elevation):
11550   To (elevation):
11551   Select objects to scale in X, Y and Z directions.
11552   Enter X-scale factor (or R for Reference):
11553   Enter Y-scale factor (or R for Reference):
11554   Create a mean (averaged) point from a cluster of points / blocks
11555   Mean (average) point created at location:
11556   Do you want to connect each point with the mean point?
11557   Enter Z Scale Factor
11558   Error: This computer
11559   does not have any active & valid GeoTools portable license installed.
11560   The 'GeoToolsUser25_??_??.RGS' file that you are using is not authorized for this computer
11561   GeoTools is running in un-registered, limited period evaluation mode.
11562   Not defined.
11563   default settings
11564   Enter FUZZY tolerance distance to search around points of interest
11565   Error: There is an ARC'ed polyline with duplicate vertices. Please fix this before running the GT_INTEX command
11566   Breaking polylines...
11567   Build common edges along closed, adjacent polygons
11568   Cannot open 'Polyline Specialist' online user-manual
11569   Cannot find 'PLSPEC.VLX' file to determine installed software location
11570   Enter block selection mode
11571   Extract object table data struture to ASCII text files.
11572   Object Table structure export file name
11573   Table Name:
11574   Field Name
11575   Field Description
11576   Field Type
11577   Field Default Val.
11578   Object Table Name :
11579   Processing Object Table :
11580   Enter geographical coordinates (Latitude,Longitude,[Height]) in D M S format
11581   Error: Latitude value must be between -90.0 degrees and +90.0 degrees
11582   Error: Longitude value must be between -180.0 degrees and +180.0 degrees
11583   Incorrect geographic coordinates entry format. Please enter the coordinate as 'Latitude,Longitude,[Height]' in D M S format
11584   was not renamed.
11585   Starting Width:
11586   Ending Width:
11587   Create tapered lines or change existing ones to tapered lines.
11588   1 polyline with more than 2 vertices was ignored.
11589   Draw tapered lines:
11590   for instructions on getting registration.
11591   Pick center point of slot:
11592   Slot width:
11593   Slot length:
11594   Specify slot angle:
11595   Please obtain a valid user registration file for this computer from your Polyline Specialist
11596   dealer or from DesignSense Software Technologies e-mail: rakesh.rao@thedesignsense.com
11597   You will need to send us your application key to authorize your use of Polyline Specialist
11598   on this computer. This can be obtained now by typing 'PSAppKey' on the command line
11599   Please see 'Register_PolylineSpecialist.Txt' for further instructions on how to obtain a valid user registration
11600   The disk-based application key for this computer is :
11601   The serial number of this CAD software is :
11602   The 'PolylineSpecUser.RGS' file that you are using is not authorized for this computer
11603   System Information:
11604   CADPower is running in un-registered, limited period evaluation mode.
11605   Polyline Specialist Notification
11606   Point Labeling and annotation tool
11607   File:
11608   Please select some objects for 'Visit'
11609   Enter zoom height to display on screen:
11610   Error: Zoom height should be a non-zero and positive value.
11611   Error: Already at the end of the visit selection set.
11612   Please use 'Previous' to browse in the backward direction.
11613   Error: Already at the start of the visit selection set.
11614   Please use 'Next' to browse in the forward direction.
11615   Error. Current Visit selection set entity is not readable.
11616   Detect free ends (dangles) of lines,polylines and arcs
11617   Checking for dangles [free ends]...
11618   Your current GeoTools license file is valid for the following serial numbers:
11619   Your current GeoTools license file is valid for the following application keys:
11620   Your current Polyline Specialist license file is valid for the following serial numbers:
11621   Your current Polyline Specialist license file is valid for the following application keys:
11622   Mark intersection points along lines,polylines,arcs and splines
11623   Example: +2.5%, -2.5%, +1:4, -1:4 where the + sign represents a uphill grade and - sign represents downhill grade.
11624   Endpoint of line
11625   -----
11626   Only closed, 2d polylines will be used for INwards or OUTwards offset operation. Other types of polylines in the selection will be ignored.
11627   Pick center point of tube:
11628   Enter inner radius of the tube:
11629   Enter outer radius of the tube:
11630   Error: Outer radius of tube cannot be less or equal to inner radius.
11631   Enter the height of the tube:
11632   Only polylines with 3 or 4 vertices will be converted to a 3DFACE, other polylines in the selection will be ignored.
11633   Pick insertion point for
11634   Error: Center of gravity cannot be determined for an open curve.
11635   AutoCAD Point object created at the centroid location.
11636   Error: Cannot use 'Stacked fields' in 'Linear' Export Mode. Stacked fields output is allowed only in 'Points' Export mode.
11637   drawing stamps changed.
11638   Error: Cannot set export mode to 'Linear' if Stacked fields output is checked. 
11639   date stamps changed.
11640   GeoTools Alert: Please be informed that decimal precision values for XYZ coordinates & distances can be set using the GT_GENSET command only. The coordinates precision is NOT set in this command.
11641   Create upright readable text always?
11642   Select start point of text along curve:
11643   Processing row #
11644   Select point/block/text objects around which to create closed polylines.
11645   Select polygon edge [boundary] objects.
11646   Processing points
11647   Success: A new closed polyline with
11648   vertices was created with the 'Boundary' command.
11649   Ignored: Duplicate point found within polygon area. A new polygon was NOT created at this point.
11650   'Boundary' command failed. A new closed polyline was not created.
11651   new closed polylines were created.
11652   Pick a point at which to interpolate elevation:
11653   Select first adjacent polyline:
11654   Select second adjacent polyline:
11655   The Z elevation at this point is :
11656   Both the polylines selected are the same. Please select two different objects.
11657   Enter initial zoom window size
11658   Enter layer name(s) for polylines to acquire elevation from
11659   Error: Could not find a pair of adjacent polylines even after 20 zoom iterations.
11660   Please try again after increasing the initial zoom scale value.
11661   Check for Object Data equality also?
11662   Ignore Z elevations while checking coordinates?
11663   Checking Z elevations in polylines...
11664   vertices weeded from
11665   polylines
11666   No polyline vertex weeded as the weed criteria was not satisifed.
11667   polylines could not be processed because the vertex weeding results in less than two vertices.
11668   polylines with exactly 2 vertices were ignored.
11669   Pick counter location
11670   Old Attribute:
11671   changed to
11672   Flips (reverses) the sign of the elevation[Z] from selected objects.
11673   Select text [counter] object, after which to insert new counter object:
11674   Select block [counter] object, after which to insert new counter object:
11675   Error: Please select a text object only.
11676   Error: Please pick a block with the name:
11677   Error: Please select a block object only.
11678   Pick location to place new
11679   Select text objects [for update]:
11680   Old Text:
11681   Vertical Offset distance:
11682   Mark junctions in a network of linear objects.
11683   A junction is a point where at least three or more segments branch out in as many different directions.
11684   Enter zoom height to keep during each search
11685   This command has been renamed. Please type 'GT_ALIGNTEXT' instead.
11686   This command has been renamed. Please type 'GT_ALIGNTEXT2LINE' instead.
11687   Insert a Map Sheet Index Block.
11688   Block:
11689   Pick insertion point of map sheet:
11690   Enter horizontal extent [X] of sheet
11691   Enter vertical extent [Y] of sheet
11692   Enter sheet name
11693   Select sheet index block or polyline to draw grid within [or ENTER to pick corners points of grid]:
11694   Error: Please pick a sheet index block named:
11695   Pick origin point of grid [lower left corner]:
11696   Pick upper left corner of grid:
11697   --------
11698   --------
11699   Error: Cannot find the block 'GRID_CROSS' within the drawing or in the GeoTools 'Blocks' folder.
11700   Select object type
11701   Select Layer(s)
11702   Select Block(s)
11703   Select Layer
11704   Select Block
11705   Select Complex Feature ID
11706   Select Relation Feature ID
11707   Select Point Feature ID
11708   Select Line Feature ID
11709   Select Area Feature ID
11710   Error: Cannot find the block 'TICK_LEFT' within the drawing or in the GeoTools 'Blocks' folder.
11711   Error: Cannot find the block 'TICK_RIGHT' within the drawing or in the GeoTools 'Blocks' folder.
11712   Error: Cannot find the block 'TICK_BOTTOM' within the drawing or in the GeoTools 'Blocks' folder.
11713   Error: Cannot find the block 'TICK_TOP' within the drawing or in the GeoTools 'Blocks' folder.
11714   Pick the bottom center point of truncated cone:
11715   Enter bottom radius of truncated cone:
11716   Enter top radius of truncated cone:
11717   Enter height of truncated cone:
11718   Error: Top radius cannot be greater or equals to base radius
11719   Pick lower right corner of grid:
11720   -------
11721   -------
11722   Error: Sheet index polylines must have EXACTLY 4 vertices.
11723   Sheet index polylines must contain EXACTLY 4 vertices and they must be defined in the following clock-wise order:
11724   Lower Left -> Upper Left -> Upper Right -> Lower Right
11725   Save grid scale parameters in ASCII file
11726   Restore grid scale parameters from ASCII file
11727   Error: There are no map scales defined. Please add a scale set first before saving the parameters.
11728   Pick base point for scaling:
11729   Scale text objects also?
11730   Scale blocks also?
11731   Create polylines by joining sorted points.
11732   In AutoCAD 2009/2010, the GeoTools pull-down menu is automatically visible in the 'AutoCAD Classic workspace' only
11733   In other workspaces, the GeoTools menu can also be accessed by clicking on the AutoCAD icon [menu browser] at the top left corner of the screen.
11734   Show all Polyline Specialist Toolbars.
11735   Hide all Polyline Specialist Toolbars.
11736   Polyline Specialist Registration Notice
11737   Thank you for your interest in Polyline Specialist software.
11738   This is a 30-day evaluation copy of Polyline Specialist.
11739   All users are required to register Polyline Specialist within 30 days
11740   GeoTools can be purchased online through our website at
11741        http://www.4d-technologies.com/shop/purchase.htm
11742        http://www.4d-technologies.com/polyline_specialist/register.htm
11743   Once you purchase Polyline Specialist, your order will be shipped to
11744   You can also purchase Polyline Specialist using several other methods
11745   the file PolylineSpecialistOrderForm.Txt located in your installation folder
11746   Polyline Specialist is a product of DesignSense Software Technologies, Bengaluru, INDIA
11747   *This notice does not appear once Polyline Specialist has been registered*
11748   Your 30-day period for registering Polyline Specialist has passed.
11749   Please refer to your documentation 'Register_PolylineSpecialist.Txt' on how
11750   to register your Polyline Specialist.
11751   Please contact your distributor from whom you bought
11752   The 30-day grace period for registering Polyline Specialist was from
11753   Polyline Specialist license information
11754   The Polyline Specialist application key for this computer is
11755   Display Polyline Specialist Application Key for this computer.
11756   Application key cannot be generated unless CADPower is initialized.
11757   Please select any CADPower command from 'CADPower' pull-down menu
11758   and then rerun the 'CP_AppKey' command.
11759   Error: Polyline Specialist cannot continue. Your computer does not have a FIXED hard disk.
11760   does not have any active & valid Polyline Specialist portable license installed.
11761   Polyline Specialist Version
11762   Successfully read Polyline Specialist registration information...
11763   Please reopen your drawing if you wish to run this command again
11764   or you can continue your evaluation of other commands
11765   notification
11766   Number of remaining trial runs for this command:
11767   Registration notice
11768   Please wait while
11769   starts in un-registered mode.
11770   In AutoCAD 2009, the 'Polyline Specialist' commands are automatically loaded in the 'AutoCAD Classic workspace' only
11771   The 'Polyline Specialist' menu can also be accessed by clicking on the AutoCAD icon [menu browser] at the top left corner of the screen.
11772   Select label layer
11773   Error: Cannot select 'Multiple objects for processing' if 'Auto-Incrementing text' option is turned on.
11774   Error: Cannot select 'Auto-Incrementing text' if 'Multiple objects for processing' option is turned on.
11775   Select centroid layer
11776   Enter TEXT string to set as object data (or . for null string):
11777   Enter TEXT string to set as block attribute (or . for null string):
11778   Import MINEX stratified reserves data file into CAD
11779   Select polylines/arcs to draw the arc-center to arc-end connections:
11780   Purge or remove all unreferenced entries from the 'ScaleListEdit' command
11781   Scale List:
11782   Unresolved external reference file:
11783   detached from current drawing.
11784   Attached external reference file:
11785   bound to current drawing.
11786   This command is not available in BricsCAD.
11787   Detaches all un-referenced XREFs and binds all others into current DWG.
11788   Error: You are using a
11789   license and this cannot be used with
11790   Scan selected image files and build image boundary list.
11791   Image          :
11792   attached.
11793   X Extents :
11794   Y Extents :
11795   Error: Could not read world file for the image:
11796   (image will be ignored)
11797   Error: Please run the GT_ImageScan command first to read the images and scan the extents.
11798   Insert geo-referenced image corresponding to selected area of interest [AOI]
11799   Found
11800   images
11801   Error: There are no images in memory matching selected area of interest [AOI]
11802   image files selected.
11803   Select image files to search
11804   Error: Could not obtain geo-referencing information from world file:
11805   Error: Cannot find world file for image:
11806   images selected.
11807   1 polyline without arcs found and ignored.
11808   record(s) of table
11809   transferred.
11810   Error: Source object does not contain the object tables selected for transfer.
11811   Please select an extended entity data application and atleast one field name to use for labeling.
11812   Please select an extended entity data application name.
11813   Please select an extended entity data field name.
11814   GeoTools discontinued command. Please use the 'GT_Xfer_Od_Xd' command instead.
11815   There are no extended entity data apps defined for transfer. Please run the 'GT_Xfer_Od_Xd' command first.
11816   The following extended entity data are attached to this object:
11817   Overwrite existing extended entity data?
11818   1 extended entity data of application
11819   Source object does not contain any extended data attached to it.
11820   Selected object does not contain any extended entity data belonging to application:
11821   Create text labels from Object table data / extended entity data.
11822   GeoTools discontinued command. Please use the 'GT_Od_Xd_Label' command instead.
11823   Exports multiple drawings in various formats
11824   1 3d Polyline found and was ignored.
11825   This command requires an empty drawing.
11826   Everything in the current drawing will be erased.
11827   Do you want to continue with this command?
11828   'GT_MultExport' warning
11829   Error: No export format selected. Please select an export format before exiting.
11830   Error: No drawings selected. Please select some drawings for export.
11831   building polygons were squared.
11832   Select building polygon polyline to square adjust:
11833   Error: Please select a polyline object only.
11834   Polyline segment:
11835   will adjust as displayed in
11836   Ok to accept?
11837   is already a right angle, skipped, no change.
11838   Specify segment lengths in a polyline.
11839   Contour elevation:
11840   Please note that all line/polyline segments with be either 2d or 3d for the join to be successful.
11841   A mix of 2d and 3d objects will not be joined.
11842   Place points (at user-defined spacing) along linear network
11843   Building master list of linear objects
11844   Objects traced:
11845   total trace length:
11846   Tracing network
11847   Select layer to place the nodes
11848   Weed points which are closer to each other than a specified distance.
11849   Converting text objects to attribute definitions...
11850   Convert attribute definitions to text objects
11851   Convert text objects to attribute definitions
11852   Select adjusted profile line for level re-computation:
11853   Enter datum height
11854   Enter horizontal exaggeration factor
11855   Enter vertical exaggeration factor
11856   Pick the point to show datum level:
11857   Select a sample text object to be used for level annotation:
11858   Enter horizontal annotation interval [or 0 to annotate at each vertex]:
11859   Error: Please pick a text object only
11860   Error: Only polylines can be picked as profile objects
11861   marker points created on layer:
11862   vertices snapped.
11863   Check ends of linear objects with coincident XY but with differing Z values.
11864   Checking elevations at ends of linear objects...
11865   coincident XY end points found.
11866   The coincident XY points have been marked on the GeoTools temporary layer:
11867   Adjust the levels created by a profile, based on a new modified cross-section profile line.
11868   1 Polyline with less than 3 vertices found and ignored
11869   Converting polylines to polyface mesh objects...
11870   Convert polylines to polyface mesh objects.
11871   Select text [counter] object to delete:
11872   Select block [counter] object to delete:
11873   Flip [mirror] arc segments of polylines
11874   Create output in which layer?
11875   Processing selection #
11876   Select polylines to place blocks/points:
11877   Vertex #
11878   Old.Elev =
11879   New.Elev =
11880   Next zig-zag point
11881   Next jump point
11882   Next centerline point
11883   Connect blocks in a specified order (based on attribute values)
11884   Creating list of blocks...
11885   Lowest point number:
11886   Highest point number:
11887   Place a stretched block along each segment of a line,polyline.
11888   Specify length of tangent:
11889   edge passes:
11890   <start point>:
11891   Vertex:
11892   Select text object for annotation [or RETURN to enter a string]:
11893   Enter annotation string
11894   or
11895   Select a block attribute to make upright (or type 'S' for settings):
11896   Move block attribute to a new location
11897   Select a block attribute to move:
11898   Pick new location for attribute:
11899   Rotate a block attribute
11900   Select a block attribute to rotate:
11901   Rotate block attributes so that they are readable
11902   Pick rotation angle:
11903   Please select some blocks first
11904   Convert block attributes to extended entity data.
11905   Transferring Block Attributes to extended entity data
11906   Modified WBLOCK command for BricsCAD, to be used to preserve AutoCAD Map data in DWG.
11907   Specify WBLOCK file name
11908   BricsCAD will now save your current drawing named
11909   and create a new WBLOCKed drawing called
11910   Ok to continue?
11911   This command is not available in AutoCAD.
11912   Object selection filters
11913   Selected Object :
11914   Object layer :
11915   Pick a point:
11916   Select dimension style(s)
11917   Select linetype(s)
11918   Select text style(s)
11919   Select a segment of line or polyline (or [S]ettings):
11920   Annotation length=
11921   Select TEXT object [or ENTER to create a new text]:
11922   Pick insertion point of text:
11923   Original length=
11924   You are currently running BricsCAD version
11925   It is HIGHLY recommended that you download and install BricsCAD Version 9.3.9 or above
11926   with GeoTools because of significant bug fixes and improvements in the geometry library.
11927   Please be aware that some of the GeoTools functions MAY NOT work correctly with this version of BricsCAD.
11928   Triangulating...
11929   Drawing triangles
11930   This command is available only in AutoCAD versions 2008 and above.
11931   Please select a tag to delete before exiting this dialog box.
11932   Layer to create offsetted polyline:
11933   Enter layer-name to set for offsetted polylines:
11934   Please select a block each to place at the start and end of the curve.
11935   Please select a block to place at the end of the curve.
11936   Please select a block to place at the start of the curve.
11937   Annotating ends of curves...
11938   Choose Z value entry mode
11939   Enter new Z value:
11940   Pick point to acquire Z from:
11941   Select TEXT object showing Z elevation:
11942   Ask 'Z Value Entry Mode' again while entering Z values
11943   GeoTools is a product of DesignSense Software Technologies, Bengaluru-INDIA
11944   In-memory settings of the command
11945   reset to default values.
11946   This is a FREEWARE command from GeoTools. This message will not appear in registered versions.
11947   Select a TABLE object:
11948   The TABLE object must be either an anonymous block or of type 'ACAD_TABLE'
11949   What do you want to do?
11950   Pick side to offset: Both/BOX/Layer/Xit <Xit>:
11951   Perform Bowditch's traverse adjustment
11952   Select traverse polyline to adjust:
11953   What type of traverse is this?
11954   Pick actual end-point of open traverse:
11955   Warning: The picked point has an elevation of 0.0. Ok to continue?
11956   There is no closing error in this traverse, therefore nothing to adjust.
11957   Compare block attributes and create a block-wise report
11958   Compiling/collating attribute list from block...
11959   Creating output list...
11960   Attribute tag Names
11961   Report file to create
11962   Update existing traverse and created adjusted geometry?
11963   Please select an attribute/object data field
11964   You have chosen 'None' for 'Store Point Descriptions/Numbers as'. They will be imported automatically. No further settings required.
11965   is already entered.
11966   Field value:
11967   Please select a field value to remove
11968   Save 'GT_EasyOD' parameters to INI file
11969   There are no field values entered yet. Please do so before attempting to save the parameter file.
11970   Restore 'GT_EasyOD' parameters from INI file
11971   WARNING: You are about to change the table name.
11972   Any pre-defined values you have set for the field names will be lost.
11973   You can Save the values to an ASCII file PRIOR to this operation, if required.
11974   Do you want to continue with this operation?
11975   'GT_EasyOD' warning
11976   Edit object data fields
11977   WARNING: You are about to change the block name.
11978   Any pre-defined values you have set for the attributes will be lost.
11979   un-used
11980   un-used
11981   'GT_EasyATT' warning
11982   Edit attribute values
11983   Attribute value:
11984   Please select an attribute value to remove
11985   Save 'GT_EasyAtt' parameters to INI file
11986   There are no attribute values entered yet. Please do so before attempting to save the parameter file.
11987   Restore 'GT_EasyAtt' parameters from INI file
11988   WARNING: You are about to restore a new set of parameters from INI file.
11989   Please select a block named
11990   Selected object does not contain any object data, new data record attached.
11991   Edit object table data, user-friendly, multiple-choice editor
11992   Edit multiple attribute data, user-friendly, multiple choice editor
11993   Orient text, mtext and attributes such that they are upright [readable].
11994   Select TEXT, MTEXT and/or blocks with attributes.
11995   Orienting text features
11996   Transfer AutoCAD Map Object table data into extended entity data(for BricsCAD editing).
11997   This command is meant to be run in BricsCAD or plain vanilla AutoCAD only.
11998   Select objects for Xdata to Object Data transfer
11999   Converting Xdata to Object data...
12000   Current INI file:
12001   Select DWG/block to insert
12002   Enter X Scale Factor
12003   Enter Y Scale Factor
12004   Folder:
12005   this folder has already been added to the list.
12006   added to list.
12007   Select folder for DWG files
12008   Select folder
12009   Save GT_DWGBrowser parameters to INI file
12010   Restore 'GT_DWGBrowser' parameters from INI file
12011   Please select a folder to display
12012   open polylines/splines were ignored and not processed.
12013   Select objects to label with handles.
12014   Enter horizontal offset distance
12015   Enter vertical offset distance
12016   Explode blocks to a specified layer
12017   Specify layer name to place the exploded blocks in:
12018   Exploding block...
12019   Enter line-width to set for block objects
12020   layer descriptions written to file:
12021   layer descripions read from file:
12022   Pick first annotation point:
12023   Pick next annotation point:
12024   Create annotations based on layer descriptions/interval distances.
12025   1 polyline object ignored. The 'Fit' method can be used only on SPLINE objects, and not on polylines.
12026   1 polyline object ignored. The 'Control' method can be used only on SPLINE objects, and not on polylines.
12027   1 polyline object ignored. The 'DXF' method can be used only on SPLINE objects, and not on polylines.
12028   Select objects to measure
12029   Enter or pick segment length
12030   Enter block name to place (or . for none)
12031   Align block with curve?
12032   Place points/blocks at start and end of curve also?
12033   Please select atleast one attribute tag to export
12034   Enclose with
12035   Object to use
12036   is too short to strip characters at specified location.
12037   is too short to add characters at specified location.
12038   new horizontally projected 3dFACE objects were created.
12039   First occurrence of code in xdata structure
12040   Second occurrence of code in xdata structure
12041   Third occurrence of code in xdata structure
12042   th occurrence of code in xdata structure
12043   Error: Could not find xdata at position=
12044   with code=
12045   Error: GeoTools cannot continue. Your computer does not have a valid 'Media Access Control' address.
12046   The GeoTools application key [using MAC-address] for this computer is
12047   The MAC-address based application key for this computer is
12048   Make polylines/3dfaces planar by setting elevations to adjacent vertices
12049   Enter tolerance for determining Z value match
12050   1 polyline ignored. Polylines must have exactly 4 or 5 vertices only.
12051   polyline(s) ignored. Either the vertex elevations match or they are exceed the specified tolerance.
12052   1 open polyline ignored.
12053   changed to
12054   Vertex insert mode?
12055   Pick a new location for the inserted vertex (or enter distance from mid-point):
12056   Creating block attributes report for block
12057   ***** Report of Block Attribute values *****
12058   *** Block Name:
12059   Unique Attribute values:
12060   Number of occurences:
12061   ***** Report of Block Attribute Tags *****
12062   GeoTools license file:
12063   found at
12064   not found.
12065   GeoTools is installed in the folder:
12066   GeoTools Version:
12067   This license file is for GeoTools for AutoCAD
12068   This license file is for GeoTools for BricsCAD
12069   as setup by the 'GT_EasyAtt_Setup' command.
12070   Select a block named
12071   or press ENTER to insert a new block:
12072   Pick insertion point for block
12073   Insert a block and position the attributes manually
12074   Enter block name
12075   Pick insertion point of block
12076   Error: Please select an attribute name before clicking 'Ok'
12077   Error: Attribute values have not been set. Please run the GT_EasyAtt_Setup command first.
12078   Change block layer and color based on attribute values.
12079   1 block object processed. Layer changed to:
12080   1 block object processed. Color changed to:
12081   1 block object ignored. No matching attribute value found.
12082   No record selected.
12083   Error: There aren't enough fields in the selected record. The handle is expected to be in field position #
12084   Error: Cannot locate object matching handle specified in field position #
12085   Enter ASCII file name
12086   Press the ENTER key to continue.
12087   Now displaying object
12088   with handle
12089   Error: 1 polyline ignored. The AREA command failed on this object. If you are running AutoCAD 2010, this could be due to AutoCAD bug. Please verify your results.
12090   Do you want to drape the source polylines across EVERY layer of target polylines individually?
12091   If you answer with a 'Yes', this will create a copy of NEW draped polylines in each layer of intersecting target polylines.
12092   If you answer with a 'No', only one draped polyline per source will be created across all layers of intersecting target polylines.
12093   'DrapePoly' Message
12094   vertices added.
12095   A new 3d draped polyline was created in the layer
12096   In BricsCAD, only the first 3000 records from the ASCII file will be displayed because of a bug/limitation of the dialog box control.
12097   Apply arithmetic/statistical operations on text objects
12098   Select blocks named
12099   Select TEXT/MTEXT objects:
12100   Error: Could not read block attribute named
12101   from selected block.
12102   The arithmetic mean [average value] of the selected numbers is :
12103   The median value of the selected numbers is :
12104   The mode [most frequently occuring value] of the selected numbers is
12105   The sum of the selected numbers is :
12106   The standard deviation of the selected numbers is :
12107   The geometric mean of the selected numbers is :
12108   The highest value amongst the selected numbers is :
12109   The lowest value amongst the selected numbers is :
12110   Pick point to place new BLOCK object:
12111   Pick point to place new TEXT object:
12112   The harmonic mean of the selected numbers is :
12113   Select HATCH objects to create a report on:
12114   HATCH pattern report
12115   *** SOLID & GRADIENT fill hatch
12116   Area under SOLID fill hatch:
12117   Area under 1-Color Gradient hatch:
12118   Area under 2-Color Gradient hatch:
12119   sq.units  [# of objects =
12120   *** PATTERN hatches
12121   Area under the hatch
12122   vertices changed in
12123   3D Polyline(s)
12124   (shown in highlight):
12125   Delete selected paper-space layouts
12126   There is only 1 paper-space layout named
12127   and it cannot be deleted
12128   Select layout(s) to delete
12129   Layout:
12130   deleted.
12131   Flip the Entity Coordinate Systems of all arcs with negative WCS normals.
12132   Select ARC objects [only those with negative WCS normals will be processed]:
12133   arcs with negative WCS normals were flipped.
12134   No arcs with negative normals were found.
12135   zero-length or single-vertex polylines deleted.
12136   Bearing and Distance command
12137   Enter or show text size
12138   Bearing & Distance->From point [ENTER to finish]:
12139   Bearing & Distance->To point:
12140   Draw cross-section lines across TIN limits, compute cross sections and volumes.
12141   Select a closed polyline representing the area to be processed [or ENTER to profile a single 3D polyline]:
12142   Creating profiles, processing 3dpolyline....
12143   Selected object is not a closed polyline.
12144   Selected object is not a polyline.
12145   Enter to show cross-section profile sampling interval [spacing]:
12146   <Enter orientation angle> or pick two points to show angle: First point:
12147   Pick second point to show angle:
12148   Cross-section angle set to
12149   degrees
12150   Select layer for outline polyline
12151   Select a TEXT or MTEXT object:
12152   Your FIXED hard disk drive identification could not be found.
12153   You will need to register this computer using the MAC-address based appkey, obtained by typing 'GT_AppKey' on the command line.
12154   Please contact 'rakesh.rao@thedesignsense.com' for assistance.
12155   Error: Please select a TEXT or MTEXT object only.
12156   Edit extended entity data in a dialog-box interface
12157   Select an object to view/edit Xdata:
12158   XDATA written and saved in the object.
12159   Error: Selected object has no xdata attached to it.
12160   Select 3dface objects representing the TIN model [or ENTER to type layer name(s)]
12161   Select 3d polyline objects representing the TIN model [or ENTER to type layer name(s)]
12162   Reading TIN
12163   Read
12164   triangles in memory.
12165   Select layer for slope representation
12166   Show all CADPower Toolbars.
12167   Hide all CADPower Toolbars.
12168   You can Flip it across the curve / Reverse the direction / Mirror the text / Tumble it over or simply exit if all is well.
12169   text objects placed in active[previous] selection set.
12170   Object type :
12171   is not supported for curve text labeling.
12172   Enter or show text offset distance from curve
12173   Enter or show spacing between each character
12174   Enter or show spacing between each word
12175   Enter to show text height
12176   Enter to show annotation interval
12177   Does the text look good?
12178   Your trial or subscription period for registering CADPower has passed.
12179   Refer to your documentation 'Register_CADPower.Txt' for instructions
12180   on how to register your CADPower
12181   Please contact your CADPower distributor from whom you bought
12182   Successfully read CADPower registration information...
12183   The 30-day grace period for registering CADPower was from
12184   CADPower notification
12185   CADPower Registration Notice
12186   Thank you for your interest in CADPower software.
12187   This is a 30-day evaluation copy of CADPower.
12188   All users are required to register CADPower within 30 days
12189   Please refer to your documentation 'Register_CADPower.Txt' on how
12190   to register CADPower.
12191   Thank you for downloading this evaluation copy of CADPower
12192   CADPower can be purchased online through our website at
12193   Once you purchase CADPower, your order will be shipped to
12194   the file CADPowerOrderForm.Txt located in your installation folder
12195   *This notice does not appear once CADPower has been registered*
12196   CADPower is a product of DesignSense Software Technologies Pvt. Ltd., Bengaluru-INDIA
12197   CADPower is a product of DesignSense Software Technologies, Bengaluru-INDIA
12198   CADPower license information
12199   does not have any active & valid CADPower portable license installed.
12200   You will need to register this computer using the MAC-address based appkey, obtained by typing 'CP_AppKey' on the command line.
12201   The 'CADPowerUser25_??_??.RGS' file that you are using is not authorized for this computer
12202   Please obtain a valid user registration file for this computer from your CADPower
12203   dealer or from DesignSense Software Technologies Pvt. Ltd.: rakesh.rao@thedesignsense.com
12204   You will need to send us your application key to authorize your use of CADPower
12205   on this computer. This can be obtained now by typing 'CP_AppKey' on the command line
12206   Please see 'Register_CADPower.Txt' for further instructions on how to obtain a valid user registration
12207   Your current CADPower license file is valid for the following application keys:
12208   Your current CADPower license file is valid for the following serial numbers:
12209   Error: CADPower cannot continue. Your computer does not have a FIXED hard disk.
12210   Error: CADPower cannot continue. Your computer does not have a valid 'Media Access Control' address.
12211   CADPower Version
12212   CADPower is a product of DesignSense Software Technologies Pvt. Ltd..
12213   About CADPower
12214   GeoTools Order form
12215   CADPower Order form
12216   CADPower readme & installation instructions
12217   CADPower is in Script Mode. All commands will now display a non-dialog box interface.
12218   CADPower is in dialog box mode. All commands will now display a dialog box interface.
12219   Delete block attribute tag(s) and update all inserted blocks
12220   license file cannot not found.
12221   Software End User License Agreement [E U L A]
12222   Turn Command-line mode?
12223   CADPower license file:
12224   Error: Please check the folder permissions for the license folder location:
12225   CADPower requires create, write & delete permissions in this folder.
12226   Floating license master file found at location:
12227   This computer
12228   has already logged in as a CADPower user.
12229   A new license will NOT be issued for this computer
12230   The existing license will be used.
12231   has been added to the CADPower logged-in users list.
12232   A new license HAS BEEN ISSUED for this computer
12233   Error: Reached the maximum number of
12234   simultaneous users.
12235   There are no more floating licenses available at the moment.
12236   Please try after some time.
12237   Error in floating license file. Number of licenses should be greater than 0. CADPower will exit now.
12238   Please contact technical support.
12239   Attempting to read floating license transaction file...
12240   License transaction file cannot be accessed. Operation timed out.
12241   Please try again or contact your network administrator for help.
12242   Error in floating license file. The path
12243   cannot be accessed and/or the file cannot be found.
12244   Error trying to locate floating license file. There is no location path set for the license file.
12245   There is no close down reactor to remove.
12246   Error: Cannot find floating license transaction file.
12247   The file
12248   cannot be found
12249   Error in floating license file. The file
12250   GeoTools requires create, write & delete permissions in this folder.
12251   has already logged in as a GeoTools user.
12252   has been added to the GeoTools logged-in users list.
12253   Error in floating license file. Number of licenses should be greater than 0. GeoTools will exit now.
12254   GeoTools Message
12255   CADPower Message
12256   GUID file was found and your license file was updated.
12257   GUID File could not be obtained. Maybe there is no internet connection
12258   Your license file DOES NOT contain GUID info.
12259   In this mode, you have to select a sample template block in the 'Block Name' section at the top of the dialog and also specify the attribute options setup as usual
12260   All block names matching the wildcard based filter criteria will be processed with the expectation that each one of them have attributes similarly named as the template block.
12261   Error: You must select a block with attributes only.
12262   Attribute
12263   populated with value
12264   Select a block whose name matches the wildcard
12265   Please specify a text editor before clicking the 'Ok' button
12266   Select text editor executable [EXE] file
12267   Enter EASYATT parameters file name (use forward slash for pathing)
12268   <not yet determined>
12269   Enter EASYOD parameters file name (use forward slash for pathing)
12270   Edit XDATA in a dialog box interface
12271   Select an object to view/edit Xdata:
12272   Edit Xdata values
12273   XDATA written and saved in the object.
12274   Select 3dface objects which form an enclosing area.
12275   Change object visibility to:
12276   1 polyline was in a non-parallel UCS and has been ignored.
12277   Convert extended entity data to AutoCAD Map Object Table data
12278   Type mismatch: Cannot link XDATA code
12279   to object data field type
12280   Unsupported field type. Cannot link to this field type.
12281   Please select an object table, object field, xdata application, and xdata field before you can link.
12282   Please select XD-2-OD mapping to unlink.
12283   There is no XD-2-OD conversion mapping specified. Please use the 'Link' button to do so before you can proceed further.
12284   Please select an Xdata Code to search for.
12285   Please select a 3d polyline object only.
12286   Please select a polyline object only.
12287   Select
12288   to snap to polyline.
12289   Select text objects to round off bearings.
12290   Selected polyline is not a 3d polyline. Convert to 3d polyline?
12291   Select source polyline to acquire elevations into:
12292   Select target polyline to acquire elevations from:
12293   Change the order of attributes in a block
12294   Warning: There are no attribute definitions (ATTDEFs) in this drawing.
12295   Already at the top of the list.
12296   Already at the bottom of the list.
12297   Error: No attribute definitions(ATTDEF) have been selected for reordering
12298   Enter block name(s) to process [separated by commas]
12299   Enter layer name(s) to process [separated by commas]
12300   Enter XD2OD INI file to read
12301   Save mapping parameters: Select XD2OD INI filename
12302   Restore mapping parameters: Select XD2OD INI file
12303   CADPower File Manager - Copy, Move, Erase, Count, Touch your files.
12304   already exists and will not be over-written.
12305   Copying...
12306   (done)
12307   not processed [does not meet the date/time filter criteria].
12308   Moving...
12309   Deleting...
12310   Touching (date/time)...
12311   Counting files...
12312   There are no files matching the filter criteria
12313   in the folder:
12314   Select root folder to process files from
12315   All files matching the filter criteria located in this folder and all folders beneath it will be processed.
12316   Select root folder to process files to
12317   This category of commands is not licensed.
12318   Please send an email to 'rakesh.rao@thedesignsense.com' and request a
12319   category license.
12320   Additional payment applies.
12321   GeoTools license manager message
12322   CADPower license manager message
12323   Select dimension entities to change precision.
12324   Specify a precision for the dimension:
12325   MatchProp: Select entity to copy properties from:
12326   Select objects to copy properties to:
12327   Creates a new skin for BricsCAD, offering familiar commands in familiar locations.
12328   Found file:
12329   Cannot find file:
12330   Cannot find 'CADPower.VLX' file to determine installation folder
12331   File deleted.
12332   The file
12333   was NOT found.
12334   was FOUND.
12335   You do not need an update now. The
12336   version
12337   on this computer is the latest version.
12338   The
12339   version on this computer, V
12340   There is a newer version, V
12341   available for download. Do you want to download now?
12342   is newer than the version, V
12343   available on the web. You do not need an update now.
12344   Error: The
12345   version info file does not exist on our web-site.
12346   version info file could not be downloaded.
12347   Perhaps there is no internet connection available.
12348   Please check and try again.
12349   This computer is licensed based on the appkeys [machine-id]
12350   This computer is licensed based on the CAD software serial number.
12351   This computer is licensed with a GeoTools floating license.
12352   Floating license file location:
12353   Floating license file was FOUND at the above location.
12354   Floating license file was NOT FOUND at the above location.
12355   The GUID assigned to this license is:
12356   GUID Check on the internet is enabled.
12357   GUID Check on the internet is disabled.
12358   is not registered. No license information is available.
12359   Expires
12360   This computer is licensed with a CADPower floating license.
12361   This license file is for CADPower for AutoCAD
12362   This license file is for CADPower for BricsCAD
12363   Enter layer name(s) to process, separated by commas (or . to select)
12364   Add another feature class?
12365   created successfully [for KMZ export].
12366   Enter KML file name
12367   Enter KML Document name
12368   Enter KML Document description
12369   Error: Cannot find 'EXIFTOOL.EXE' in the search path.
12370   Please ensure this executable file is available.
12371   Error: Cannot find '7Z.EXE' in the search path.
12372   Error: Cannot find '7Z.dll' in the search path.
12373   Please ensure this DLL is available.
12374   Enter KML Folder name
12375   Enter KML Folder id
12376   Additional extracts: Export 'Object Type'?
12377   Additional extracts: Export 'Object Handle'?
12378   Additional extracts: Export 'Layer'?
12379   Additional extracts: Export image data attached to objects (defaults to KMZ output)?
12380   Additional extracts: Export image data attached as URL (defaults to KMZ output)?
12381   What to export?
12382   XDATA application name to export
12383   Enter XDATA code to use as KML object label
12384   Position of XDATA code (for object label) from start
12385   Position of XDATA code (for attached image) from start
12386   Block name to process (for data export)
12387   Enter attribute name for KML label
12388   Enter attribute name for attached image export
12389   Object table name to export (for data export)
12390   Enter object data field name for KML label
12391   Enter object data field name for attached image export
12392   Create binary variant (KMZ) file also?
12393   Tokenize fields where a 'Par=Value' character is present, and export only the 'Value'
12394   Perform Lat-Long validity check?
12395   Select objects to convert into KML format
12396   (exists)
12397   (does not exist)
12398   Save drawing objects into KML file
12399   KMZ Binary output enabled.
12400   copied.
12401   deleted.
12402   Error 1: No EXIF data was found on this object
12403   Error 2: No EXIF data was found on this object
12404   WARNING: This co-ordinate
12405   is outside the limits of geographic data
12406   Permitted range for geographic coordinates: -90.0 < Lat < 90.0 |and| -180.0 < Long < 180.0
12407   You choices are:
12408   1. Stop processing - you must correct the data before restarting again
12409   2. Allow processing - export the data to KML as they are (this process only).
12410   Please select your choice:
12411   Stop
12412   Allow
12413   'GT_Dwg2Kml' warning
12414   Select objects for coordinate conversion
12415   Source coordinate system:
12416   Target coordinate system:
12417   [POINT] Source [original] coordinate:
12418   [POINT] Target [transformed] coordinate:
12419   [INSERT] source [original] coordinate of insertion point:
12420   [INSERT] target [converted] coordinate of insertion point:
12421   [VERTEX]: Source [oringinal] coordinate:
12422   [VERTEX]: Target [converted] coordinate:
12423   Do you want to zoom to the transformed objects?
12424   Hit the ENTER key to continue with Wblock'ing the transformed objects.
12425   Save transformed drawing objects as
12426   Error: Source and target coordinate systems cannot be the same
12427   The processing choices you have made performs only a datum shift operation
12428   No coordinate conversion is performed during this process
12429   If you are sure this is what you want, click on 'Proceed' below
12430   Else, you can re-specify your coordinate conversion parameters and try again
12431   Proceed
12432   Go Back
12433   'GT_COORDTRAN' warning
12434   Please select a target coordinate system before clicking 'Ok'
12435   Please select a source coordinate system before clicking 'Ok'
12436   Please select a reference ellipsoid before clicking 'Ok'
12437   Error: Lat-Long coordinates not in range.
12438   Eccentricity:
12439   Inverse flattening:
12440   Flattening:
12441   GeoTools is not authorized to run on this computer because this appkey
12442   has been disabled. Please contact GeoTools support.
12443   CADPower is not authorized to run on this computer because this appkey
12444   has been disabled. Please contact CADPower support.
12445   This is a FREEWARE command in CADPower. This message will not appear in registered versions.
12446   Please make sure you type the attribute name(s) accurately.
12447   Multiple attribute names must be separated by commas.
12448   If blocks do not contain the specified attribute(s), they will be ignored.
12449   Old text:
12450   New text:
12451   Your current GeoTools license does not include the GEOLOGICAL & MINING module
12452   Select 2d object for cross-section profile:
12453   Selected polyline is 3d: cross-section profile can only be a 2d object.
12454   Selected polyline is open: cross-section profile should be closed.
12455   Selected spline is open: cross-section spline should be closed.
12456   Selected object is not parallel to current UCS.
12457   Please select a closed 2d polyline, spline / ellipse or region object
12458   Select path curves.
12459   Extruding objects...
12460   Please select a pattern for extruding.
12461   Create new consolidated object as:
12462   Pick Insertion point of TEXT:
12463   Delete original text objects?
12464   Lineweight:
12465   Dimension Style:
12466   Polyline width:
12467   attribute tag[s]
12468   Select blocks [for update]
12469   times
12470   Vertex #
12471   X-Coord
12472   Y-Coord
12473   Z-Coord
12474   SegmentLength
12475   SegmentSlope(%)
12476   SegmentSlope(degs)
12477   Azimuth(Bearing)
12478   CADPower is installed in the folder:
12479   Make text upright
12480   Algorithm Copyright 2008 Jeff Winship. Re-used in CADPower with permission
12481   Select 3-sided planes, can be 3dfaces or 3d polylines:
12482   1 polyline with more than 3 vertices ignored.
12483   Intersection Objects: with [P]rojectedPoints/[L]ines?
12484   Mark Intersections: [A]ctual intersections only/[P]rojected intersections also?
12485   Select POINT objects to project [intersect] with this plane.
12486   Select LINE objects to determine intersection with this plane.
12487   Error: please select a 3dface or polyline object only.
12488   Error: 1 line skipped. The selected point and plane are coplanar.
12489   Projected intersection point created at:
12490   Error: 1 point skipped. The selected point and plane are coplanar.
12491   Projected [actual] intersection point created at:
12492   Do you want to join the original points and their projected intersection with lines?
12493   Compute detailed paper space statistics?
12494   Error: Cannot set text value to an empty string.
12495   text objects were reduced to empty strings after trimming and were deleted.
12496   CADPower Block Names Manager
12497   Block Name
12498   Error: Cannot rename block
12499   destination block
12500   Error:Cannot rename block
12501   Block
12502   Please select some block name(s) first
12503   Enter CSV Export file name
12504   CSV Export file:
12505   Enter delimiter to use in file
12506   Enter number of columns in CSV file
12507   Enter text scan direction
12508   Delimiter:
12509   Number of columns in CSV file:
12510   Scan direction:
12511   Select column #
12512   of text.
12513   Selection for column #
12514   has
12515   First column has
12516   objects. All other columns must have same number of objects in the selection
12517   Exporting CSV file
12518   Error: Current selection has
12519   Number of objects in each column must be
12520   as set by the first column size.
12521   Select points, blocks to triangulate:
12522   You have selected
12523   objects. Do you want to process them in (P)arts or (A)ll together?
12524   Number of rows and columns to split into
12525   Selection has
12526   Slope of triangle:
12527   Color
12528   (processed)
12529   (ignored)
12530   Pick start point of SLOPE table:
12531   StartSlope(%)      EndSlope(%)         Color               Area (sq.units)
12532   There are no
12533   objects in the selection.
12534   Select 3DFACE or 3DPOLYLINE to determine slope:
12535   Error: Please select a 3 or 4 vertex polyline only.
12536   Error: Please select a 3dpolyline or 3dface object only.
12537   Select a VIEWPORT to update clipping boundary:
12538   Select a clipping entity:
12539   Please select a polyline or circle entity only for clipping boundary.
12540   This viewport is not clipped.
12541   Select a VIEWPORT to extract boundary:
12542   A VIEWPORT boundary polyline with
12543   vertices created.
12544   A CIRCLE entity (representing viewport boundary) created.
12545   This viewport has not been clipped.
12546   You must pick a VIEWPORT entity.
12547   StartSlope(degs)   EndSlope(degs)      Color               Area (sq.units)
12548   The subtraction of the selected numbers is :
12549   The multiplication of the selected numbers is :
12550   Enter BOM parameter INI file name
12551   WARNING: There is an existing table in this drawing
12552   What do you want to do with it?
12553   Your choices are:
12554   1. Delete this table and specify a new table location
12555   2. Keep the table as it is. Create a new one now.
12556   Please select your choice:
12557   'CADPower BOM/BOQ message'
12558   Do you want to scale the BOM?
12559   Enter BOM scale factor
12560   CADPower BOM module: Report of attribute tags defined in the INI file v/s what was found in the block
12561   *** List of attribute tags defined in the INI file FOUND in the block:
12562   INI file:
12563   *** List of attribute tags defined in the INI file and NOT FOUND in the block:
12564   (none)
12565   CP_BOM Message: Warning: There are no blocks in this drawing.
12566   You can run only the 'Import Table' option in this run
12567   All existing attribute tag mapping in your INI file
12568   will be retained and not changed.
12569   Any new tags added will have a default description.
12570   You may change it as necessary using the 'Edit' option.
12571   Please confirm:
12572   Error: Please select a block with attributes, to export tags into INI file.
12573   Error: You can perform this operation only when you are doing an 'Attribute Extract' BOM
12574   Error: Please enter a valid attribute template file.
12575   Any pre-defined block names in your existing INI file will be
12576   retained. New block names will be added with a default description
12577   You may edit it later with the 'Edit'  option.
12578   Error: There are no blocks selected.
12579   Error: Please enter a valid attribute export file.
12580   Error: Please enter a valid attribute import file.
12581   Please select an index attribute first.
12582   Please select a block name first.
12583   Error: The specified attribute template file
12584   cannot be located.
12585   Please choose an INI file or create one by clicking on 'Save' button in the dialog box
12586   Export file (comma delimited text-CSV)
12587   Import file (comma delimited text-CSV)
12588   Select BOM parameters definition file
12589   Select 'BOM/BOQ' template
12590   Creating table header...
12591   Creating table contents...
12592   records written on file.
12593   Importing ASCII file...
12594   Updating attributes...
12595   with
12596   1 block with matching handle not found, attribute update skipped.
12597   1 block not found, import file does not contain handle.
12598   Warning: Attribute extract INI file has not yet been set. Any parameters set will not be saved.
12599   Use the 'Save' button to save and create an INI file
12600   Temporary block named
12601   was ignored and not added. Please add it manually if you want.
12602   viewport(s) in current layout
12603   display locked.
12604   Error: You must be in a paper-space layout for this command to function.
12605   display un-locked.
12606   Processing layouts...
12607   viewports
12608   viewport(s) display locked.
12609   viewport(s) display un-locked.
12610   unlocked
12611   locked
12612   (no viewports)
12613   Select block to edit:
12614   Enter attribute to update with scale values (. for none)
12615   Do you want to interactively edit the X Scale factor?
12616   Enter X Scale factor increment
12617   Enter or pick anchor point (default=insertion point)
12618   Anchor point must be on the block, ideally one of the edge-point of the tile.
12619   X Scale changed from
12620   Continue again?
12621   Error: It is not possible to further re-scale the block due to technical reasons.\nPlease run the command again to continue.
12622   Do you want to interactively edit the Y Scale factor?
12623   Enter Y Scale factor increment
12624   Y Scale changed from
12625   Enter data definition INI file name
12626   Use real values precision from INI file?
12627   Error: XDATA structure in entity does not match the XDATA structure in INI file.
12628   Error: Number of XDATA records in entity does not match the number of XDATA records defined in INI file.
12629   Updating XDATA....
12630   Error: There are no sections in the INI file.
12631   The CP_LINEQTY tool performs total weight & cost calculation based on 'per unit length' values
12632   It requires that you have atleast 3 fields denoting a 'Name', 'Weight per unit length' and 'Cost per unit length' parameter in the same order.
12633   The first parameter 'Name' [STRING] identifies the linear item under consideration
12634   The second parameter 'Weight per unit length' [REAL] denotes the weight of the item per unit of dwg length
12635   The third parameter 'Cost per unit length' [REAL] denotes the cost of the item per unit of dwg length.
12636   The fourth optional parameter 'Supplier' [STRING] denotes the supplier of manufacturer of the item under consideration
12637   'CADPower CP_LINEQTY message'
12638   Select linear objects for quantity calculation:
12639   Cost per unit length=
12640   Weight per unit length=
12641   Total Weight
12642   Name
12643   Total Cost
12644   Total Length
12645   Number of items
12646   WARNING: There is an existing CP_LINEQTY table in this drawing
12647   Supplier/Mfgr
12648   Enter table scale factor
12649   Enter quantities export file-name
12650   There is no data available to create output table.
12651   Enter gap distance
12652   Select a rectangular sheet (or type 'S' for settings):
12653   Success: You have picked a perfect rectangle/square.
12654   The sides are:
12655   Pick first cut point:
12656   First point vertex: 
12657   Error: Please pick a closed polyline only.
12658   Pick adjacent side end-point:
12659   Pick point to slide to:
12660   Pick point to slide from:
12661   Select a closed polyline:
12662   Error: Polyline must have exactly 4 vertices.
12663   Error: The two pairs of sides are not identical. It is not a rectangle.
12664   Error: The sides of the 4-sided figure do not form a rectangle.
12665   Success
12666   Error: The position of the picked points cannot be determined.
12667   Warning: Opposite sides of the polygon were not picked. You probably picked adjacent sides.
12668   Enter or show new distance from start point:
12669   Segment length:
12670   distance from start point:
12671   Opposite sides picked.
12672   Second point vertex = 
12673   Symmetric cut
12674   Pick second cut point (or type S for Symmetric cut):
12675   Perform automatic segment length roundoff?
12676   Enter round-off value for segment lengths
12677   Original length of segment #
12678   New length:
12679   Floor Footprint layer   :
12680   Wall layer              :
12681   Window layer            :
12682   Door layer              :
12683   Ventilator layer        :
12684   Lofts layer             :
12685   Annotations layer       :
12686   Fixtures layer          :
12687   Current Floor           :
12688   Select a floor footprint polyline:
12689   Selected object is not in the current foot-print layer
12690   Do you want to change it to the current foot-print layer?
12691   Error: Please pick only a heavy-weight polyline or line object.
12692   Select SpacePlanner parameters definition file
12693   Wall #
12694   Set wall height:
12695   Default wall height:
12696   Pick point to draw the wall:
12697   Current opening type:
12698   OpeningType
12699   Width =
12700   Height =
12701   Depth =
12702   Enter sill height from floor level
12703   Height:
12704   Fixture:
12705   [in plan] placed at a sill level of
12706   from floor level.
12707   Warning: There is no wall elevation view associated with this wall segment.
12708   Cannot determine the wall to place the fixture on.
12709   Error: No wall footprint found in layer
12710   at picked point.
12711   Wall found. No numbering info available.
12712   [in elevation] placed at a sill level of
12713   Enter horizontal distance from LEFT edge of wall [ENTER 0 to skip]
12714   Enter horizontal distance from RIGHT edge of wall [ENTER 0 to skip]
12715   placed at a distance of
12716   from LEFT edge of wall.
12717   from RIGHT edge of wall.
12718   Error: Cannot locate a wall in which this fixture can been placed.
12719   A new
12720   opening size of
12721   was added to the list
12722   placed at a sill level of
12723   Elevation Wall found. No numbering info available.
12724   Warning: Elevation wall and plan wall segment have different wall numbers.
12725   Elevation wall segment number:
12726   Plan wall segment number:
12727   Warning: SpacePlanner parameters INI file has not yet been set. Any parameters set will not be saved.
12728   Use the 'Save' button to save and create an INI file
12729   Error: Cannot find parameters INI file
12730   Reading parameters INI file
12731   Wall-Opening area schedule Export file (comma delimited text-CSV)
12732   Select annotations layer
12733   Wall/Openings Schedule
12734   CSV output file
12735   Pick point for table of quantities:
12736   Type
12737   Size
12738   Quantity
12739   Unit Area
12740   Total Area
12741   Unit Cost
12742   Total Cost
12743   Grand Total Openings Area:
12744   Grand Total Wall Area:
12745   Net Wall Area:
12746   Total Openings Area:
12747   Total Area:
12748   Total Cost:
12749   Schedule of fixtures/openings:
12750   Floor Number:
12751   Current Floor:
12752   1 entity without XDATA was ignored.
12753   1 block object ignored.
12754   Select wall [front-view] entities and associated openings.
12755   Wall entities must be selected from
12756   layers only.
12757   1 entity ignored, was in incorrect layer. Current Floor:
12758   Openings layer:
12759   selected
12760   Do you want to put numbering before the text?
12762   You must specify a name for target block.
12763   You must specify a name for source object table.
12764   'Annotation Expert' Version
12765   'Conversion Expert' Version
12766   'Draw Expert' Version
12767   'Miscellaneous Expert' Version
12768   'Polyline Expert' Version
12769   'Quantity Expert' Version
12770   'Text Expert' Version
12771   CADPower is a product of DesignSense Software Technologies.
12772   GeoTools is a product of DesignSense Software Technologies.
12773   'Blocks Expert' Version
12774   Select symbols to insert
12775   Pick second cut point:
12776   Select a polygon to cut (or type 'S' for settings):
12777   Draw 3D spline with elevation prompts
12778   Next point of spline
12779   Enter spline point elevation
12780   Cannot close a 3d spline with less than three points.
12781   Switching to World coordinate system...
12782   overlapping objects move to $DUPLICATE$ layer.
12783   overlapping objects(s)
12784   Overlapping objects moved to $DUPLICATE$ layer and placed in active [previous] selection set...
12785   There are no overlapping objects in the selection.
12786   WARNING: Anchor point picked is not on the block.
12787   X Scale:
12788   Y Scale:
12789   See more placement options?
12790   ***on_doc_load.lsp file is found in the following
12791   location(s)
12792   license file is found in the following
12793   Enter CADPower command to display online help (needs internet)
12794   Enter CADPower command to display online help (needs internet)
12795   ** This command requires internet connection.
12796   is not accessible.
12797   Local copy:
12798   found.
12799   There is no Youtube video associated with the command
12800   The command
12801   does not exist in the lookup table of either GeoTools or CADPower.
12802   System folders
12803   Windows desktop
12804   Start Menu\Programs
12805   My Computer\Control Panel
12806   My Computer\Printers
12807   My Documents
12808   <user name>\Favorites
12809   Start Menu\Programs\Startup
12810   Recycle Bin
12811   User Desktop
12812   My Computer
12813   Network Neighborhood
12814   Windows fonts
12815   Application Data
12816   Windows directory
12817   System directory
12818   Program Files
12819   My Pictures
12820   Select a folder option to browse to [0 to exit]
12821   System folders cannot be displayed in BricsCAD Classic.
12822   Drawing folders
12823   Current drawing folder
12824   Xref Load Path
12825   BricsCAD Search path
12826   Save File Path
12827   Chapoo Temporary folder
12828   BricsCAD ImageCacheFolder
12829   Local Root Folder
12830   Roamable Root Folder
12831   Temporary files folder
12832   Texture Map Folders
12833   Render Materials Folder
12834   Read-only path for static render materials, like preview
12835   Path to the Sheet Set Template folder
12836   Path for relative hyperlinks
12837   Path to the default mnu (cui)
12838   Most recently used path
12839   Stores a list of project names, each holding list of folders
12840   Path to the log file
12841   Path to tool palette folder(s) [multiple]
12842   Path to the sheet set templates folder
12843   Path to the drawing templates folder
12844   Default path for creating plot files
12845   Plotter Configuration Folder
12846   Specifies path to the plot style folder
12847   *** PAT file***:
12848   Do you want to check hatch patterns in this file
12849   hatch patterns in this file.
12850   Press ENTER to continue
12851   Do you want to compare two PAT files?
12852   Enter the two numbers of the files [separated by commas] you want to compare
12853   First  PAT file:
12854   Second PAT file:
12855   Hatch patterns common in both files:
12856   common hatch patterns in this file.
12857   Common patterns=
12858   Hatch pattern found in (1) but not in (2):
12859   Hatch pattern found in (2) but not in (1):
12860   Error:Both PAT files selected are the same.
12861   Error: please type two numbers separated by comma.
12862   Select points/blocks to draw Voronoi polygons.
12863   Enter or show maximum TIN triangle length
12864   'GeoTools GT_TRIANGULATE message'
12865   WARNING: If your selection contains exact duplicate points, it will be ignored and not processed twice
12866   If there are points with identical X & Y values but differing Z values, this can cause errors and a crash
12867   You are advised to identify and fix these kinds of data to ensure a smooth processing and creation of TIN data
12868   This option is available in BricscAD only.
12869   There are no BricsCAD installations in this computer.
12870   There are no AutoCAD installations in this computer.
12871   Creating profiles, processing 3dpolyline....
12872   Skipping polyline....
12873   Error: File
12874   could not be opened for writing.
12875   RouteName
12876   SerialNumber
12877   Chainage
12878   Seg.Length
12879   Easting
12880   Northing
12881   Height
12882   Enter tile block name(s) to count (comma delimited)
12883   Enter tile-count BOQ parameters INI file name
12884   All blocks have 3D information in them.
12885   All blocks do NOT have 3D information in them. Will be considered as 2D.
12886   Size-wise Report:
12887   Warning: There is no cost defined for the block
12888   for size
12889   Please check your INI file or select a different block.
12890   Material Name:
12891   Quantity:
12892   Cost:
12893   Time:
12894   Additional Resources\nMaterial
12895   Pick insertion point of
12896   Enter SIZE table scale factor
12897   records written on file.
12898   sizes with no cost information in the INI file.
12899   Do you want to add these to the INI file with a dummy cost of 0.0? You can edit it later.
12900   Current settings:
12901   Tile block            :
12902   Image in block        :
12903   Attributed block      :
12904   Size Attribute        :
12905   Description Attribute :
12906   Warning: There are no material/resource information attached to this object. No resource info added.
12907   Width [horizontal] of tile:
12908   Height [vertical] of tile:
12909   Pick insertion point of tile:
12910   Select polygonal area to fill:
12911   Error: Please select a closed polyline/spline object.
12912   Error: Could not detect segment.
12913   Error: Please select a closed area object only.
12914   Processing panels....
12915   Select tile blocks to offset:
12916   Do you want to select the entire row of tile blocks?
12917   Select direction and distance to scan along the blocks (or S to swap):
12918   Additional Resources, if specified in the INI file, will be attached to the tile objects.
12919   Please select a TILE block first.
12920   The picked dimensions will be rounded off to the nearest multiple of
12921   in X and
12922   in Y, as specified in this dialog.
12923   Select size attribute
12924   Select description attribute
12925   Select an image file
12926   already exists in current drawing.
12927   WARNING: Block
12928   Define a new block by this name?
12929   'CP_TILEPLACE message'
12930   Additional parameters for this command can be set using the CP_TILEPLACE command.
12931   Select a closed polygonal region to cover:
12932   Floor:
12933   Component:
12934   WallNum:
12935   Pick origin point:
12936   Pick next point for alignment direction:
12937   Enter block name to use (or create)
12938   Enter tile description
12939   Enter layer for placing tiles
12940   Enter or show X dimension
12941   Enter or show Y dimension
12942   Enter or show roundoff dimension in X (along) direction
12943   Enter or show roundoff dimension in Y (across) direction
12944   Enter or show gap in X (along) direction
12945   Enter or show gap in Y (across) direction
12946   Enter joint stagger (offset) distance (in X direction)
12947   Is it a 3d element?
12948   Enter the Z (depth) dimension
12949   Enter size attribute(or . for none)
12950   Enter description attribute(or . for none)
12951   Ignore closed regions inside main polygon?
12952   Additional resources to be added to these tiles?
12953   Error: polylines should not have arc segments.
12954   Error: Please select a closed polyline only.
12955   Block definition
12956   already exists and will be used.
12957   already defined. Over-write it?
12958   The tile block
12959   will have two attributes, SIZE and DESC.
12960   Do you want to make the DESC attribute invisible?
12961   Do you want to make the SIZE attribute invisible?
12962   Select TILE block to edit:
12963   Enter or pick anchor point (default=insertion point)
12964   Anchor point must be on the block, ideally one of the edge-point of the tile.
12965   Are there more blocks in the same orientation to be fixed with the same parameters?
12966   Select direction and distance to scan along the blocks (or S to swap):
12967   Error: Please select a block INSERT object only.
12968   This section is used during the 'Count BlockNames' BOQ workflow
12969   Here, you must specify the block name followed by (=) and the description, cost, time(or weight),Code,......
12970   <BlockName>=<Description>,<Cost>,<Time-or-Weight>,<Code>
12971   For example:
12972   BALOON_BLOCK=Standard baloon,150.00,2.0,1.3,998766
12973   BP-PLATE=Base Plate-generic,100.00,1.5,0.5,998772
12974   BP-SB=Base Plate Square,200.00,3.4,1.2,998665
12975   (these are pre-defined constants, put them in any order you like)
12976   LENGTH_UNIT_FACTOR=0.001 (the drawing length will be scaled by this amount)
12977   LENGTH_UNIT=mm (This is the specified drawing unit, other options are cm, in, ft, m, yards)
12978   AREA_UNIT=sq.m (This is the specified area unit, other options are sq.mm, sq.cm, sq.ft)
12979   VOLUME_UNIT=cu.m (This is the specified volume unit, other options are cu.ft, cu.yds)
12980   WEIGHT_UNIT=kg (This is the specified weight unit, other options are pounds, tons)
12981   WEIGHT_PER_UNIT_AREA=1.0 (This is the weight of one square unit of the specified area unit)
12982   WEIGHT_PER_UNIT_VOLUME=1000.0 (This is the weight of the material per unit volume)
12983   COST_UNIT=INR (This is the cost unit, not yet used)
12984   This section is used during the 'Count ScaleFactor' BOQ workflow
12985   This line is comma separated and you must specify in this order:
12986   <blockname>, <'xLength' X 'yLength'>, <Description>, <Cost>
12987   <blockname>,1x1,Unit Size-Demo,100.0
12988   <blockname>,300 x 800,Full-Sized,1700.0
12989   This section is used during the 'Indexed BOQ' workflow.
12990   Here, you must specify the index followed by (=) and the description
12991   <Index>=<Description>
12992   1=Description of first entry
12993   2=Description of second entry
12994   A=Description of another entry
12995   This section is used during the 'Count Attribute Values' BOQ workflow.
12996   Here, you must specify the attribute value followed by (=) and the description, cost, time(or weight)
12997   <Attribute Value>=<Description>,<Cost>,<Time-or-weight>
12998   ATTVALUE1=<description1>,<cost1>,<time1-or-weight1>
12999   ATTVALUE2=<description2>,<cost2>,<time2-or-weight2>
13000   This section is used during the 'Dynamic Blocks' BOQ workflow.
13001   Here, you must specify the 'Visibility' parameter value followed by (=) and the description, cost, time
13002   <VisibilityStateValue>=<Description>,<Cost>,<Time-or-weight>
13003   All Chairs=Full View, 60.0,7.0
13004   End Chairs Only=Two chairs,25.0,9.0
13005   This section is used to define the quantity, cost and time/weight per unit area of the tile
13006   Here, you must specify the resource name followed by (=) and the Quantity, Cost & Time/weight per unit area of the tile
13007   <MaterialName>=<Quantity>,<Cost>,<Time-or-weight>
13008   Block name selected
13009   IS specified in INI file.
13010   Error: Block name selected
13011   is NOT specified in INI file.\nPlease edit your INI file and fix the problem
13012   Error: Please enter a valid import file.
13013   Select block to flip scale:
13014   Enter INI file to edit
13015   Please select a single record before which to insert a new row item.
13016   An empty record has been created.\n\nPlease fill up the contents and click on 'Update'
13017   Please select a single record after, immediately after which to create a duplicated record.
13018   You cannot duplicate an empty record. There must be atleast 1 record before you can duplicate it.
13019   Please select a single record to delete.
13020   All records deleted.
13021   Please select a single record to update.
13022   Please select a single row item to move up
13023   Please select a single row item to move down
13024   Please select a parameter
13025   Error: Cannot toggle the value unless it is initially set to 'On'(1) or 'Off'(0)
13026   Error: Cannot set an On/Off value when the parameter name is blank
13027   Please select a record to update.
13028   There are no sections to edit. Please create a new section using the 'New' button
13029   There is no section selected to copy.
13030   SectionHeader:
13031   contents updated and saved in memory [not on disk yet].
13032   Section name
13033   is already defined in the INI file.
13034   Support path:
13035   Installed path:
13036   Please select a BricsCAD version first.
13037   Please select an AutoCAD version and installation
13038   Sorry, not yet implemented.
13039   successfully
13040   default.cui copied to
13041   Enter new location to copy default.cui to
13042   How to show toolbars in BricsCAD
13043   Show/manage Commandline, Ribbons & Pull-Down Menus in BricsCAD
13044   How to Create Lofted 3D Solids and Surfaces in BricsCAD
13045   Cannot save drawing in BricsCAD: How to fix this error
13046   Text is misplaced / overlapping in BricsCAD
13047   Select Bricsys TV video to watch
13048   Select BricsCAD Support TV video to watch
13049   Select CADPower-GeoTools TV video to watch
13050   CP_STARTUP.LSP file found at
13051   *** Also found at:
13052   CP_STARTUP.LSP file not found.
13053   GT_STARTUP.LSP file found at
13054   GT_STARTUP.LSP file not found.
13055   There is no command called
13056   in
13057   Will check in
13058   now.
13059   Path:
13060   copied to clipboard.
13061   No item selected.
13062   Error: Please select a folder from the list.
13063   Error: Please select a folder category from the list.
13064   (not set)
13065   Select folder to copy default.cui to:
13066   default.cui file found at
13067   Error: BRICSCAD+ partial menu is not loaded.
13068   UCS, Viewports and QuickTools TOOLBAR switched ON
13069   Command line prompt text set as:
13070   Enter command line text (or . for none)
13071   Bricsys Network License Manager Folder
13072   Bricsys Support TV: APERTURE, PICKBOX, SNAPMARKERSIZE & CUSRORSIZE explained
13073   Bricsys Support TV: Change background color of screen
13074   Your current GeoTools license does not include the 'Railway Design' module
13075   Your current GeoTools license does not include the 'Transmission Design' module
13076   Segment number
13077   of polyline picked.
13078   offsetted polylines created.
13079   Original polyline has
13080   vertices. Offsetted poyline has
13081   vertices.
13082   Enter slope in degrees (or enter slope in 1:n format)
13083   Enter desired change in elevation from original polyline
13084   Select 2d/3d polyline to use as center-line path:
13085   Select 2d polyline to use as cross-section (CS) for offset:
13086   Pick an anchor point on the CS polyline:
13087   Error: Please select an open polyline only as cross-section.
13088   Error: Please select a 2d polyline only as cross-section.
13089   Left Side of center.
13090   Right Side of center.
13091   The number of vertices in ofsetted section polylines are not same. Therefore, they cannot be reliably joined in cross-section.
13092   Number of points in the cross section:
13093   Number of points in the direction of the center-line:
13094   Number of points in the direction of the 3D center-line:
13095   Select center-line offset layer
13096   Select cross-section polylines layer
13097   Select DTM 3dfaces layer
13098   Pick point to place table:
13099   Area Table
13100   Do you want to scale the table?
13101   Enter scale factor
13102   Select CSV export file name
13103   Determine the intersection of two 3DFACE planes
13104   Select first plane 3DFACE:
13105   Select second plane 3DFACE:
13106   Shapes must be geometrically closed entities.
13107   Select shape objects [polylines] [ENTER to select from layer]:
13108   Do you want to join them first into closed polylines before processing?
13109   Processing shapes...
13110   Shapes List manager REPORT:
13111   SHAPE name
13112   Key Dimensions
13113   Warning: Object Table Data has not been set to store the shape parameters. They will be displayed in a table only, and not stored as data within the DWG.
13114   Please select a TARGET pattern to replace
13115   Please select a SOURCE pattern to replace.
13116   Creating output CSV file...
13117   Pick point to place SHAPE table:
13118   Shape Properties & Quantity Table
13119   Shape
13120   Quantity
13121   Area
13122   Length
13123   Description
13124   Dimensions
13125   Replacing...
13126   replacements done.]
13127   Warning: Ensure that the linear features make valid sense for TIN data, else you will get wrong results.
13128   Select point, blocks, lines, polylines to consider for TIN:
13129   Select points, blocks for Voronoi polygons
13130   A closed boundary polyline showing the extents of the selected points has been created.
13131   Warning: There are no objects crossing the boundary, nothing to trim.
13132   Creating Voronoi polygon closed boundaries....
13133   A closed polyline hugging the outer boundary of the points has been created.
13134   Warning: Please be aware that this process can significantly increase (5x or more) processing time.
13135   You can create a merged outline boundary using the 'GT_MERGEPOLY' command as well.
13136   Creating Voronoi polygon boundaries....
13137   Select closed polygon for hole table frame:
13138   Error: Please pick a closed polygon boundary.
13139   Error: Please pick a polyline, spline or circle object only.
13140   All circles, blocks, closed polylines and splines inside the frame will be selected automatically.
13141   Error: There is nothing inside the frame polyline to create a hole table out of.
13142   Pick origin point:<
13143   Pick point on X axis of hole table:<
13144   objects found inside the selected frame polyline.
13145   Warning: 1 open polyline inside the boundary was ignored.
13146   Current Hole table parameters stored in frame entity.
13147   Pick point to place hole-table:
13148   Hole Table - Circular Shapes
13149   Hole Table - Polygonal Shapes
13150   Hole Table - Blocks with attributes
13151   Hole Table - Polygonal Shapes
13152   Hole Table - Block Names/Attributes
13153   Quantity Table - Circular Shapes
13154   Quantity Table - Attribute Values
13155   Quantity Table - Block Names
13156   Quantity Table - Polygonal Shapes
13157   Quantity Table - Blocks
13158   Quantity Table - Circular Shapes
13159   Quantity Table - Polygonal Shapes
13160   Do you want to scale the hole/quantity table?
13161   Hole table info written to file:
13162   Select hole-table layer
13163   Error: Please select a block and an attribute as your selection includes blocks.
13164   Error: There are no objects selected for polygon edges.
13165   GT_CCPOLY cannot proceed without some polygon edge objects.
13166   A new boundary polyline was created.
13167   The boundary polyline created already exists.
13168   There are no objects selected for the polygon edge layers.
13169   Objects from the layers
13170   in the current view will be selected for the boundary edges.
13171   Error: There are no boundary edge objects found in the current view and matching layers
13172   A boundary centroid POINT object was created in the layer:
13173   A boundary centroid BLOCK object was created in the layer:
13174   the bounding polygon area is
13175   and centroid at
13176   Polygon area value
13177   written to area attribute
13178   written to CADPower Object table data
13179   in field
13180   objects selected.
13181   Error: The Area field name specified
13182   does not exist in the table
13183   Please choose a different field name.
13184   Error: The Area field selected is of type 'Integer'. The area value will be stored as an integer.
13185   Error: The Area field selected is of type 'String'. The area value will be stored as a string.
13186   Error: The Area field selected must be either of 'Integer', 'Real' or 'String' type only.
13187   Error: Please select an object table field name before you can exit this dialog.
13188   Error: Please select a block to insert @ centroid location.
13189   Error: There are no blocks in this drawing. Resetting back to 'Points'
13190   Select block to place @ centroid
13191   This is the composite blocks section. Composite blocks are assemblies which contain embedded parts
13192   The list of parts is defined as a collection of blocks with their quantities
13193   All block names listed in this section is considered a composite block, with a parts list as specified
13194   For example:
13195   This means that, when the block FEL is seen in the selection, it is counted once
13196   and an additional quantity of 5 'R-AL' blocks and 10 'R-CC' blocks are added to the quantity list
13197   The closed polygons must contain blocks named
13198   Select closed polygons to process:
13199   The attribute
13200   in these blocks will be checked for these values listed below (comma separated)
13201   Warning: UnitCost for attribute value
13202   Warning: Description for attribute value
13203   set to 0.0 as it was not specified in the INI file.
13204   Warning: Time/weight resource for attribute value
13205   is *NOT* defined in the INI file and this block will be ignored and not processed.
13206   All existing visibility states and their cost/time-weight resource already defined in your INI file
13207   will be retained and not changed
13208   Any new visibility state will have the default description, cost and time/weight resource values
13209   All existing attribute values/cost/time-weight already defined in your INI file
13210   Any new attribute values added will have the default description, cost and time-weight resource values
13211   Error: You can use this option only when the 'Dynamic Blocks' BOM-Q option is chosen.
13212   Error: Please select an attribute who values you want to transfer to the INI. You can choose this in the 'Index attribute' pull-down above.
13213   Error: You can use this option only when the 'Count Attribute Values' or 'Count scale factors' BOM-Q option is chosen.
13214   Copied to clipboard:
13215   Selected
13216   No blocks in current drawing.
13217   Error: There are no block names defined in the INI file. Block names must first be defined in INI file to continue further.
13218   Attribute tag
13219   already exists in INI file, not added.
13220   added to INI file.
13221   added to INI file with default parameters.
13222   blocks in polygon selected
13223   accepted.
13224   Added:
13225   to the INI file.
13226   sizes added to the INI file.
13227   Pre-processing objects....
13228   Select a custom boundary [closed polyline]:
13229   Error: Please select a mapped atribute to unlink.
13230   Error: Please select a Source and Target attribute to link.
13231   Error: This attribute link
13232   Select entities to attach CADPower object table data [or ENTER to select by layer]:
13233   fields from object table
13234   for editing
13235   The [*RECORD] section defines the structure of the data that you are creating
13236   This is the same format of INI file as used by the CP_DATAMAN command
13237   The first entry NAME=<value> is mandatory and defines the name of the data holder
13238   For example: Name=DUCT_INFO
13239   The second entry Type=XDATA is mandatory and leave it as it is, no change required
13240   The third entry is of format: FIELD=<Name>,<Type>,<Description>
13241   This is the general description of the linear item
13242   For example: FIELD=Duct Name,String,Linear Part
13243   The fourth entry is mandatory and should be exactly like this: FIELD=Weight per unit length,Real,<Value>
13244   For example: FIELD=Weight per unit length,Real,500.0
13245   The fifth entry is mandatory and should be exactly like this: FIELD=Weight per unit length,Real,<Value>
13246   For example: FIELD=Cost per unit length,Real,110.0
13247   The sixth (and subsequent) entries are optional and should be exactly like this: FIELD=<Name>,<Type>,<Description>
13248   For example: FIELD=Supplier, String, Supplier Info
13249   For example: FIELD=Width, Real, Duct Width
13250   The [*FIELD_VALUES] section defines the structure of the values that each data field can take
13251   This is the same format of INI file as used by the CP_DATAMAN command
13252   The first line is of format: <Name>=<NameValue>
13253   For example: Name=Cost  (specifies that this field record contains all the Cost information)
13254   The next lines are repeating values that are allowed for this parameter
13255   For example:
13256   Values=60.0
13257   Values=80.0
13258   Template INI file for CP_LINEQTY created at:
13259   with the following default information.
13260   Primary ID [Name] field:
13261   Primary ID [Name] field: (none)
13262   First parameter field:
13263   First parameter field: (none)
13264   Second parameter field:
13265   Second parameter field: (none)
13266   Parameter 2 (second lookup parameter) is not defined in the INI file but available in the selected entities. Please check and correct your INI file.
13267   Error: CADPower object table
13268   already exists.
13269   You are about to delete the CADPower Object table
13270   Are you sure you want to delete this table?
13271   All fields and associated data with this table definition will be deleted.
13272   Data attached to entities will NOT be deleted.
13273   CP_DATAMAN Message
13274   CADPower Object Table data
13275   deleted successfully from drawing.
13276   definition does not exist in current drawing.
13277   You can now define a new Object Data Table. Please enter the name in the provided box and click on 'Create'.
13278   You can add it using the 'Add/Update' button below
13279   Error: X, Y, Z, HANDLE, OBJECTTYPE and LAYER are reserved names. They cannot be used as field names.
13280   Do you want to update the definition of this field with current values?
13281   The type is
13282   and the default value is
13283   CP_DATAMAN Message: Field
13284   updated with type
13285   and default value of
13286   Do you want to add this field to the table?
13287   The field is of type
13288   CP_DATAMAN Message: New field
13289   created with type
13290   Error: Object table name
13291   is not defined in this drawing. Looks like this is an internal error.
13292   Error: Please select an field type.
13293   Error: Please create or select an object table name first.
13294   Error: Please enter a field name to create.
13295   Select CADPower object table data INI file to save
13296   Select CADPower object table data INI file to restore
13297   Error: CADPower Object Table Data
13298   is already defined in this drawing. Cannot import this table
13299   Error: The INI file could not be read correctly.
13300   Error: No CADPower Object Table Data has been specified. Please select one before you can proceed further.
13301   fields saved to table
13302   in file:
13303   Select objects to attach CADPower Object data.
13304   1 selected object contains existing CADPower object data and will be overwritten.
13305   1 selected object contains existing CADPower object data and will be skipped. No new data will be attached.
13306   1 object contains existing CADPower object data. Do you want to overwite the same with new default data?
13307   Attaching CADPower Object Table Data belonging to table
13308   Error: The Current Object Table Data Fields List is not set.
13309   Error: The selected CADPower Object Table is not defined in the drawing.
13310   Error: There are no CADPower Object Tables defined in this drawing.
13311   Select objects to detach CADPower Object data [or ENTER to select by layer]:
13312   There are no CADPower Object Table data attached to the selected objects.
13313   CADPower Object Table Data belonging to table
13314   removed....
13315   Select objects to query CADPower Object data.
13316   Enter name of ASCII file to create
13317   Error: No CADPower Object Table Data has been specified for query. Please select one before you can proceed further.
13318   First search criteria:
13319   object(s) meeting [first] query criteria
13320   There are no objects in the selection which meet the [first] query criteria.
13321   Second search criteria:
13322   object(s) meet [first] query criteria and
13323   object(s) meet [second] query criteria
13324   object(s) meeting both [first] and [second] query criteria
13325   There are no objects in the selection which meet the [first] and [second] query criteria.
13326   Select source object to copy data from:
13327   Error: There are no CADPower Object Table Data attached to the selected objects.
13328   Select objects to copy object table data to:
13329   1 selected object contains existing CADPower object data of table
13330   and will be overwritten.
13331   and will be skipped. No new data will be copied.
13332   1 object contains existing CADPower object data of table
13333   . Do you want to overwite the same with new data?
13334   Copying CADPower Object Table Data belonging to table
13335   Select objects to edit CADPower Object data  [or ENTER to select by layer]:
13336   [Single Object Editing]: Editing CADPower Object Table data of table
13337   Error: The selected object does not contain any CADPower Object Table Data.
13338   The selected
13339   objects contain data from the following CADPower object tables:
13340   [Single Object Editing,
13341   Editing CADPower Object Table data of table
13342   Updating entities with modified object data.... field
13343   set to value
13344   Error: There are no Object Table Data defined in this drawing.
13345   Error: Please select a CADPower Object Field name to edit, before clicking 'Ok'
13346   Error: Please select a CADPower Object Table name to edit, before clicking 'Ok'
13347   1 Data type in CADPower object data does not match the field type definition of the table
13348   CADPower object data updated successfully.
13349   This entity does not contain CADPower Object Table Data belonging to table
13350   Error: Please select a CADPower Object Table Data Name to attach, before you can exit from this dialog.
13351   Error: Please select a CADPower Object Table Data Name to detach, before you can exit from this dialog.
13352   CADPower Object Data listing (TableName:
13353   Field Name                 Value
13354   case-sensitive
13355   not case-sensitive
13356   partial search also
13357   full search only
13358   Select DTM objects: 3d polylines, lines or 3dfaces to use for elevation data.
13359   Select points or blocks to acquire elevations for:
13360   Pre-processing, building points list....
13361   Pick enclosing 3d object (3d polyline or 3dface):
13362   Error: Please pick a closed polyline or 3dface object only.
13363   Select layer for DEM points
13364   Select layer for DEM 3dfaces
13365   Error: Surface
13366   does not have TIN data in the drawing. Import it if not done already.
13367   You are exiting the dialog box but no surface was selected. You can select 3dfaces or polylines manually and interpolate elevations from them.
13368   Pick first corner of grid:
13369   Pick other corner of grid:
13370   Building DEM points list....
13371   (dummy value -999.0 set on point, elevation not found)
13372   Layer Area Statistics
13373   X, Y & Z coordinates precision set to:
13374   X precision:
13375   Y & Z precision:
13376   Y precision:
13377   Z precision:
13378   Exaggeration factor                              :
13379   Length of the profile                            :
13380   Reference Height                                 :
13381   Profile swath width                              :
13382   Total Soil Cross section area (from ref. height) :
13383   Total Soil Volume (from ref.height)                =
13384   Select polyline representing finished ground level [or ENTER to specify design level]:
13385   Reference height:
13386   Enter finished ground level
13387   Error: Finished ground level must be higher than reference height.
13388   Error: please select a line, polyline or spline as your finished ground profile.
13389   Error: Finished Ground (FG) profile does not fully cover the existing ground area.
13390   Please check your FG profile.
13391   Error: A start point for the selected finished ground profile could not be found.
13392   Please check your finished ground profile curve.
13393   Starting distance of FG at EG start point:
13394   Error: Could not obtain necessary finished ground intersection points.
13395   Please make sure your FG profile covers the entire EG space.
13396   Net volume/swath =
13397   Total Cut Volume/swath  =
13398   Total Fill Volume/swath =
13399   Select 2d representations [closed polylines] of 3d profile [existing ground]
13400   Finished ground 3d polyline was created in the layer:
13401   Error: Mis-match in number of vertices between finished ground profile and source polyline.
13402   Finished ground 3d polyline was not created.
13403   Finished Ground (FG) 3d polyline cannot be created as the profile distance measurement was set as 'Slope', not 'Horizontal'.
13404   Please re-create the profile with 'Slope' distance measurement setting and try again if you need FG 3d polyline
13405   The rest of this volume computation command has functioned normally. Please verify results.
13406   Finished Ground (FG) 3d polyline cannot be created as the profile type is set as 'Interpolate'.
13407   Only profiles with 'Source' polyline points will be possible to create Finished Ground (FG) 3d polylines.
13408   Error: Could not find the handle to the 3d polyline from which this 2d profile data was created.
13409   Error: 2d polyline must be closed. This polyline has been ignored.
13410   Grand Total Cut Volume  =
13411   Grand Total Fill Volume =
13412   Grand Net volume =
13413   Error: 1 3dface ignored. Its volume could not be determined
13414   1 3dface ignored. Its minimum elevation
13415   is higher the specified datum of
13416   3dface with more than 3 non-unique points ignored.
13417   Surface 1: Total Volume as measured using
13418   3dfaces from datum
13419   Surface 2: Total Volume as measured using
13420   Surface 2: Total Volume difference between the two surfaces is:
13421   Surface 1 (minus) 2: Total difference between the two surfaces is:
13422   objects found.
13423   Select 3dfaces/3dpolylines for first surface:
13424   Select 3dfaces/3dpolyline for second surface:
13425   Select first surface
13426   Error: There are no 3dfaces or 3dpolyline objects in the surface layer:
13427   You must first import a surface using GT_IMPORTSURFACE command.
13428   Select second surface
13429   Total # of objects in the surface:
13430   Minimum X value :
13431   Minimum Y value :
13432   Minimum Z value :
13433   Maximum X value :
13434   Maximum Y value :
13435   Maximum Z value :
13436   List of each side of triangle
13437   Radius
13438   Length X Width
13439   List of each side of quadrilateral
13440   List of each side of polygon
13441   Length of side of pentagon
13442   Length of side of hexagon
13443   Length of side of hepatgon
13444   Length of side of octagon
13445   Length of side of nonagon
13446   Length of side of decagon
13447   Radius & Length
13448   Radius & D
13449   Length of side =
13450   Length of sides =
13451   Side =
13452   Radius =
13453   Length =
13454   Width  =
13455   Error: One object was found with area equal to or less than 0.0, and was ignored.
13456   Insert a geo-tagged photo block and provide URL link to it.
13457   Please ensure this tool is available.
13458   Error: Cannot find
13459   in the search path.
13460   Please ensure this drawing is available.
13461   Next Highest ID counter set to:
13462   Error: There are no matches for the specified prefix
13463   There are no blocks named
13464   in this drawing.
13465   Select image files
13466   Image file
13467   is already selected
13468   Extracting EXIF data from
13469   Error: No GeoTagInfo found in :
13470   image blocks inserted successfully.
13471   images could not be inserted.
13472   No geotag info found in the following EXIF files:
13473   All measurements will NOW be made from THIS point.
13474   Pick a NEW START point on the curve:
13475   Pick a NEW START point on the curve
13476   The new start distance of the curve is at:
13477   The remaining length of the curve available for multi-variable measure is:
13478   from the start point of the curve.
13479   The picked point is:
13480   A BLOCK object was placed at the new specified start measure point of the polyline.
13481   A BLOCK object was placed at the start of the polyline.
13482   A POINT object was placed at the new specified start measure point of the polyline.
13483   A POINT object was placed at the start of the polyline.
13484   A POINT object was placed at the end of the polyline.
13485   Enter measured distance from the NEW START measure point: <
13486   Enter measured distance from the NEW START measure point: [X to exit]
13487   >: [X to exit]:
13488   Enter measured distance from start point: <
13489   Enter measured distance from start point: [X to exit]:
13490   Enter the next segment distance, as measured from the NEW START measure point: <
13491   >: [X to exit]
13492   Enter the next segment distance, as measured form the NEW START measure point: (Press RETURN to exit)
13493   Enter the next segment distance, as measured from the last point: <
13494   Enter the next segment distance, as measured from the last point: [X to exit]
13495   A BLOCK object was placed at a distance of
13496   from the start of the curve.
13497   from the last measured point.
13498   A POINT object was placed at a distance of
13499   Please enter a positive, non-zero value for distance.
13500   Error: Please select a block to place along the polyline.
13501   Import Google Earth images into CAD
13502   This tool will provide you with step-by-step instructions to capture a Google Earth image
13503   and bring it into CAD. This is a semi-automatic procedure.
13504   IMPORTANT: Please follow the instructions carefully.
13505   [GoogleEarth]: Some useful commands in Google Earth.
13506   N - Reset view so North is up
13507   U - Reset tilt to top-down mode
13508   [GoogleEarth]: Start Google Earth and zoom in to the area on the map which you want to capture.
13509   When you are done, Press ENTER to continue.
13510   Step 1:
13511   Step 2:
13512   [GoogleEarth]: Make sure that coordinates in Google Earth is set to Lat Long (geographic) or UTM as desired.
13513   [GoogleEarth]: The coordinates as specified will be used to insert the image in your CAD program
13514   Step 3:
13515   [GoogleEarth]: Next, we need to capture the coordinates of the LOWER LEFT corner of the image.
13516   [GoogleEarth]: Bring the cursor to the lower LOWER LEFT corner of the image as precisely as possible.
13517   [GoogleEarth]: When done, Press 'Control-Shift-C' to capture the coordinates into clipboard.
13518   The coordinate system is:
13519   UTM Zone:
13520   The Lower left corner picked is:
13521   The coordinates of the LOWER LEFT point could not be captured. Please try again.
13522   Step 4:
13523   [GoogleEarth]: Next, we need to capture the coordinates of the UPPER RIGHT corner of the image.
13524   [GoogleEarth]: Bring the cursor to the UPPER RIGHT corner of the image as precisely as possible.
13525   [GoogleEarth]: Do not change the zoom/view extents of the screen.
13526   The Upper Right corner picked is:
13527   Error: UPPER RIGHT corner must to to the right and above the LOWER LEFT corner.
13528   Error: The coordinate system has been changed since the LOWER LEFT corner was captured. Please reset it back to the same.
13529   The coordinates of the UPPER RIGHT point could not be captured. Please try again.
13530   [GoogleEarth]: The Google Earth coordinate system is:
13531   [GoogleEarth]: The LOWER LEFT corner coordinates are:
13532   [GoogleEarth]: The UPPER RIGHT corner coordinates are:
13533   [GoogleEarth]: Now, Save the image using the File -> Save -> Save Image or type Control-Alt-S key.
13534   Enter Google Earth image file to import (~ or ? to browse)
13535   Error: You have not captured the coordinates yet. Please try again.
13536   GT_GEIMPORTIMAGE tool:
13537   Step 5:
13538   Error: Cannot find GeoTools GPS point block GT_GPS_POINT.dwg in the search path.
13539   GT_GEIMPORTPOINT tool:
13540   Import Google Earth point into CAD, and store both Lat-Long and UTM coordinates in the point block.
13541   This tool will provide you with step-by-step instructions to capture a point in Google Earth
13542   [GoogleEarth]: Start Google Earth and zoom in to the point on the map which you want to capture.
13543   [GoogleEarth]: Next, we need to capture the coordinates of the POINT in Lat-Long units.
13544   [GoogleEarth]: Ensure that the coordinates are set to Lat-Long viz. Decimal Degrees -or- Degrees-Minutes-Seconds
13545   [GoogleEarth]: This is done by going to Tools->Options and select the '3D View' tab in this section
13546   [GoogleEarth]: Next, bring the cursor exactly to the point you want to capture, as precisely as possible.
13547   The Lat-Long coordinates of the picked point is:
13548   Error: The coordinates are not in LatLong units. Please check your Google Earth settings
13549   The coordinates of the point could not be captured. Please try again.
13550   [GoogleEarth]: Next, we need to capture the coordinates of the SAME POINT in UTM units.
13551   [GoogleEarth]: Ensure that the coordinates are set to Universal Transverse Mercator
13552   [GoogleEarth]: Now, ensure that the cursor is on the same point at exactly the same location as last
13553   [GoogleEarth]: capture. When done, Press 'Control-Shift-C' to capture the coordinates into clipboard.
13554   The UTM coordinates of the picked point is:
13555   Error: The coordinates are not in UTM units. Please check your Google Earth settings.
13556   Insert into which coordinates?
13557   Enter CSV file to edit
13558   Warning: Minimum one CSV record must exist. Cannot delete the only remaining record.
13559   Error: There are no CSV records to delete.
13560   updated.
13561   New Angle
13562   Error: Sheet block parameters not set. Please run the 'GT_SheetIns' command first.
13563   Select closed polyline, circle or spline:
13564   Error: Selected polyline is not closed.
13565   Error: Please select a closed polyline, circle or spline object only.
13566   Current area of polygon:
13567   Enter required area of polygon
13568   Program mode?
13569   Do not enter negative values. The direction of change is decided by target and source area values.
13570   Enter percentage change in area during each iteration
13571   You have entered a negative value for percentage change. It is ignored and only the actual positive valeu will be used.
13572   Enable clash detection?
13573   Pick anchor point
13574   Area needs to be reduced. Scale factor:
13575   Area needs to be increased. Scale factor:
13576   *** Clash detected. You may try changing the anchor point
13577   Do you want to re-specify the anchor point?
13578   'PolyAreaCreate' warning
13579   Pick new anchor point:
13580   Clash detection is not possible if polygon has arc segments.
13581   New area:
13582   Prev area:
13583   Reqd.Area:
13584   Change:
13585   Press ENTER to continue.
13586   Reverting back to the original polygon whose area is
13587   Final new area of polygon:
13588   Required area:
13589   Is the result ok?
13590   Filtering selection...
13591   Connecting arcs...
13592   Average spacing between text =
13593   List all your openings (doors, windows etc) here, one per line.
13594   Example:
13595   Door
13596   Window
13597   Ventilator
13598   This section shows all the general operating parameters used by this command
13599   Creating slope hatches from
13600   Warning: Hatch pattern object warning temporarily limit increased to
13601   Hatching un-processed objects...
13602   Processing selections that could not be hatched in the normal way...
13603   Slope Categories/Area Table
13604   Enter slope table scale factor
13605   Enter Slope info output CSV file-name
13606   Find slope: To point:
13607   The slope between the picked points is
13608   Select polyline to edit multiple vertices:
13609   Error: Please pick only a polyline object.
13610   Point already selected.
13611   Error: Your must select exactly two vertices for the 'Dynamic Custom' move method to wfunction
13612   Select custom movement method
13613   This is only a one-off 'Set Length' operation. You will be asked to select the interactive operation again after the length is set
13614   Enter or pick new length for this segment
13615   New length of segment set as
13616   Initial area:
13617   Perimeter:
13618   Distance:
13619   <not determined>
13620   Pick dimension location:
13621   Select CIRCLE objects.
13622   Enter part name
13623   Part names assigned to the cut pieces are:
13624   [left] and
13625   [right]
13626   Enter or pick text height for label
13627   Enter part name for first part
13628   Enter part name for second part
13629   Enter layer name(s) to process
13630   Enter or pick side offsets
13631   Enter or pick front-back offsets
13632   Do you want to trim along the edges?
13633   Do you want to WBLOCK the sheet-cut drawing?
13634   Processing sheet LS data...
13635   Pick an empty space to copy the selected objects to:
13636   Sheet trimming was not done as requested.
13637   Wblocked drawing:
13638   Error: 1 polyline ignored, no entities were found inside its corridor bounding box.
13639   Error: 1 polyline ignored, it could not be successfully offset.
13640   Error: 1 polyline ignored. Cannot create sheet boundary with closed polylines.
13641   Error: One of the section defining polylines could not be found. Please report this error to rakesh.rao@thedesignsense.com
13642   sections were successful processed and WBLOCK drawing created.
13643   sections were ignored and could not be processed.
13644   Sections not processed have been placed in the active [previous] selection set.
13645   Select sheet boundary to trim to:
13646   Specify which side to trim?
13647   Do you want to erase everything outside the boundary?
13648   Do you want to erase everything inside the boundary?
13649   Error: The polyline must be closed.
13650   P E R F O R M A N C E   A D V I S O R Y
13651   If you are processing multiple sections together, it is strongly advised to turn OFF UNDO logging
13652   before running this program. This will disable undo history logging but improve performance and
13653   reduce paging etc.

13654   Import CADPower Object Table Data from ASCII (CSV) files.
13655   Enter name of CADPower Object data CSV file to import
13656   Error: Please select a valid CSV file for import of CADPower Object data.
13657   Updating CADPower Object Table Data belonging to table
13658   1 CSV record with handle
13659   was skipped as the corresponding entity cannot be found in the drawing.
13660   1 CSV record was skipped as the handle information is not available.
13661   Error: Cannot determine the <Handle> information position in the CSV file.
13662   Error: Specified CADPower object table data
13663   is not defined in the current drawing.
13664   Error: There is no header data in the CSV file with the <Handle> information in it. This file cannot be imported.
13665   Export CADPower Object Table Data to ASCII (CSV) files.
13666   Select objects which have CADPower Object data of table
13667   Error: Number of object data fields in entity [
13668   ] does not match table definition [
13669   fields]. 1 entity ignored.
13670   Error: 1 object did not have object data belonging to table
13671   and has been ignored.
13672   Building export list....
13673   records written to export file....
13674   No export file as created as no objects matching object data was found.
13675   Warning: Please be aware that 'Handle' is a required export if you want to import the data back using CP_CPOD_IMPORT/GT_CPOD_IMPORT command and synchronize data.
13676   Please choose your options accordingly.
13677   Error: Please select atleast one field to export.
13678   Error: Please select a CADPower Object Table Data to export.
13679   objects had a redundant closing vertex added.
13680   objects had a redundant closing vertex removed.
13681   No polyline vertices were modified. Nothing processed.
13682   Current Match flags (Special):
13683   Average width of segments in target polyline:
13684   Circle/Arc center:
13685   Text/MText height:
13686   Hatch pattern:
13687   Hatch pattern scale:
13688   Break all lines,arcs,polylines and splines along a polyline.
13689   Select cutting edge polyline:
13690   Processing polyline edge...
13691   Spline skipped
13692   Processing intersecting objects...
13693   Breaking intersecting objects...
13694   Error: Please pick a polyline object only.
13695   DistAngWeed Message
13696   The drawing unit selected is:
13697   and conversion unit is
13698   Level difference will be converted from
13699   Pick datum point:
13700   Enter datum elevation
13701   Datum:
13702   Pick level point [ENTER to finish]:
13703   Select annotation layer
13704   Enter part name for highlighted part
13705   Apply running part numbers based on CP_TC settings?
13706   Running part numbers will be applied to selected entities. Settings will be taken from CP_TC command.
13707   Sort direction?
13708   selected]: Enter new part name
13709   Part name:
13710   assigned to object.
13711   Select parts to label:
13712   Enter text alignment
13713   displayed from selected object:
13714   Select parts to count:
13715   processed for counting:
13716   Part Number Table
13717   Enter or select CSV export file name
13718   Output file:
13719   Select objects to remove part names from:
13720   ----Contact DesignSense----
13721   CADPower is a product of DesignSense Software Technologies Pvt. Ltd. Bengaluru-INDIA
13722   CADPower LastOpened date does not exist, trial expires
13723   runs
13724   CADPower was last run on:
13725   trial expires
13726   or after
13727   Computer date appears to be reset after CADPower was installed.
13728   CADPower license has already expired on
13729   that is
13730   days back
13731   CADPower license will expire in
13732   days, on
13733   Error: Cannot create #MnuDir_CP [using-dos-mkdir] , determined as
13734   CADPower AppData folder:
13735   created [using-dos-mkdir]
13736   Error: Cannot create #MnuDir_CP [using-vl-mkdir], determined as
13737   created [using-vl-mkdir]
13738   Messages file...
13739   was read successfully.
13740   could NOT be read successfully [unencrypted].
13741   Error: CADPower startup Lisp
13742   could not be loaded.
13743   Copying support files...
13744   Warning: AutoCAD serial number could not be obtained. Please run a command again and try.
13745   CADPower Licenses available:
13746   used:
13747   CADPower messsage
13748   The computername is:
13749   and user name is:
13750   The menu name
13751   [not available]
13752   <not applicable>
13753   There is no SaveComplete reactor to close
13754   ROLLOVERTIPS display has been turned OFF. If you turn it on, it *may* interfere with the right-click menu experience.
13755   QUAD display has been turned OFF. If you turn it on, it *may* interfere with the right-click menu experience.
13756   Error: BMP file:
13757   could not be deleted.
13758   Error: Windows TEMP folder not set, could not be determined.
13759   GeoTools 'LastOpened' date does not exist, trial expires
13760   GeoTools was last run on:
13761   Computer date appears to be reset after GeoTools was installed.
13762   GeoTools license will expire in
13763   Error: Cannot create #MnuDir_GT [using-dos-mkdir] , determined as
13764   GeoTools AppData folder:
13765   Error: Cannot create #MnuDir_GT [using-vl-mkdir], determined as
13766   could NOT be read successfully.
13767   Error: GeoTools startup Lisp
13768   GeoTools Licenses available:
13769   Select block objects to explode, retain attributes.
13770   Select point/block/text objects around which to create closed polylines [or ENTER to select by layer]:
13771   Your current CADPower license does not include the 'Line-And-Space' module.
13772   Transfer Block Attributes to CADPower Object table data.
13773   There are no CADPower Object Data Tables in this drawing.
13774   Type the CP_AOD/GT_AOD command to manually transfer block attribute data.
13775   Transferring Block Attributes to CADPower Object Table Data
13776   CADPower Object table records transferred.
13777   Select layer(s) to process polylines from
13778   Shape
13779   Attaching object data to processed shapes...
13780   Google Earth Rubber Sheeting tool (with Google Earth control points):
13781   Perform rubber sheeting of CAD vector data to fit in Google Earth (Lat-Long coordinates)
13782   This tool will provide you with step-by-step instructions to do rubber sheeting of CAD vector data
13783   to enable it to be super-imposed in Google Earth. This  is a semi-automatic procedure.
13784   Please note that this command ensures that your data is converted to a Lat-Long KML file to enable import in Google Earth.
13785   If you are looking at doing the opposite (convert to UTM), please use the 'Rubber sheeting with drawing control points' command.
13786   IMPORTANT: Please follow the instructions carefully.
13787   GT_GERSHEET Message
13788   Step 1:
13789   [GoogleEarth]: Some useful commands in Google Earth.
13790   N - Reset view so North is up
13791   U - Reset tilt to top-down mode
13792   [GoogleEarth]: Start Google Earth and zoom in to the area of interest in the map.
13793   [GoogleEarth]: Ensure that the coordinates in Google Earth is set to Lat-Long (Decimal Degrees).
13794   [GoogleEarth]: This can be checked from Tools Menu -> Options -> Show Lat/Long section.
13795   When you are done, Press ENTER to continue.
13796   Step 2:
13797   [CAD Drawing]: Zoom into the same area of interest in the CAD drawing also.
13798   Pick FIRST point in the CAD drawing:
13799   [CAD Drawing]: The FIRST point coordinates are:
13800   [GoogleEarth]: Next, we need to capture the coordinates of the same FIRST point on the Google Earth image.
13801   [GoogleEarth]: Bring the cursor to the same FIRST point in Google Earth as precisely as possible.
13802   The FIRST point picked is:
13803   Error: The coordinate system in Google Earth must be set to LatLong only.
13804   Pick SECOND point in the CAD drawing:
13805   [CAD Drawing]: The SECOND point coordinates are:
13806   [GoogleEarth]: Next, we need to capture the coordinates of the same SECOND point on the Google Earth image.
13807   [GoogleEarth]: Bring the cursor to the same SECOND point in Google Earth as precisely as possible.
13808   The SECOND point picked is:
13809   [GoogleEarth]: The FIRST point coordinates are:
13810   [GoogleEarth]: The SECOND point coordinates are:
13811   Select objects to rubber-sheet
13812   [CAD Drawing]: Please be aware that, after rubber-sheeting, the coordinates of the drawing will be changed to Lat-Long
13813   [CAD Drawing]: to make it compatible with Google Earth use, and for export using the GT_DWG2KML command.
13814   [CAD Drawing]: Please save this drawing under a differnt name so that you do not lose your original data
13815   Google Earth Rubber Sheeting tool (with drawing control points):
13816   Select *FIRST* GPS control point block:
13817   Lat-Long coords:
13818   UTM coords:
13819   Error: The GPS point block GT_GPS_POINT selected does not have proper LL/UTM coordinates
13820   Error: Please pick a GPS point block named GT_GPS_POINT
13821   Select *SECOND* GPS control point block:
13822   Select objects to rubber-sheet [only points, lines and polylines are allowed]
13823   Building master list of elevations of polylines....
13824   Applying original elevations back into the polylines...
13825   object was ignored as its elevation match was not found in the stored list.
13826   Error: Executable file '7Z.exe' could not be located.
13827   Warning: No attribute selected for KML Image. No image will be attached.
13828   Error: Please select an attribute for KML Label.
13829   Error: Please select a block name for attribute export.
13830   Warning: No object data field selected for KML Image. No image will be attached.
13831   Error: Please select a field for KML label.
13832   Error: Please select an object table for export.
13833   Warning: No valid position selected for KML Image. No image will be attached.
13834   Error: Please enter a valid position number for XDATA field 'Label'.
13835   Error: Please select an XDATA application name.
13836   A floating license has NOT been requested as the last returned license was less than
13837   minutes back.
13838   The floating license of this computer
13839   has been returned to the server. It can be retrieved on this computer after
13840   minutes.
13841   Error: There are no active floating licenses to return.
13842   CADPower is running in un-registered mode now.
13843   The license has been marked as 'returned' already.
13844   Error: There are no active floating licenses to return. CADPower is running in un-registered mode now.
13845   Error: You are not running a floating (network) license. This command is not applicable here.
13846   The floating license will be re-acquired automatically upon startup
13847   minutes after last return
13848   GeoTools is running in un-registered mode now.
13849   Error: There are no active floating licenses to return. GeoTools is running in un-registered mode now.
13850   XLSX data exists in memory and will be used. If XLSX file has changed. Please re-select the SheetName to read.
13851   Error: XLSX file is not defined.
13852   Error: XLSX sheet name is not defined.
13853   Pick point to place TABLE of current selection information:
13854   Excel Matching Records
13855   Error: Attributed block cannot be created unless a title row is defined in the XLSX file. Please specify a title row.
13856   Pick point to place the current selection information:
13857   Pick point to place the row information:
13858   Please select from Excel or a text file the data that you want to bring in to the CAD, and click on 'Ok' when done.
13859   Error: Nothing found in clipboard. It is empty.
13860   The specified search value
13861   will be searched in column
13862   occurences of
13863   in rows.
13864   Showing Searched row #
13865   from XLSX file
13866   Error: The XLSX Sheet name has not been specified. Please select a sheet name from the list of available sheet names in the XLSX file.
13867   Error: It appears that the XLSX file has not been specified. Please do so now.
13868   Error: It appears that the XLSX file has not been read or it does not contain the required info. Please check the settings.
13869   Error: There is nothing to search. Please enter a search value criteria in the 'Property value to search' box.
13870   No matching rows found with the specified data
13871   Error: No title information is available at this row number.
13872   Error: Maximum permitted row number is 500.
13873   Showing Title Row
13874   The property value could not be determined.
13875   Select XLSX file to read
13876   XLSX file changed. The previous data in memory cleared.
13877   XLSX file was not changed. The previous data in memory is retained.
13878   Showing Row
13879   Extracted Excel information copied to clipboard.
13880   Command added on:
13881   is a 'Geological and mining' command
13882   is a 'Transmission Lines Design' command
13883   is a 'Railway Design' command
13884   Checking for duplicate objects...
13885   already loaded.
13886   installation folder
13887   already exists in the search path.
13888   added to support files search path
13889   moved to the top of the support files search path
13890   moved to the bottom of the support files search path
13891   Error: Unable to connect to the specified drawing
13892   TABLE contents placed in active [previous] selection.
13893   Warning: Number of columns in TABLE set to
13894   as per incoming data structure.
13895   Error: Cannot delete a profile that is current.
13896   Profile name:
13897   is not defined in the current CAD setup.
13898   Error: Target file
13899   Error: Object selected is neither a line or polyline.
13900   "Error: Cannot find 'EXIFTOOL.EXE' in the search path.
13901   [done]
13902   Format error in geographic coord string:
13903   Error: There is no directory called
13904   Please ensure that the output path is valid and has file-create permissions.
13905   File copied successfully from :
13906   Error: Cannot open file
13907   for output. Maybe it is already opened by another program?
13908   -Or- you don't have permission to create file in this folder.
13909   Existing file:
13910   Average X coordinate :
13911   Average Y coordinate :
13912   Average Z coordinate :
13913   Pick point to place polyline info:
13914   -or user manual methods to select and specify TIN objects for the surface
13915   Polyline vertex tweaking tool
13916   Select point on polyline to tweak (use OSNAP if necessary, ENTER to finish):
13917   Picked point is ON the vertex of the polyline.
13918   Picked point is ON the segment of the polyline.
13919   Pick new location for tweaked point:
13920   Please pick a polyline object only.
13921   Enter or show gap distance
13922   Error: Cannot find block '
13923   in the current drawing or in the search path. Could not insert block.
13924   Error: Target block for attributes is not defined.
13925   1 polyline created.
13926   Error: The import type has been specified as 'Blocks' but no block name has been selected.
13927   The pattern must contain XY or EN coordinates compulsorily, and can have ignorable field(s) specified by 'I'. Point number should be specified as 'P' and Description as 'D'\n\nExamples: PIIENZDI, IIXYII, INEII and similar\\n\\nHere, I is the field be ignored and E,N or X,Y represent the coordinates, either cartesian or geographic (Long[E]-Lat[N])\n\nExample: PIIENZDI format means that first field is point number, second and third to be ignored, fourth, fifth and sixth are coordinates, seventh is description and eighth to be ignored\\n\\nIf the option 'Specify position-based descriptions' is enabled, the description field must be specified as [D1], [D2] and so on, to specify the location of the description field to consider.\\nFor example, \\n\\nThis option is to be used when the other standard options don't qualify
13928   Error: Please select a valid file name for view/edit
13929   Error: Cannot enable this option.\n\nThe Point import format does not contain description as a field item.
13930   Pick internal point for HATCH:
13931   Hatch pattern name:
13932   Angle:
13933   File 'iso.pat' copied to
13934   successfully.
13935   Error: Cannot find 'iso.pat' file in the CADPower installation folder
13936   Error: Cannot find 'default.pat' file in the CADPower installation folder
13937   Select CTB/STB file to copy to BricsCAD support folder
13938   Destination file
13939   already exists. Ok to owerwrite?
13940   SUCCESS: Source file:
13941   copied to
13942   ERROR: Source file:
13943   could not be copied
13944   Select objects to search [for proxy object reference removal]:
13945   blocks with proxy connections found. They will be exploded and reconstructed.
13946   1 anonymous/dynamic block ignored.
13947   Processing blocks...
13948   Enter handle to search
13949   Select objects to search:
13950   Object with handle
13951   placed in active selection set.
13952   not found in selection set.
13953   is a CADPower command.
13954   is a GeoTools command.
13955   is neither a GeoTools or CADPower command.
13956   GeoTools commands list
13957   found
13958   CADPower commands list
13959   Commands which are common to both GeoTools & CADPower
13960   Command Name:
13961   Found At:
13962   Commands which are in CADPower only, not in GeoTools
13963   Enter file name to save the commands list
13964   Report file:
13965   No objects found in implied selection
13966   Select dimensions to change precision.
13967   Select dimensions to 'Move Text, No Leader'.
13968   Select dimensions to 'Move Text, Add Leader'.
13969   Select dimensions to 'Keep dimension line with text'.
13970   Select dimensions to 'Keep dimension text outside line'.
13971   Select dimensions to 'Keep dimension text inside line'.
13972   Select dimensions to 'Change arrow type'.
13973   Select dimension arrow type:
13974   Select dimensions to 'Change text obliquing angle'.
13975   Select Text Obliquing angle:
13976   Select dimensions to 'Change text width factor'.
13977   Select text width factor:
13978   Select dimensions to 'Update-Retain individual settings'.
13979   File name:
13980   WBlock with select entities and insertion point
13981   Layer:
13982   Audits and fixes MTEXT objects which have wrong DXF codes or exceeding string lengths.
13983   1 MTEXT object with string length exceeding 250 was fixed.
13984   1 MTEXT object with invalid DXF code 72 was fixed.
13985   Select a HATCH object to add vertex:
13986   Error: You must pick a HATCH object only.
13987   Please select a HATCH object.
13988   Enter or show text height
13989   Enter text creation mode
13990   Dimension values will be created as text objects with default linear units
13991   and precision
13992   Processing dimension objects...
13993   Pick a point to place text:
13994   Pick new base point for hatch:
13995   Hatch origin was moved by the following amounts:
13996   Select objects to convert to an anonymous block:
13997   Explode blocks in the selection?
13998   1 anonymous block ignored (you cannot put one anonymous block inside another).
13999   Pick insertion point of block:
14000   1 anonymous block
14001   created.
14002   Select nested block to copy internal block:
14003   Select a block:
14004   The following commands are defined as FREEWARE commands in CADPower and will NEVER expire.
14005   Select XREF objects to bind.
14006   Select LINE to convert to arced polyline.
14007   The CADPower trial has expired. Please contact
14008   for a license.
14009   Your CADPower license is compromised and not valid.
14010   The license file you are using is identified as an illegal license on this computer
14011   Continuing to use CADPower with an illegal license can result in serious computer data damage
14012   -and/or- CADPower can produce incorrect results compromising your designs
14013   ****Designsense Software is not responsible for the consequences.***
14014   If you have purchased CADPower and think this error message is by mistake, please email rakesh.rao@thedesignsense.com
14015   and request for a legal license of CADPower. IMPORTANT: Please switch off your computer *NOW* and un-install CADPower if you want to be safe.
14016   Else, Do you wish to accept the risk and continue?
14017   WARNING: ****Designsense Software is not responsible for the consequences. You are solely responsible.***
14018   Select dimensions to update, based on style settings.
14019   An exception will be made for the linear scale factor, which will be retained as in original dimension.
14020   Updating dimensions, retaining original DIMLFAC settings...
14021   WBlock * with ODA stamp removal
14022   There is nothing in this drawing to save.
14023   Error: Existing recovery file
14024   "*** CADPower Drawing Recovery Process ***
14025   Recovered drawing file will be restored as
14026   CADPower Drawing Recovery Manager
14027   Last saved version of this drawing recovered and saved as
14028   *** CADPower Drawing Recovery Process ***
14029   The auto-saved file has already been recovered once
14030   Do you want to open it now?
14031   The auto-saved file has already been recovered once and is opened now.
14032   Error: Cannot locate the file:
14033   There is no auto-save file available for this drawing. There is nothing to recover.
14034   The CP_RECOVER command is this version of BricsCAD.
14035   The following auto-save backup files for the current drawing were found in the
14036   folder.
14037   Auto-save backup file:
14038   successfully copied to
14039   successfully moved to
14040   successfully copied as
14041   .bak file folder set to
14042   There is no .bak file available for the current drawing.
14043   Select folder to move all .bak files to
14044   There is no BAK or autosave (sv$) file for the current drawing.
14045   Move the backup .BAK files to a specified folder.
14046   The option to 'Create a polyline hugging the surface boundary' has been disabled due to a bug. It will be enabled once the bug is fixed.
14047   Select objects for DTM surface [ENTER to select by layer]:
14048   Select layer(s) for DTM surface
14049   Error: Cannot create a surface unless a boundary is defined and available.
14050   Display the Select Template dialog box or use a default template (from BASEFILE sysvar)
14051   Display the Startup and the Create New dialog boxes
14052   Display the Start page
14053   Display the Start page (with ribbons preloaded)
14054   Do not display
14055   Display @ Last Location
14056   Display @ Top Left
14057   Display @ Top Right
14058   Display @ Bottom Left
14059   Display @ Bottom Right
14060   Scientific
14061   Decimal
14062   Engineering
14063   Architectural (always displayed stacked)
14064   Fractional (always displayed stacked)
14065   As Set in Control Panel
14066   Sets the size (in pixels) of the entity selection target [1-50].
14067   Sets the size (in pixels) of the entity snap aperture box [1-50].
14068   Sets the size (in pixels) of the snap marker [1-50].
14069   Sets the cross-hair size as a percentage of the screen size [1-100].
14070   Sets the size (in pixels) of the grips marker [1-255].
14071   Linear units set to decimal.
14072   Linear units set to architectural.
14073   Grips within blocks turned ON
14074   Grips within blocks turned OFF
14075   Error: The GRIPBLOCK system variable does not exist.
14076   Current dimensions primary units set to:
14077   The units specified here defines the primary dimension unit of the current dimension style.
14078   Information: Isometric SNAP drawing planes can be changed (toggled) using F5 key.
14079   Default save drawing format now set to
14080   Clipboard exchange format now set to
14081   Implied windowing is enabled. A selection window opens up when clicked in a blank area (when no command active).
14082   No implied window is created when mouse is clicked in a blank area (when no command active).
14083   Defines a drawing unit value for automatic scaling when insetting or attaching blocks, images or XREFs
14084   When both INSUNITS and PROPUNITS are on, length, area, volume and/or inertia units are formatted with their unit.
14085   Sets the drawing units as Imperial or Metric for the current drawing.
14086   This controls whether ANSI or ISO hatch patterns and linetype files are used.\nThis also sets the current drawing units as decimal [metric] or architectural [imperial]
14087   Select folder for .BAK files
14088   The .BAK file after every SAVE will be moved here.
14089   Selected .BAK folder:
14090   No .BAK folder was selected.
14091   Because of technical reasons, this functionality is available only in BricsCAD V18+ [or] in a Pro/Platinum flavor of BricsCAD.\n\nPlease upgrade accordingly.
14092   When views are changed, the UCS is automatically set to the orthographic projection view.
14093   When views are changed, the UCS is NOT automatically set to the orthographic projection view.
14094   Default drawing template saved as
14095   Select image cache folder" imgFolder "When large images need to ba cache, this folder will be used
14096   Selected image cache folder:
14097   No image cache folder was selected.
14098   Please upgrade accordingly.
14099   Because of technical reasons, this functionality is available only in BricsCAD V18+ [or] in a Pro/Platinum flavor of BricsCAD.
14100   Dynamic UCS switched ON
14101   Dynamic UCS switched OFF
14102   Dynamic input mode switched ON
14103   Dynamic input mode switched OFF
14104   QUAD display turned ON
14105   QUAD display turned OFF
14106   Roll Over Tips switched ON
14107   Roll Over Tips switched OFF
14108   Hot Key Assistant switched ON
14109   Hot Key Assistant switched OFF
14110   The GeoTools trial has expired. Please contact
14111   Your GeoTools license is compromised and not valid.
14112   Continuing to use GeoTools with an illegal license can result in serious computer data damage
14113   -and/or- GeoTools can produce incorrect results compromising your designs
14114   If you have purchased GeoTools and think this error message is by mistake, please email rakesh.rao@thedesignsense.com
14115   and request for a legal license of GeoTools. IMPORTANT: Please click on 'No' if you want to be safe.
14116   Do you wish to accept the risk and continue?
14117   GeoTools ALERT: Automatic menu loading has been disabled in the OS X and Linux platforms. Please load it manually using the MENULOAD command.
14118   Select text objects to update
14119   Scan direction
14120   Enter or show search distance around text
14121   Select a block with attributes:
14122   Error: Selected block does not have attributes.
14123   Error: Selected object is not a block object.
14124   Error: There is nothing inside the frame polyline in the specified layers
14125   to create a hole table out of.
14126   WARNING: There are
14127   sets of concentric circles. The holetable lists the entires for all the cencentric circles. Please check and verify your results.
14128   Enter or show label text height
14129   Enter or show initial offset distance for dimensions
14130   Enter or show next offset distance for dimensions
14131   *** HATCH: Color-based report
14132   Area under hatch of color
14133   *** HATCH: Layer-based report
14134   Area under hatch in layer
14135   Pick point to place HATCH table:
14136   Hatch Pattern Count Table
14137   Hatch Color Count Table
14138   Hatch Layer Count Table
14139   Specify file name for CSV export of hatch areas
14140   Hatch pattern data CSV file:
14141   Select file to restore layer descriptions
14142   new layer description were assigned to all previously un-assigned layers
14143   No new layer descriptions were assigned. All existing layers already assigned with descriptions
14144   Specify file to save layer descriptions
14145   Please note that the CP_BUILDWALLS command expects the plan footprint drawing unit to be in MM.
14146   If it is not in MM, please go to 'More Settings' and specify the drawing unit accordingly.
14147   It is MM-Continue
14148   Not MM-Specify units
14149   CP_BUILDWALLS Message
14150   [in elevation] placed.
14151   Pick point for fixtures quantity table:
14152   Warning: There are no doors/windows/fixtures to create quantity table.
14153   Pick point for wall areas quantity table:
14154   Wall Number
14155   Total Surface Area
14156   Fixtures Area
14157   Net Wall Area
14158   Wall Areas Table
14159   Select option:
14160   pick text location
14161   Hatch pattern style
14162   [GoogleEarth]: It is recommended that you switch off all the labels and other annotations on your map that you don't need
14163   [GoogleEarth]: You may also put your map in Full-Screen mode using the F11 (or View -> Full Screen) key in GoogleEarth
14164   [GoogleEarth]: This will give you maximum screen space for your image, and improve accuracy of capture.
14165   [GoogleEarth]: You may also Add a Placemark in GoogleEarth and use that as a reference to capture the Lat-Long and UTM coordinates as instructed here.
14166   [GoogleEarth]: This is only a suggestion and not mandatory. You can even capture the coordinates from a known location precisely.
14167   [GoogleEarth]: Please ensure that your GoogleEarth screen view is always vertical facing and your North direction is always pointing upwards.
14168   [GoogleEarth]: Failure to comply with this rule will produce inaccurate results, and GeoTools is not responsible for the same.
14169   added to INI ile.
14170   Pick first corner of tile [ENTER to finish]:
14171   Enter or show rotation angle:
14172   Error: It is not possible to place a tile at this location.
14173   Width [horizontal]  of tile:
14174   Error: Cannot find tile-block
14175   in current drawing
14176   Tile description
14177   was taken from the INI file.
14178   was taken from the dialog box, as set by the user.
14179   Enter or show vertical dimension of the tile
14180   The round-off distance
14181   is more than the vertical (Y) dimension
14182   of the tile.
14183   It will be reset to 10 % of tile-Y size, which is
14184   Enter or show horizontal dimension of tile
14185   is more than the horizontal (X) dimension
14186   It will be reset to 10 % of tile-X size, which is
14187   Error: Please specify a SIZE attribute before you can proceed further.
14188   Error: Please specify a DESCRIPTION attribute before you can proceed further.
14189   Error: There are no attributes defined for the selected block
14190   Error: Please select a block name for the tile.
14191   Error: The block name for the tile has not been defined yet. Please choose one from the list or specify in the dialog box.
14192   Select tile placement layer
14193   Add ERP info in the exported CSV/XLSX file?
14194   Select TEXT,MTEXT objects forming the table.
14195   Enter CSV file name to export
14196   Enter assembly/part name for this export
14197   Getting geometric extents of the selection...
14198   The average text height of the objects is:
14199   Any MTEXT objects found in the selection was converted to TEXT.
14200   You may perform an UNDO operation to revert to MTEXT
14201   ERP Project Name
14202   ERP Project Number
14203   ERP Revision Number
14204   rows of table data exported to
14205   Select closed polyline to nest along longest side [S to select a specific segment]:
14206   Select closed polyline to nest along selected side:
14207   Please select a closed polyline object only.
14208   Select entities to scale to a unit size in the X extents (direction)
14209   Select a LINE to convert to XLINE:
14210   Search and zoom to an object whose handle is specified
14211   Do you want to individually zoom to each object found?
14212   Enter handle(s) to search (separate by commas, type . to finish):
14213   Now displaying object with handle:
14214   is an invalid handle.
14215   Do you want to zoom to extents of all objects found?
14216   Enter reference length for X scale (or pick points):
14217   Enter new length for X scale (or pick points):
14218   New X Scale:
14219   New Y Scale:
14220   Enter reference length for Y scale (or pick points):
14221   Enter new length for Y scale (or pick points):
14222   Select text objects to change justification.
14223   Select text objects to change precision.
14224   Select justification to apply.
14225   Select justification to apply:
14226   Reference scaling (X):
14227   Specify new X Scale by showing old and new lengths:
14228   Reference scaling (Y):
14229   Specify new Y Scale by showing old and new lengths:
14230   Start date and end date are not the same. Elapsed time cannot be reported.
14231   Error: Cannot join them as one of them is a 3d entity and the other one is not.
14232   Select object on source layer:
14233   Select layer to copy to:
14234   Please run the CP_BO command before running the CP_BI command
14235   Select block to update in:
14236   BlockName:
14237   Enter complete file path
14238   Enter layer name to start from
14239   Showing layer
14240   . Press ENTER to continue, ESC to cancel [you can re-start from current layer later].
14241   The specified layer
14242   does not exist in this drawing.
14243   Enter attributed block name to create
14244   Select objects for blocks:
14245   Enter (or show) attribute height
14246   Enter attribute tag to add (separate multiple attributes by a comma) [press ENTER to finish]
14247   Attributed block definition:
14248   Please select a block name with attributes which is to be used as the tile block
14249   Error: Please specify an ERP data common export folder location
14250   Select common folder for all CSV/XLSX exports
14251   All CSV and XLSX ouput will be created in this folder.
14252   This function uses Civil functions on BricsCAD V
14253   You are using BricsCAD V
14254   This function requires BricsCAD Pro V22.2.02 or higher
14255   You are using BricsCAD Lite. This function requires BricsCAD Pro V22.2.02 or higher
14256   Select points/blocks or BricsCAD TIN object(s) to drape around.
14257   Adding points to TIN...
14258   Created a closed boundary polyline with
14259   points.
14260   GeoTools uses Civil functions on BricsCAD V
14261   If you upgrade to V 22.2.02 or higher, you can drape over a BricsCAD Civil TIN surface also. In this version, draping is allowed only across polylines and 3dfaces.
14262   No target selection objects have been specified. Please select some target objects for processing.
14263   Select [target] objects [lines,polylines,arcs,3dfaces] to get elevations from
14264   Select (underlying) BricsCAD TIN surface:
14265   Error: Selected entity is not a Bricsys TIN surface object.
14266   Warning: There are splines [highlighted] in the crossing/corridor area of target objects. They will be ignored.
14267   If you need them to be considered for processing, please convert them first to polylines using the GT_SPL2PL command.
14268   Processing segments....
14269   Checking new polyline for duplicate points...
14270   Updating 3d polyline with the new interpolated points...
14271   Getting segment intersections and acquiring elevations.....
14272   Enter or show length along main line to create the cross-drape polyline
14273   Enter or show length of cross-drape polyline [placed perpendicular to main line]
14274   A crash-dump analysis file called
14275   will be created in the drawing folder
14276   Error: Please select some source objects before you can exit this dialog.
14277   Drawing statistics - Object count
14278   Circle diameter summary
14279   Linear objects summary
14280   Area objects summary
14281   Object Type
14282   Count
14283   Diameter
14284   # of circles
14285   Number of objects
14286   Width
14287   Summary of polyline length based on segment width
14288   Select objects for DWF export.
14289   Enter DWF file name
14290   Please be aware that existing elevations in selected polyline will be ignored, and new elevations acquired from intersecting polylines.
14291   Select a polyline to step-trace through or ENTER to pick two points to step-trace:
14292   Error: Please select a non-arced polyline only. Polylines containing arcs are not supported.
14293   Pick first point to step-trace:
14294   Pick second point to step-trace:
14295   QUAD display has been turned OFF. If you turn it on, it may interfere with the right-click menu experience.
14296   ROLLOVERTIPS display has been turned OFF. If you turn it on, it may interfere with the right-click menu experience.
14297   Make sure all the required layers are ON and VISIBLE.
14298   Select polylines [must be closed 4-vertex polylines] for PDF print [or sheet blocks]:
14299   Error: PDF file
14300   Select text and/or mtext objects.
14301   Pick point to place the TEXT count table:
14302   Select block insert objects.
14303   Pick point to place the BLOCK count table:
14304   Enter or show map sheet size in X direction
14305   Enter or show map sheet size in Y direction
14306   Security update: Your CADPower license needs to be replaced. We apologize for the inconvenience.
14307   Contact rakesh.rao@thedesignsense.com / +91-9243438300 / +91-8073279755 to know more and for assistance.
14308   You will receive the updated license file within ONE working day.
14309   Checking CADPower license....
14310   Security update: Your GeoTools license needs to be replaced. We apologize for the inconvenience.
14311   GeoTools appkey information copied to clipboard. You can paste it in your email body and send it to 'rakesh.rao@thedesignsense.com'
14312   CADPower appkey information copied to clipboard. You can paste it in your email body and send it to 'rakesh.rao@thedesignsense.com'
14313   The 'What to annotate' option has been set as 'Source'.
14314   If you feel your cross-section data has too many points, you may change it to 'Interpolate'.
14315   Error: Profile section block drawing
14316   GeoTools Interpolated Profile Report
14317   This command requires BricsCAD V 22.2.02 Pro or higher.
14318   Please upgrade to a higher version of BricsCAD.
14319   Lite version. This command requires BricsCAD V 22.2.02 Pro or higher.
14320   Please upgrade to a higher (Pro+) version of BricsCAD.
14321   This function is available in BricsCAD V 22.2.02 Pro and above only.
14322   Please upgrade to BricsCAD Pro V22 or higher to use the Civil features.
14323   Select first BricsCAD TIN surface:
14324   Select second BricsCAD TIN surface:
14325   Error: You cannot pick the same TIN surface twice. Please pick two different TIN objects.
14326   Error: Selected object is not a BricsCAD TIN object.
14327   Select closed polylines, circles or splines as boundaries to generate a volume surface.
14328   Computing cut/fill volumes per surface...
14329   Error: Selected object is not a closed polyline.
14330   Please upgrade to BricsCAD Pro V22 to use the Civil features.
14331   Select BricsCAD TIN volume surfaces to compute cut/fill.
14332   (Automatic mode) Multiple volume grid surfaces will be created with the specified grid size.
14333   (Manual mode) Volume grid surfaces will be created for each selected boundaries.
14334   Enter or show label text size
14335   Enter or show volume grid size
14336   If you upgrade to V 22.2.02 or higher, you will get a much better performance using GeoTools with BricsCAD Civil tools.
14337   The GeoTools floating license for this computer has been returned to the server.
14338   Please try again
14339   minutes after license was last returned.
14340   Important: You must restart your
14341   for the license to be acquired again.
14342   The CADPower floating license for this computer has been returned to the server.
14343   Program Name
14344   Current Drawing Name:
14345   GeoTools-CADPower requires BricsCAD V 23.1.03 or above. You are running BricsCAD V
14346   Please update your BricsCAD to the required version.
14347   GeoTools-CADPower requires BricsCAD V 22.1.04 or above. You are running BricsCAD V
14348   Your current BricsCAD build is
14349   GeoTools-CADPower will not run on this version due to a bug in the Lisp engine.
14350   Please install BricsCAD build 21.2.04 or later, or earlier than 21.2.03.
14351   GeoTools-CADPower requires BricsCAD V 21.1.04 or above. You are running BricsCAD V
14352   GeoTools-CADPower requires BricsCAD V 20.1.05 or above. You are running BricsCAD V
14353   Error: GeoTools/CADPower requires BricsCAD V16 or later. Please upgrade your BricsCAD to a more recent version.
14354   Installation Error:
14355   not found on the ZWCAD search path.
14356   Please copy this file to the search path before attempting to start again.
14357   not found on the BricsCAD search path.
14358   Warning: doslib not loaded, although this is BricsCAD Pro+
14359   BricsCAD Lite version: doslib is not loaded.
14360   not found on the AutoCAD search path.
14361   Please copy this file to the search path before attempting to start GeoTools.
14362   Error: You are using an incorrect version
14363   of Doslib. This software needs DosLib Version 8.xx
14364   of Doslib. This software needs DosLib Version 8.xx or 9.xx
14365   of Doslib. This software needs DosLib Version 9.xx
14366   deleted
14367   Searching for enclosing polygon...
14368   Select objects to create chainage annotations
14369   Select points, blocks to annotate along the curve.
14370   could not be opened for write. Please check if the file has been opened by another application (like Excel)
14371   Error: Cannot find chainage descriptions file:
14372   please ensure that it is a valid file
14373   Warning: Please be aware that intersections will be determined only if the intersecting objects are 2D and at the same elevation.
14374   No block name is selected. A POINT object will be placed during the MEASURE operation.
14375   Enter or show distance to place blocks/points
14376   The selected block does not have any attributes. Cannot set CP_TC properties
14377   There is no blockname selected. The CP_MEASUREMANY command will use points.
14378   There is no need to set CP_TC properties
14379   Select polylines to define the sheets (or ENTER to specify layer)
14380   Select a map sheet [block or closed polyline]:
14381   Select an open polyline representing the mapping area to be covered with sheets:
14382   Error: Polyline is closed. Please select an open polyline object only.
14383   Error: Please select an open polyline object only.
14384   Error: Polyline must have exactly 4 vertices and must be in clockwise direction.
14385   Error: Polyline is open. Please select a closed polyline object only.
14386   Sheet placement mode
14387   Coverage overlap factor
14388   Placing sheet at cut-off length of
14389   Create layouts automatically from map sheets.
14390   Select sheet insertion blocks or polylines representing the sheets
14391   The map sheet block has not been set yet. PLease run the GT_MAPSHEETCREATE command.
14392   The map sheet block must be named
14393   and must already be available and placed.
14394   Enter layout name to create for this sheet
14395   has too many or too few viewports. Please select desired viewport.
14396   Select a viewport in which to zoom the sheet
14397   Type of grid
14398   Pick center of the circular grid:
14399   Pick first [inner] point of grid:
14400   Pick second [outer] point of grid:
14401   Please add suffix: 'I' for inner and 'O' for outer distances, 'A' for angles.
14402   Clockwise distances/angles are +ve and counter-clockwise are -ve.
14403   Multiple distances can be separated by commas.
14404   Pick circular grid point [or enter linear distance/angle from last grid line]:
14405   Distance will be measured from inner point
14406   Pick cross-grid point [or ENTER to specify linear distances from inside point]:
14407   Please add an 'I' suffix for distance from inner point and 'O' from outer point.
14408   Enter linear distances from inside/outside point (multiple values should be separated by commas)
14409   Pick other corner of grid [or ENTER to specify next point for grid orientation (rotated grid)]:
14410   Pick point to determine the primary direction of the grid:
14411   Pick point to determine the other direction of the grid:
14412   Pick start point of horizontal grid line:
14413   Pick start point of vertical grid line:
14414   Pick end point of horizontal grid line:
14415   Pick end point of vertical grid line:
14416   Error: You must draw a horizontal line only.
14417   Error: You must draw a vertical line only.
14418   Pick start point of inclined [horiz axis] grid line:
14419   Pick end point of inclined [horiz axis] grid line:
14420   Pick point for next grid line [or enter distance from last picked point]:
14421   Pick a rotation angle [or enter a rotation anle value].
14422   objects placed in active selection set.
14423   Enter or show grid spacing in X direction
14424   Select Grid Labels Layer
14425   Select Grid Circles Layer
14426   Error: Start angle must be less than end angle [measured clockwise from 0]
14427   Pick start point of inclined [vertical axis] grid line:
14428   Pick end point of inclined [vertical axis] grid line:
14429   Distance of inserted point within segment:
14430   from end.
14431   Distance from mid of original segment:
14432   Parameter 1 (first parameter lookup) is not defined in the INI file but available in the selected entities. Please check and correct your INI file.
14433   CAUTION: You are about to change the object table definition by deleting a field
14434   This can affect data in your drawing which are already attached with the older data structure
14435   Such data will not be automatically updated by this operation
14436   Only new object data attached to entities from now on will have the updated table/field structure
14437   CAUTION: You are about to change the object table definition by moving *UP* the field
14438   CAUTION: You are about to change the object table definition by moving *DOWN* the field
14439   CADPower Object Data Table Name:
14440   Error: There is not enough data to know which object table data must be copied. Please run the command again and specify.
14441   Please select a sheet name from the XLSX file.
14442   Starting row number of data cannot be greater than the ending row number of data.
14443   Ending row number of data cannot be lesser than the starting row number of data.
14444   Processing attributed blocks...
14445   populated with value:
14446   replaced with
14447   Found Title:
14448   Processing text, mtext, dimensions....
14449   A blank tag value
14450   found in XLSX/CSV has been ignored.
14451   Error: One of the tag values
14452   does not start with a '&' or '#' character. Please correct this error before proceeding.
14453   Error: The first title tag must be named as &dwgname. At the moment, it is
14454   Please correct this error before proceeding.
14455   Error: There is no column named '&dwgname'. This parameter is compulsorily required to specify the drawing name to create.
14456   Error: Cannot open .BAT file
14457   for writing. Please check file name and permissions.
14458   Windows BATch File:
14459   Sheet Name has not been selected.
14460   Sheet Name has not been changed.
14461   Select template DWG file
14462   Checking for new updates....
14463   message
14464   Select CADPower license file
14465   CADPower license successfully copied to
14466   Please restart your CAD application to activate the license
14467   Error: CADPower license could not be copied. Please check your file permissions.
14468   Error: The CADPower license file must be a named
14469   only. Please select the file again.
14470   Select GeoTools license file
14471   GeoTools license successfully copied to
14472   Error: GeoTools license could not be copied. Please check your file permissions.
14473   Error: The GeoTools license file must be a named
14474   Error: CADPower installation folder is not defined.
14475   Error: CADPower AppData folder is not defined.
14476   Error: GeoTools installation folder is not defined.
14477   Error: GeoTools AppData folder is not defined.
14478   Lisp applications loaded.
14479   The CADPower installation folder, as set by #AppDir_CP is:
14480   Error: The CADPower installation folder is not set.
14481   The CADPower AppData folder, as set by #MnuDir_CP is:
14482   Error: The CADPower AppData folder is not set.
14483   The GeoTools installation folder, as set by #AppDir_GT is:
14484   The GeoTools installation folder is not set.
14485   The GeoTools AppData folder, as set by #MnuDir_GT is:
14486   Error: The GeoTools AppData folder is not set.
14487   This computername is:
14488   Start date of license:
14489   End date of license:
14490   Your CADPower license has expired [time-based].
14491   Your CADPower license is active [time-wise].
14492   Your GeoTools license has expired [time-based].
14493   Your GeoTools license is active [time-wise].
14494   This
14495   configuration does not use DOSLIB although Pro+ is running.
14496   configuration does not use DOSLIB since Lite is running.
14497   configuration is set to NOT load the CUI(X) file since the 'DoNotLoadUI_CP.Txt' file is present and found.
14498   configuration is set to NOT load the CUI(X) file since the 'DoNotLoadUI_GT.Txt' file is present and found.
14499   Select Windows System Folder to browse to
14500   No Windows System folder was selected.
14501   Select folder to browse to
14502   No folder was selected.
14503   [copied to clipboard]
14504   Enter PAT file to split
14505   Enter patter name to extract (or ALL)
14506   Creating PAT file...
14507   Enter first PAT file [master PAT-to merge into]
14508   Enter second PAT file [to merge from, or 'F' for folder]
14509   Select folder with multiple .PAT files for merging
14510   All .PAT files from this folder will be merged with the source.
14511   Please be aware that the source master PAT file will be updated with the added new patterns from individual PAT file in the selected folder.
14512   Error: This operation requires the dos_getdir function from doslib, if you are using BricsCAD Lite, it will not work. Upgrade to Pro or higher.
14513   Produce detailed listing of PAT data on commandline?
14514   Definition:
14515   Enter new merged HATCH PAT file to create
14516   File update done. Press ENTER to continue
14517   Error: The CADPower application directory location is not set. please try re-installing or set the path to the installation folder.
14518   You must restart BricsCAD for the changes to take effect.
14519   Copied
14520   Target file
14521   Error: The source file 'iso.pat' was not found.
14522   Error: The source file 'default.pat' was not found.
14523   1. Update existing PAT file with an updated, enhanced one [includes geological and architectural hatches].
14524   2. Add AutoCAD SHX files and update BricsCAD support folder.
14525   Error: Cannot find 7z.exe in the same folder where 'ZipInstall.des' exists. Please ensure this file is available.
14526   Error: Cannot find 7z.DLL in the same folder where 'ZipInstall.des' exists. Please ensure this file is available.
14527   Error: The AppData folder could not be determined. Please contact
14528   technical support.
14529   added to support files search path.
14530   No changes have been made to the support files search path.
14531   To specify install location, selected any file on [custom]
14532   Selected [custom]
14533   installation folder:
14534   Selected [default]
14535   Error: Please select a GeoTools ZIP file first to install.
14536   Error: Please select a CADPower ZIP file first to install.
14537   Reading crash report...
14538   CADPower: Create macro to switch off CADPower toolbars
14539   CADPower: Create macro to switch off GeoTools toolbars
14540   CADPower: Create macro to switch off CADPower & GeoTools toolbars
14541   Show Windows System path
14542   BricsCAD Setup/Organize: Show BricsCAD related Support folder path
14543   BricsCAD Setup/Organize: Overwrite default.cui with factory defaults
14544   BricsCAD Setup/Organize: Copy BricsCAD *.PAT files to specified location
14545   BricsCAD Setup/Organize: Copy BricsCAD *.LIN files to specified location
14546   BricsCAD Setup/Organize: Copy BricsCAD *.PAT files to install default location
14547   BricsCAD Setup/Organize: Copy BricsCAD *.LIN files to install default location
14548   BricsCAD Setup/Organize: Copy BricsCAD Drawing Templates to a specified location
14549   BricsCAD Setup/Organize: Copy BricsCAD Drawing Templates to install default location
14550   BricsCAD Setup/Organize: Copy BricsCAD Plot Styles to a specified location
14551   BricsCAD Setup/Organize: Copy BricsCAD Plotter Configuration to a specified location
14552   BricsCAD Setup/Organize: Set command prompt string
14553   BricsCAD Setup/Organize: Create an AutoCAD-like toolbar with common tools
14554   BricsCAD Setup/Organize: Check text for missing (replaced) fonts
14555   BricsCAD Setup/Organize: Copy BricsCAD default.cui file to specified location
14556   AutoCAD Setup/Organize: Copy AutoCAD *.PAT files to specified location
14557   AutoCAD Setup/Organize: Copy AutoCAD *.LIN files to specified location
14558   AutoCAD Setup/Organize: Copy AutoCAD Drawing Templates to a specified location
14559   AutoCAD Setup/Organize: Copy AutoCAD Plot Styles to a specified location
14560   AutoCAD Setup/Organize: Copy AutoCAD Plotter Configuration to a specified location
14561   BricsCAD licensing: Cannot connect to a network license server (error 17)
14562   BricsCAD licensing: How to migrate my license (up to V13) to another computer?
14563   BricsCAD licensing: How to try a higher features level (Pro, Mechanical, BIM)?
14564   BricsCAD licensing: How can I see which license key is in use on a computer.
14565   BricsCAD licensing: Can't connect to Bricsys License Activation Server (err:132/136)
14566   BricsCAD licensing: License Error Code 1024
14567   BricsCAD licensing: Windows Network License server setup help
14568   BricsCAD licensing: How do I setup my network license server on the same computer as license
14569   BricsCAD licensing: How to activate a single license or volume license
14570   BricsCAD licensing: How to configure the proxy server for license activation
14571   BricsCAD licensing: How to configure the proxy settings permanently for Network License use
14572   BricsCAD licensing: Manual License Activation procedure
14573   BricsCAD licensing: Error reading from network (error: 105)
14574   BricsCAD licensing: Manual license activation fails (error: 1007)
14575   BricsCAD licensing: How to revoke an activation after system crash?
14576   BricsCAD licensing: Display the local computer network server administration
14577   BricsCAD licensing: Unknown error - 1030
14578   BricsCAD licensing: How to move a network license to another server?
14579   BricsCAD licensing: Error in http transaction with Activation server. (Error code -136)
14580   BricsCAD licensing: Error Code 3
14581   BricsCAD System requirements
14582   Download the REPRISE network license manager
14583   Network license server administration
14584   Windows network license server setup
14585   Windows: Services
14586   Windows: Remote Desktop Connection
14587   Windows: System information
14588   Windows: Backup and Restore
14589   Windows: Computer Management
14590   Windows: Disk cleanup utility
14591   Windows: Event viewer
14592   Windows: Control Panel
14593   Windows: Microsoft Management Console
14594   Windows: System resource monitor
14595   Windows: Change screen resolution
14596   Windows: Take snap-shot using sniping tool
14597   Windows: Task Manager
14598   Windows: Mouse properties
14599   Windows: Problem Steps Recorder
14600   Windows: Start Chrome browser
14601   Windows: Start Firefox browser
14602   Windows: Action Center
14603   Windows: Add/Remove programs
14604   Windows: Network Connections
14605   Windows: Registry Editor
14606   Select maintenance task to perform
14607   Startup File:
14608   Startup file
14609   already exists @
14610   You need to restart CAD for the changes to take effect.
14611   Error: There is no support folder available with permission to create files in them.
14612   BRICSCAD License Error Code 1024
14613   Error Code 1024 means that an online activation from that computer is not possible because a proxy server is
14614   blocking the communication with our activation server, and this proxy server uses an authentication system
14615   which is not supported by the Reprise activation library we use.
14616   Workaround options:
14617   1. Allow an exception on their firewall for the URL = license.bricsys.com/actpro, port 80.
14618   2. activate the license by Manual Activation through our website.
14619   What is the way to specify the server address if my server and computer are the same?
14620   You can use the following for server name: localhost
14621   On the other hand, adjusting anything in the .lic file will usually cause it to get corrupt and no longer work.
14622   Debug dump file:
14623   The pattern must contain XY or EN coordinates compulsorily, and can have ignorable field(s) specified by 'I'. Point number should be specified as 'P' and Description as 'D'
14624   Examples: PIIENZDI, IIXYII, INEII and similar
14625   Here, I is the field be ignored and E,N or X,Y represent the coordinates, either cartesian or geographic (Long[E]-Lat[N])
14626   Example: PIIENZDI format means that first field is point number, second and third to be ignored, fourth, fifth and sixth are coordinates, seventh is description and eighth to be ignored
14627   If the option 'Specify position-based descriptions' is enabled, the description field must be specified as [D1], [D2] and so on, to specify the location of the description field to consider.
14628   For example,
14629   This option is to be used when the other standard options don't qualify.
14630   Select layer to UNLOCK [ENTER to type name(s)]:
14631   You need BricsCAD Pro V22.2.02 or higher to run this command.
14632   This command does not run in AutoCAD. You need BricsCAD Pro V22.2.02 or higher to run this command.
14633   1 polyline with 2 vertices was ignored. This command needs atleast 3 vertices in a polyline.
14634   3. Update existing LIN file with an updated, enhanced one [includes ARROW linetype and more].
14635   Error: The source file 'iso.lin' was not found.
14636   Error: The source file 'default.lin' was not found.
14637   Pick new location for attribute [ENTER to leave it where it is]:
14638   Show new rotation angle [or type a value / ENTER for no rotation]:
14639   Select alignment object (logitudinal):
14640   Pick point on the alignment where you want the cross-section to be scanned:
14641   The chainage at the picked point is:
14642   Error: The alignment point could not be selected. Please ensure that you are picking a point on the selected alignment only.
14643   Error: This point is invalid.
14644   Check for overlapping entities, if any, to avoid wrong selections.
14645   The suggested number of
14646   points for the cross-section were NOT FOUND.
14647   Do you want to consider processing with the existing points found? There are
14648   of them.
14649   This highlighted selection has
14650   objects. Accept this?
14651   Found a selection with exactly
14652   objects. Accept this for processing?
14653   Enter (or show) corridor thickness to scan for points
14654   Enter (or show) sampling distance along longitudinal section
14655   Enter (or show) corridor width
14656   Select objects to group
14657   Select dimensions to 'Manage extension lines and gaps'.
14658   Select images to detach.
14659   Initial perimeter:
14660   New perimeter:
14661   Select images to reload.
14662   Select images to unload.
14663   Select objects to convert to a block:
14664   Windows: Disk management
14665   GeoTools uses Coordinates Converison functions on BricsCAD V
14666   This function is available in BricsCAD V 24.2.03 Pro and above only.
14667   This command requires BricsCAD V 24.2.03 Pro or higher.
14668   trial expired on
14669   Please upgrade to BricsCAD Pro V 24.2.03 or higher to use the Coordinate transofrmation functions.
14670   Lite version. This command requires BricsCAD V 24.2.03 Pro or higher.
14671   version download reminder will be made after
14672   days.
14673   Yes
14674   No
14675   Buy upgrade
14676   Remind after 7 days
14677   Remind me after 15 days
14678   Do not show this message again
14679   No upgrade, continue with current version
14680   Selected object is on a different floor layer
14681   Error: The source file 'iso-original.pat' was not found.
14682   Error: The source file 'default-original.pat' was not found.
14683   What's New in this update?
14684   A summary of new features in CADPower V25 will be displayed in a web-page
14685   A summary of new features in GeoTools V25 will be displayed in a web-page
14686   once you exit from this dialog box.
14687   You will need to purchase an upgrade to the current version of
14688   The area specified here are in the reporting area units, if specified differently from the source area units
14689   Hole Table - points positions
14690   Enter marker character to check (the new string will be added AFTER the first occurence of this character)
14691   Enter marker character to check (the new string will be added AFTER the last occurence of this character)
14692   The CP_DIMENSIONTAG command uses many settings from the CP_TC command for block name, attribute, scale factor etc.
14693   Other settings for this command can be changed using the CP_DIMENSIONTAG-SETTINGS command.
14694   Select dimensions to tag:
14695   Program mode:
14696   Please restart the command CP_ATTUPRIGHT again to run in 'Automatic' mode. This mode will stay until your CAD software is restarted.
14697   Select blocks with attributes to set them upright.
14698   Move all block attribute to a new location
14699   Rotate all attributes of the block with a single pick.
14700   Current balloon block name:
14701   Attribute tag:
14702   scale factor:
14703   The block name
14704   is not found [not defined] in the current drawing.
14705   The balloon block name is not set.
14706   The CP_TC settings dialog will open now. You must specify a baloon block and an attribute to update.
14707   You can also set other operating parameters like scale factor etc.
14708   Draw a GIS/mapping data polygon
14709   Current settings: Merge Overlap:
14710   Default start point:
14711   Perpendicular segments:
14712   Start point of NEW polyline set as FIRST point of last polyline.
14713   Start point of NEW polyline set as SECOND point of last polyline.
14714   Start point of NEW polyline set as THIRD point of last polyline.
14715   Start point of NEW polyline set as FOURTH point of last polyline.
14716   Error: Cannot close a polygon with less than 3 points.
14717   Included angles:
14718   degrees, within tolerance:
14719   Index value:
14720   added to INI file with a default description of
14721   This section contains all the general parameters required by the program
14722   You will see all the general operating parameters as used by the
14723   An example of all the parameters you can find here is explained below:
14724   Some of the parameters shown here are not relevant as they have been deprecated with newer procedures
14725   We hope the others are self-explanatory.
14726   If you need help with any of them, email me: rakesh.rao@thedesignsense.com
14727   Description of
14728   Attribite value:
14729   Block name:
14730   The INI file already has all the scale factors of inserted blocks. Nothing new was added to the INI file.
14731   The following block scale factors were added to the INI file:
14732   CP_BOM Message
14733   Select a tile block to scale:
14734   Select closed polygonal boundary to fit this tile into:
14735   Please select a close polyline, spline, circle or ellipse object only
14736   Program halted to prevent recursion crash. Please run it again to continue the interactive edit operation.
14737   This is the section specifying Cost & Time per sq.unit area on a per-layer basis
14738   The information is specified in the following format
14739   <Hatch-Layer-Name>=Cost-Per-Sq-Unit,Time-Per-Sq-Unit
14740   You need to specify this information for all layers that you want considered
14741   for processing
14742   Layers which are not specified here will NOT be processed by the program
14743   You need to specify this information for all hatch colors that you want considered for processing
14744   Colors which are not specified here will NOT be processed by the program
14745   The Color specification can be provided as basic colors like
14746   Red,Yellow,Green,Blue,Cyan,Magenta and White
14747   This is the section specifying Cost & Time per sq.unit area on a per-pattern basis
14748   You need to specify this information for all hatch patterns that you want considered for processing
14749   Hatch patterns which are not specified here will NOT be processed by the program
14750   Hatch pattern-based report
14751   Cost-Time info INI file:
14752   Dummy cost/time information added to
14753   unused
14754   cost/time information already contained in
14755   for color
14756   for hatch pattern
14757   Hatch pattern
14758   The 'Time-Per-Sq-Unit' parameter is optional and is defaulted to 0.0
14759   -or-
14760   with a CAD color number from 1-255
14761   Hatch Pattern,Area,Num_Objects,Unit Cost,Total Cost, Unit Time,Total Time
14762   Number-Of-Objects
14763   Unit Time
14764   Total Time
14765   Hatch-Pattern,Area,Num_Objects
14766   PatternName
14767   Hatch Color,Area,Num_Objects,Unit Cost,Total Cost,Unit Time,Total Time
14768   Hatch Color
14769   Color,Area,Num_Objects
14770   Hatch Layer,Area,Num_Objects,Unit Cost,Total Cost,Unit Time,Total Time
14771   Hatch Layer
14772   Layer,Area,Num_Objects
14773   Specify the cost-time-INI file name
14774   in the current drawing [or] folder [or] search path [or] CADPower installation support folder.
14775   CADPower LevelIt tool
14776   Select a Levels block DWG to import
14777   Pick point to place reference levels block
14778   Pick point to place levels block
14779   unused
14780   Reference levels block:
14781   placed with a reference level of
14782   Levels block:
14783   placed with a level of
14784   Error: There is no reference block in this drawing. Please place a reference block before you can place a levels block on the drawing.
14785   Please select a levels block before you can place one on the drawing.
14786   A reference levels entity already exists in this drawing
14787   and has been highlighted.
14788   Do you want to replace it with a new one?
14789   If yes, you must now select a new reference level object
14790   Please select a levels block before you can place one as reference.
14791   click on 'Add block' to use this as level block.
14792   Error: No levels block has been selected. Please select one before you can configure settings.
14793   added to the list as a levels block.
14794   You can select it from the 'Levels Blocks' list.
14795   added to the list as a levels block
14796   is already selected as a Levels block.
14797   Block not selected. Please select one from the list of available blocks in this drawing.
14798   The Block scale factor has been changed. This will affect
14799   existing levels block(s).
14800   and they will be changed to the specified scale of
14801   The change will be visible when you exit all dialogs with an 'Ok'
14802   Do you want to continue?
14803   The Reference Level of the block has been changed. This will affect
14804   and their elevations will be updated as per the new reference level of
14805   Changing the block scale factor from
14806   [ESC to finish]
14807   for processing.
14808   This is the section specifying Cost & Time per sq.unit area on a per-color basis
14809   You need to specify this information for all object colors that you want considered for processing
14810   The dialog box user-interface for this command has been hidden as per user-settings. Re-open this drawing to get back the dialog boxes.
14811   Select objects for area calculation (polylines, circles, splines and ellipses are permitted)
14812   Area sorting direction has been set to 'Decreasing' since 'IslandDetect' mode is ON
14813   There are:
14814   items in selection
14815   Select polygon text label layer
14816   for layer
14817   Clr
14818   Found:
14819   area entities within this polygon.
14820   Enter (or show) search distance around point of interest
14821   Sorting direction is +X. All points with equal Y values will be grouped and sorted to create one polyline.
14822   Sorting direction is +Y. All points with equal X values will be grouped and sorted to create one polyline.
14823   Sorting direction is -X. All points with equal Y values will be grouped and sorted to create one polyline.
14824   Sorting direction is -Y. All points with equal X values will be grouped and sorted to create one polyline.
14825   SMART SORT is on: Sorting direction is +X. All points with equal Y values will be grouped and sorted to create one polyline.
14826   SMART SORT is on: Sorting direction is +Y. All points with equal X values will be grouped and sorted to create one polyline.
14827   SMART SORT is on: Sorting direction is -X. All points with equal Y values will be grouped and sorted to create one polyline.
14828   SMART SORT is on: Sorting direction is -Y. All points with equal X values will be grouped and sorted to create one polyline.
14829   The sheetname
14830   was picked up from within the sheet.
14831   The sheetname
14832   Repeat last operation?
14833   Select sheets to attach part names to:
14834   Select layer name for sheet labels
14835   Specify partnames CSV file-name
14836   There are existing
14837   hole-table annotation and table entities.
14838   Do you want to delete them?
14839   CP_HOLETABLE command cannot continue unless existing annotation entities and table are deleted.
14840   Please delete them manually or select 'Yes' in CP_HOLETABLE command to delete them automatically.
14841   The hole-table layer filter has been reset to include all entities inside the frame, irrespective of layers.
14842   You may run the CP_HOLETABLE command again to specify the layer filters, if they have changed.
14843   Current Hole table parameters updated [stored] in frame entity.
14844   Select input layers for holes
14845   File 'default.pat' copied to
14846   This command is not available in the A2B breakout module. Please use the full CADPower to get this tool.
14847   You may please contact rakesh.rao@thedesignsense.com (+91-9243438300) for more info.
14848   Enter command name to check
14849   Group named
14850   created from selected objects.
14851   Select a block insert object
14852   Please select a block insert object only
14853   Enter new block name
14854   renamed to:
14855   Error: Block
14856   Source and target block names cannot be the same.
14857   Please select a block insert entity only.
14858   Pick first clipping point:
14859   An un-named group was created from the selected objects.
14860   ARRAY
14861   ARRAY Classic
14862   BREAK
14863   Change properties [CHPROP]
14864   Change command
14865   Copy
14866   Ellipse
14867   3DPOLY
14868   Point
14869   Solid
14870   Array 3D
14871   Rotate 3D
14872   Mirror 3D
14873   Donut
14874   Erase
14875   DDEdit
14876   Fillet
14877   Insert
14878   Line
14879   List
14880   Move
14881   Mirror
14882   Offset
14883   Pedit
14884   Pline
14885   Regen
14886   Rotate
14887   Scale
14888   Object snap mode set to NODe
14889   Stretch
14890   Trim
14891   DText
14892   Undo Control None
14893   Undo All
14894   WBlock
14895   Explode
14896   Extend
14897   Zoom All
14898   Zoom Dynamic
14899   Zoom Extents
14900   Zoom Full (with margins)
14901   Zoom Previous
14902   Zoom Window
14903   3DFACE
14904   EDGESURF
14905   RULESURF
14906   TABSURF
14907   REVSURF
14908   APERTURE
14909   VPOINT
14910   CHAMFER
14911   DIM HORIZONTAL
14912   DIM VERTICAL
14913   DIM ALIGNED
14914   DIM LEADER
14915   UCS WORLD
14916   UCS X (rotate)
14917   UCS Y (rotate)
14918   UCS Z (rotate)
14919   VIEW
14920   VIEW DELETE
14921   VIEW RESTORE
14922   VIEW SAVE
14923   VIEW WINDOW
14924   VIEW ?
14925   is already on.
14926   is already locked.
14927   is already un-locked.
14928   is already switched off.
14929   is already thawed.
14930   is already frozen.
14931   is already switched on.
14932   is an XREF layer and cannot be locked.
14933   is an XREF layer and cannot be unlocked.
14934   Lock ALL layers
14935   Unlock ALL layers
14936   Create a new layer
14937   CADPower message:
14938   The PURGE All command was run twice.
14939   Set Screen Pan Factor
14940   Type of block to create:
14941   Drawing units:
14942   1. Inches
14943   2. Feet
14944   3. Millimeters
14945   4. Centimeters
14946   5. Decimeters
14947   6. Meters
14948   PowerTools Video:
14949   CADPower Cloud license requested, enter GUID code for this computer
14950   CADPower cloud license file updated.
14951   GeoTools Cloud license requested, enter GUID code for this computer
14952   Checking GeoTools license
14953   GeoTools cloud license file updated.
14954   Existing license file has been deleted.
14955   CADPower license was found at this location:
14956   Do you want to remove this license from the computer
14957   CADPower license removed successfully.
14958   Error: CADPower license could not be removed. Please check file delete permission for that folder.
14959   This computer does not contain any valid [activated] CADPower licenses.
14960   GeoTools license was found at this location:
14961   GeoTools license removed successfully.
14962   Error: GeoTools license could not be removed. Please check file delete permission for that folder.
14963   This computer does not contain any valid [activated] GeoTools licenses.
14964   DES-Lisp applications loaded.
14965   Folder name for temporary CAD files:
14966   Folder name for auto-saved dwg files:
14967   Auto-saved drawing found at:
14968   There is no auto-saved drawing available yet.
14969   Selected PAT file:
14970   Selected source PAT file:
14971   Selected .PAT folder:
14972   Selected file:
14973   Hatch Pattern List
14974   Pattern:
14975   First PAT file  :
14976   Second PAT file :
14977   Hatch patterns that are common to BOTH master file and the merge target PAT files.
14978   Hatch patterns that were FOUND in master file, but not found in the merge target PAT files.
14979   Hatch patterns that were FOUND in the merge target PAT files, but not in the master file.
14980   Warning: There is no write-access on removable drive
14981   Writeable support path:
14982   Enter macro to create
14983   Error Code 3 means probably that there is some  unwanted information in the REPRISE folders
14984   activation again. If this still does not resolve the problem, try manual  activation.
14985   But please remember that manual activation is restrictive in nature and you cannot de-activate
14986   the license again if activated manually.
14987   Please do your best attempts to activate the license online
14988   Select crash report file to save
14989   Crash report file of
14990   saved as
14991   Select crash report file to read
14992   Select GeoTools ZIP file
14993   Select CADPower ZIP file
14994   Select folder to install
14995   This operation updates the hatch patterns file, and adds several new ones.
14996   A number of commonly required but missing PAT files from AutoCAD support is copied to the below folder:
14997   The following is a complete list of the PAT files copied:
14998   This operation updates the fonts, and adds several new ones.
14999   A number of commonly required but missing SHX files from AutoCAD support is copied to the below folder:
15000   The following is a complete list of SHX files copied:
15001   This operation updates the default.lin and iso.lin files, and adds several new ones.
15002   A number of commonly required but missing linetypes from AutoCAD support is copied to the below folder:
15003   This operation copies back the original PAT file, if CADPower had earlier updated it with the enhanced one.
15004   This is usually required by some users if they feel that the HATCH command is operating too slowly while opening up the patterns list using the new PAT files.
15005   You can either revert to the original PAT files or use the CP_QHATCH command as an alternative <Default.Pat> and <Default-ISO.pat> files will be copied from
15006   the CADPower installation folder to the Support folder as shown below.
15007   Error: Cannot exit from the dialog until the PAT folder for individual PAT files has been specified.
15008   Error: Cannot exit from the dialog until the target PAT file has been specified.
15009   Error: Cannot exit from the dialog until the source PAT file has been specified.
15010   Enter source PAT file
15011   Select target PAT file folder
15012   Enter final merged PAT file
15013   Error: Please select a target folder for splitted PAT files before you can exit from this dialog box.
15014   Error: Please select a pattern name to extract from master PAT file.
15015   Error: Please select a source PAT file before you can exit from this dialog box.
15016   'GT_NODELINESNAP' message
15017   The 'GT_NODELINESNAP' command works with lines, polylines and point features.
15018   Duplicate and incorrect geometry of any kind, whether they are duplicate points,
15019   duplicate polyline vertices and/or zero-length lines and polylines can create this
15020   tool to malfunction or yield incorrect/illogical results.
15021   We advise you to check for these kinds of geometry in the data and correct them
15022   before you use this tool.
15023   Creating boundaries around the centroidal points....
15024   If must upgrade to V 22.2.02 or higher, in order to use the BricsCAD Civil and TIN features.
15025   Lite. You must upgrade to V 22.2.02 Pro or higher, in order to use the BricsCAD Civil and TIN features.
15026   Select surface name to save
15027   points in the TIN selection.
15028   Fatal error: Cannot load the TIN engine. Please check your BricsCAD license or installation.
15029   entity handle
15030   Sorting intersection points by distance...
15031   done
15032   (none selected)
15033   No new vertices were added. Drape surface interpolation was done at each vertex point of the source polyline.
15034   Select a BricsCAD TIN surface object:
15035   BricsCAD TIN surface object moved in Z direction by
15036   Please select a BricCAD TIN entity only.
15037   Select layer fo extracted TIN objects
15038   Extract triangles, points and borders from a BricsCAD TIN surface.
15039   ExtractWhat
15040   objects extracted from the TIN surface.
15041   Error: Selected object
15042   is not a BricsCAD TIN surface.
15043   Find the elevation of a BricsCAD TIN surface at a given point.
15044   Select a BricsCAD TIN surface object [or ENTER to use current entity]:
15045   Pick point to get surface elevation:
15046   The elevation of the surface at the picked point is:
15047   The elevation of the surface at the picked point could not be determined.
15048   Assigns point and lines with underlying surface elevations from a BricsCAD TIN object.
15049   Select lines, polylines, points and/or location blocks
15050   The elevation of the surface at the point
15051   could not be determined.
15052   Returns key surface statistics from a picked BricsCAD Civil surface.
15053   Get statistics for?
15054   Select a closed polyline, spline, ellipse or circle, within which to generate statistics:
15055   Error: Selected object is not closed. Please select a closed curve object.
15056   is not a valid selection for a terrain delimitation boundary. Please select a closed curve object.
15057   points in the selected TIN area.
15058   X coordinates:
15059   Minimum:
15060   Maximum:
15061   Y coordinates:
15062   Z coordinates:
15063   Error: the required TIN surface points could not be obtained. Please check the TIN surface or your area or interest.
15064   is not a valid BricsCAD Civil TIN entity.
15065   Error: temp file
15066   could not be deleted in Windows TEMP folder.
15067   Name:
15068   Error: GT_KML2DWG cannot continue.
15069   A doc.kml file could not be found in the KMZ file upon extraction.
15070   Coordinate conversion from Lat-Long to UTM is possible only while using BricsCAD Pro V 24.2.03 or above.
15071   Coordinate conversion from Lat-Long to UTM will be performed on the coordinates from the selected KML file.
15072   Enter KML/KMZ file name to read
15073   Error: Please select a KML/KMZ input file.
15074   Adjust the 3d segment length in polylines to match the selected values from clipboard
15075   Select a polyline for length setting:
15076   Error: Please select a polyline entity only.
15077   There are [
15078   ] vertices and [
15079   ] segments in the selected polyline
15080   Please select EXACTLY [
15081   ] *new* segment lengths to update. These must be copied to the clipboard.
15082   Please note that each segment length to update can be *MORE* or *LESS* than the existing segment length in the polyline.
15083   If segment length is more, the XY coordinate of the end is not changed, but the Z elevation is adjusted to get the required segment length
15084   If segment length is lesser, then the XY coordinate (and Z) of the end of the segment is change to get the required segment length
15085   When this happens, all the remaining segment lengths of the polyline are recomputed based on the new length
15086   Existing Segment lengths:
15087   Select the segment lengths from Excel (or text file) and click 'Ok' when ready.
15088   Current selection has only one row of data with
15089   The selection is not in a proper format. You must select one single row or column of data, not multiple rows or columns
15090   The clipboard is empty. Please select something into the clipboard.
15091   Segment lengths from Excel:
15092   Segment number:
15093   The new segment length
15094   is less than the existing segment length of
15095   XY will be updated.
15096   Success: Existing segment length: [
15097   Segement lengths are the same in polyline and in file, no further processing is required for this segment.
15098   The file segment length is
15099   and  the existing polyline segment length is
15100   Z will be updated
15101   Error: Number of items in the new lengths selection (
15102   ) is not the same as those in the polyline (
15103   Select attributed blocks to update:
15104   Select a text object (in order) to update [ENTER to finish]:
15105   This text object is already selected once.
15106   Error: Selected object is not a TEXT or MTEXT.
15107   Select a block object (in order) to update [ENTER to finish]:
15108   This block object is already selected once.
15109   Error: Selected object is not a block insert object.
15110   An existing
15111   was found in the vicinity of
15112   and updated.
15113   Error: Please select a block name before you can edit the 'Multiple attributes increment setup' dialog
15114   Current baloon block name:
15115   The baloon block name is not set.
15116   items
15117   Edit Civil 3D Property Set data in BricsCAD
15118   Select objects to edit Civil 3D Property set data belonging to
15119   Edit Civil 3D Property definition set
15120   1 object skipped. It did not have Civil 3D Property set data belonging to
15121   Please select a Civil 3D property set to edit, before you can proceed further.
15122   Transfer block attributes Civil 3D property definition sets.
15123   Select block with attribute:
15124   Contour interval
15125   If you upgrade to V 22.2.02 Pro or higher, you can create contours by selecting BricsCAD TIN object.
15126   Now, you can only create contours if you have existing 3dfaces, 3d polylines.
15127   Lite version. You will need BricsCAD V 22.2.02 Pro or higher to create contours from BricsCAD TIN object.
15128   Select BricsCAD TIN object (for contour extraction):
15129   Drawing a minor contour polyline of elevation
15130   [Number of vertices:
15131   Drawing a major contour polyline of elevation
15132   Select 3dfaces/polylines as input for contour creation [or ENTER to select by layer]:
15133   Select layer for TIN objects (3dfaces/polyliness)
15134   TIN objects found.
15135   The starting Z value of contours set to the minimum existing value of
15136   The ending Z value of contours set to the maximum existing value of
15137   Minimum Z of contours:
15138   Start Z:
15139   Maximum Z of contours:
15140   End Z:
15141   Drawing contours from elevation....
15142   You must upgrade to V 22.2.02 or higher, in order to use the BricsCAD Civil and TIN features.
15143   Lite. You must upgrade to V 22.2.02 Pro or higher, in order to use the BricsCAD Civil and TIN features.
15144   You must select a BricsCAD TIN object for contouring after clicking 'Ok' and exiting this dialog.
15145   You must select the TIN objects (3dfaces/polylines) for contouring after clicking 'Ok' and exiting this dialog.
15146   contourElev:
15147   Highlight last processed selection with grips
15148   Enter beep on error sound
15149   Force re-load of CUI at startup?
15150   Enable voice mode for command prompts?
15151   Enable CADPower shortcuts upon start?
15152   Automatic MOVEBAK after every save?
15153   Enter beep on error type
15154   Enter (or show) the chord length distance
15155   Enter (or show) the chord offset (crown) distance
15156   Enter (or show) the length of the polyline
15157   Enter (or show) the segment length of the polyline
15158   Enter (or show) the radius of the circle (or arc)
15159   Enter (or show) the width of the polyline
15160   Enter (or show) the start-end points distance of the polyline
15161   Getting average text height...
15162   exit.
15163   Transfer selected Excel data into object table attached data in AutoCAD
15164   Please select from Excel or a text file the data that contains the attribute/field names, and click on 'Ok' when done.
15165   existing object from layer
15166   Current selection
15167   has only one column of data.
15168   You must select a minimum of two rows, of which the first one must be the title row
15169   Current selection has
15170   row and
15171   columns of data.
15172   -Select a field name (Excel data)-
15173   Specify the field to check in Excel data:
15174   Specify the field in Excel data:
15175   Object table name:
15176   selected key field is
15177   (exist in the object table also)
15178   Select objects to attach Excel data as object table data.
15179   Object Table:
15180   Object table field:
15181   set with value
15182   from Excel data.
15183   Error: 1 object ignored: The field name
15184   from Excel does not exist in the object table.
15185   Error: 1 object ignored: The field value
15186   cannot be found in the Excel data.
15187   1 object ignored. Property value:
15188   could not be obtained.
15189   Error: There is no key field 
15190   in the object table
15191   attached to this entity.
15192   [Warning]: 1 object ignored. There is no key field
15193   attached to this entity.
15194   Error: The field name
15195   from Excel does not exist in the entity.
15196   The program will terminate now as per the error handling parameters set in the program.
15197   Warning: 1 field skipped, the field name
15198   1 object ignored. There was no matching object data with the specified key Excel field.
15199   1 object ignored. There is no object table named
15200   1 object ignored. There is no object table attached to this entity.
15201   objects not processed, placed in active selection and in layer
15202   Error: The specified key field from Excel
15203   does not exist in the object table.
15204   has only one row of data.
15205   You must select a minimum of two rows, of which the first one must be the title row.
15206   Reset object table data to its default values.
15207   Specify the object table name to reset:
15208   Enter object table name
15209   Select objects to from which to reset the object table data.
15210   Processing objects, removing object table data....
15211   Please select a CAD property to match, before you can exit.
15212   Please select a field name before you can exit.
15213   Please select an AutoCAD Map Object table before you can exit.
15214   If specified field in Excel is missing in target object table, the program will flag an error and stop.
15215   If specified field in Excel is missing in target object table, the program will ignore and continue.
15216   The object data field specified in Excel will be matched against the selected CAD property in the objects.
15217   The object data field specified in Excel will be matched against the selected object data field in the objects.
15218   Error: No target objects selected. Please select some before we can proceed further.
15219   Error: No source objects selected. Please select some before we can proceed further.
15220   entity:
15221   Enter (or show) ENDpoint search tolerance distance
15222   Enter (or show) NEArest search tolerance distance
15223   Enter (or show) NODe search tolerance distance
15224   Folder
15225   object(s) were found in the proximity of the vertex.
15226   Error: Cannot find GEOL_bore_hole_block.dwg in the current folder [or] search path [or] installation folder.
15227   Error: Cannot find GEOL_bore_hole_block_collar.dwg in the current folder [or] search path [or] installation folder.
15228   Select bore hole drill data (collar/plan) file
15229   Error: Please select a valid file name for bore hole log data file.
15230   WARNING: Strike angle position in data-file not defined
15231   Clicking 'Continue' will ignore this field?
15232   'Specify' will require you to enter a valid Strike angle data position.
15233   GeoTools-Mining message
15234   WARNING: Dip Angle position in data-file not defined
15235   'Specify' will require you to enter a valid Dip Angle data position.
15236   Error: Please select a bore-hole block name.
15237   Error: Bore-hole strata definition file not set.
15238   Error: Please select a valid bore-hole data file name to import.
15239   Error: Field position for Z-Height cannot be set as 0
15240   Error: Field position for Y-Northing cannot be set as 0
15241   Error: Field position for X-Easting cannot be set as 0
15242   Select bore hole strata presentation paramet6er file
15243   Error: No bore hole strata data could be read from the CSV file.
15244   Please check your data file.
15245   Select a layer for bore-holes
15246   Error: Bore hole strata information could not be read from the file
15247   Error: Cannot find bore-hole block
15248   objects created.
15249   Read bore-hole info from ASCII files and create lithology cross-section view [2D]
15250   This is the format of the strata presentation INI file
15251   Here, you specify each strata name, its description, hatch pattern, color, scale and angle
15252   The Litho name is followed by an '=' character and followed by the other values
15253   separated by commas.
15254   Warning: You have not selected all or some of the 'More properties' section of the CSV file
15255   If your data does not have additional strata properties, it is ok.
15256   If you have additional strata properties, and would like them to be attached to the bore-holes,
15257   please specify the data positions in this section.
15258   Do you want to continue without specifying the additional bore-hole properties?
15259   Please select a bore-hole strata definition file (CSV) before you can proceed.
15260   Please select a bore-hole strata presentation paraneter file (INI) before you can proceed.
15261   Select bore hole strata presentation parameters file
15262   Select bore hole strata definition file
15263   In the bore-hole seams data file, a suggested minimum structure is shown below
15264   It is not mandatory that the bore-hole structure must be exactly like this
15265   It is mandatory that the above fields exist, but they can be in any order
15266   If the structure is different, they must be correctly mentioned in the main
15267   dialog box in the column positions selection
15268   Error: Please select a valid file name for strata file.
15269   Warning: A valid bore-hole strata presentation file has not been
15270   selected.
15271   Do you want to continue without a strata presentation file?
15272   Error: Please select a valid bore-hole strata definition file name.
15273   Error: Field position for 'To' level cannot be set as 0
15274   Error: Field position for 'From' Level cannot be set as 0
15275   Error: Field position for 'Strata Code' cannot be set as 0
15276   Error: Field position for 'Bore-hole name' cannot be set as 0
15277   Select bore-hole adata file
15278   Select bore-hole strata presentation parameters file
15279   Error: 'Borehole-Name' is a mandatory field and cannot be left blank.
15280   Error: 'Strata-Code' is a mandatory field and cannot be left blank.
15281   Error: 'Strata Code' is a mandatory field and cannot be left blank.
15282   Error: 'From' is a mandatory field and cannot be left blank.
15283   Error: 'To' is a mandatory field and cannot be left blank.
15284   Recovery percentage information not provided, will NOT be read from the CSV file.
15285   'Recovery Total' information not provided, will NOT be read from the CSV file.
15286   Error: 'Start From Row' is a mandatory field and cannot be left blank.
15287   Error: Strata presentation file
15288   does not contain required info.
15289   Pre-processing row #
15290   Warning: The 'From' elevation of the first record of bore-hole
15291   is not 0.0
15292   If this is an error, please click 'No' and correct this error. If these are seam data that need not
15293   be shown from 0.0 contiguously, click on 'Yes' and continue further
15294   Do you want to continue processing this file?
15295   Error: The 'To' elevation
15296   is less than 'From' elevation
15297   in record number
15298   of the bore-hole
15299   Please correct the error in data-file
15300   of previous strata does the match the 'From' elevation
15301   of current strata in record number
15302   Pick start point of annotation:
15303   Processing bore-hole data....
15304   Error: Hatch for strata
15305   Success: Hatch for strata
15306   Error: Hatch for strata seam
15307   Connect lithological strata [seams] in 2D
15308   Select first lithology seam:
15309   Select second lithology seam:
15310   Error: The polyline must have exactly 4 vertices.
15311   Error: The polyline must have XDATA corresponding to the strata and presentation.
15312   Select bore-hole blocks named
15313   Strata data: of borehole
15314   stored as Xdata.
15315   Error: 1 bore-hole with no bore-hole name in the attribute BH_NAME ignored.
15316   Select layer for detailed bore-hole map
15317   Select layer for bore-hole strata border
15318   Select layer for bore-hole (axis only)
15319   Pick start point of strata annotation:
15320   Reading sheet...
15321   from
15322   Creating the TIN...
15323   Error: The soil classification in one of the rows of bore-hole
15324   is left blank. Please provide soil classification types for all strata.
15325   Row #
15326   from the XLSX ignored.
15327   Please enter or select 0 as column number if data does not exist.
15328   The selected lithology seams are:
15329   leftover (unconnected) seams in the second litho. They will be merged with the bottom of first litho.
15330   Pre-processing bore-hole data, bore-hole:
15331   1 bore-hole with no name ignored.
15332   Building 3d cross-section of bore-hole
15333   Creating a 3DFACE surface for strata
15334   Here, you must provide the general parameters required for the mining lease area
15335   Each parameter is represented by a tag and a value, which has the following format:
15336   Name=<name>
15337   This tag is repeated multiple times in the INI file
15338   The tag identifier is 'Name' and must not be changed.
15339   The tag value is <Name> and should be replaced with whatever is the actual
15340   name of the property
15341   For example, a default template value of Name=<Name> may be replaced
15342   as Name=Balaghat Mine
15343   In this way, you need to change the property names in this section
15344   You can create new entries or edit existing ones in the template
15345   Use the 'New' or 'Duplicate' feature for the same
15346   At the end of the editing, remember to 'save' the INI file before you exit
15347   from the INI_EDITOR dialog box
15348   The Feature class data is set and edited here
15349   It has an example format which looks like this
15350   Name=Mining Lease Boundary,LEASE_BOUNDARY,Polygon,1,0.40,(none)
15351   Name=Proposed Bore Hole,PROPOSED_BORE_HOLE,Point,4,0.00,GEOL_BORE_HOLE_BLOCK
15352   Name=Section Line,SECTION_LINE,Line,87,0.00,(none)
15353   Name=Water Drain,WATER_BODY_DRAIN,Line-Polygon,3,0.20,(none)
15354   The first part, 'Name=' must be left as it is and not changed
15355   The last part is the actual data and contains six fields
15356   Example: Name=<FeatureClassName>,<FeatureClassLayer>,<FeatureClassType>,..
15357   <FeatureClassColor>,<Lineweight>,<BlockName>
15358   You can give any name for <FeatureClassName> and <FeatureClassLayer> as per your project
15359   The <FeatureClassType> should be either of 'Point', 'Line', 'Line-Polygon' or 'Polygon
15360   The last parameter, <BlockName> is applicable only for 'Point' feature class
15361   It will be noted as (none) for all other feature class types
15362   A 'Point' feature class is represented by a block object
15363   A 'Line' feature class is represented by a open polyline object
15364   A 'Line-Polygon' feature class can either be an open polyline or closed polyline.
15365   A 'Polygon' feature class is represented by a closed polyline object.
15366   Read lease definition file (INI)
15367   Feature Name:
15368   FeatName
15369   FeatLyr
15370   Type:
15371   FeatType
15372   Color:
15373   FeatClr
15374   Feature Block:
15375   FeatBlk
15376   - From point:
15377   - To point:
15378   Pick point to place
15379   [Primary units]: The length [perimeter] of the digitized
15380   object is :
15381   L-Unit-Source
15382   [Primary units]: The area of the digitized
15383   [Alternate units]: The length [perimeter] of the digitized entity is :
15384   L-Unit-Reporting
15385   [Alternate units]: The area of the digitized entity is :
15386   A-Unit-Reporting
15387   Warning: Geological lease area planner parameters INI file has not yet been set. Any parameters set will not be saved.
15388   Creating layer
15389   with color
15390   There are no dwg files in the folder
15391   Press ESC to exit.
15392   In this section, you must specify the description and folder path where each set of blocks are located.
15393   As an example, we have provided the following folders ready-made in the GeoTools installation:
15394   These folders do exist in the GeoTools installation folder, and you can move them to a different location if desired.
15395   You can copy your existing library of blocks into specific folders and specify the path correctly here.
15396   If you are working on a shared network, a network folder path also can be specified.
15397   so that multiple GeoTools users can access the same library blocks resources.
15398   *Warning*: Cannot find
15399   in the current drawing [or] folder [or] search path [or] GeoTools installation support folder.
15400   Pick point to place the lithology cross-section map (2D) for this borehole:
15401   **** ENTER the SPT Values now.***
15402   Enter elevation[-1 to exit]
15403   Enter SPT value
15404   In this format, an Excel workbook is required (not CSV). The XLSX file must have the bore-hole information in separate sheets
15405   One sheet per bore-hole, and the name of the bore-hole should match the name of the sheet
15406   In each bore-hole sheet, the data is organized column-wise, with some mandatory columns and some optional.
15407   The optional columns can be ignored by entering the column number as 0
15408   The mandatory columns are coordinates (E & N), Sea-bed depth, Borehole depth and Soil classification
15409   The optional parameters are CR%, RQD and STP
15410   The order of any of these parameters in the CSV file is not important and can be specified during the program run
15411   In this format, the CSV file is expected to have [Bore-hole name], [Cumulative depth] values, [SoilClass-Lithology] as *MANDATORY* values arranged row-wise
15412   The block names for each soil classification is defined as per the soil classification.
15413   For example, PEAT block is defined as three blocks: PEAT, PEAT1 and PEATp5 with defined thicknesses of 1.5, 1.0 and 0.5 units respectively.
15414   All depth measurements are composed using a combination of these blocks
15415   and the remaining distance is achieved by scaling the last block used.
15416   Other values like [SPT-N] and [SPT distance], [RR(%)] and [RQD(%)] are not mandatory and used only if specified and available
15417   In this format, the CSV file is expected to have [Bore-hole name], [From-depth], [To-depth] and [SoilClass-Lithology] as *MANDATORY* values arranged row-wise
15418   The strata [lithology] is depicted using HATCH patterns, which must be specified in a separate INI file called the Strata Presentation parameters INI file.
15419   The order of any of these parameters in the CSV file is not important and can be specified during the program run.
15420   In this format, the lithological classification is not shown, but the strike and dip directions are drawn in the drawing in 3D
15421   The required values here are [Borehole Number], [Easting], [Northing], [RL-Elevation], [Dip-Angle], [Strike-Angle], [Dirlled Length]
15422   The bore-hole drilled length is depicted using a normal 3d polyline.
15423   Select layer for bore-hole profile
15424   Please note that the 'Sample Name' column is read until an 'END' string is found. This specifies end of the current bore-hole data.
15425   Error: You MUST select a position 1 or higher for the starting row location in the CSV file.
15426   Error: You MUST select a position 1 or higher for the depth value location in the CSV file.
15427   Error: You MUST select a position 1 or higher for the sample name location in the CSV file.
15428   Error: You MUST select a position 1 or higher for the Soil Classification location in the CSV file.
15429   Select bore hole strata file
15430   Error: The CSV file
15431   containing bore-hole strata profile cannot be found.
15432   Error: The CSV file containing bore-hole strata profile has not been specified/selected.
15433   EastingCol:
15434   NortingCol:
15435   ***Please note:: The Ground water level information for the borehole is expected to be present in the same row as bore-hole name.
15436   ***Please note:: The Reduced level of the bore-hole at surface is expected to be present in the same row as bore-hole name.
15437   ***Please note:: The Easting coordinate of the bore-hole collar at surface is expected to be present in the same row as bore-hole name.
15438   ***Please note:: The Northing coordinate of the bore-hole collar at surface is expected to be present in the same row as bore-hole name.
15439   A soil classification value is missing in column number
15440   for depth =
15441   Please correct this mistake because GEOL_STRATABUILDER cannot produce accurate results if critical data is missing.
15442   It is also possible that you may have not assigned the column positions for Soil classification correctly. Please check if that is the case.
15443   Error: Soil clasification value could not be obtained from specified column numnber
15444   Please check if you have assigned the Soil clasification column number correctly in the CSV file.
15445   Error: Depth value could not be obtained from specified column numnber
15446   Please check if you have assigned the depth column number correctly in the CSV file.
15447   Row:
15448   sets of SPT values for the bore-hole
15449   sets of RR-RQD values for the bore-hole
15450   Drawing 3d cross-section of bore-hole
15451   Strata:
15452   Cut Volume roof :
15453   Fill Volume roof :
15454   Cut Volume floor :
15455   Fill Volume floor :
15456   Select strata/seam(s) to view
15457   thawed and switched on.
15458   frozen.
15459   There are no strata/seams layers in this drawing.
15460   Select strata/seam(s) to build volumne table
15461   Computing area of
15462   of seam
15463   Enter scale factor for table
15464   error
15465   All entities in selected layers will be processed.
15466   Entities from within the selection set
15467   belonging to selected layers will be processed.
15468   Select lines, arcs, circles, polylines or splines/ellipses from the layers:
15469   ARC,CIRCLE,ELLIPSE,LINE,POLYLINE,LWPOLYLINE,SPLINE
15470   Error: No layers have been selected. Please select some layers first and then select the objects.
15471   Processing layer...
15472   objects from layer:
15473   [model-space] changed to layer
15474   There are no entities in model space in layer
15475   [paper-space] changed to layer
15476   There are no entities in paper space in layer
15477   is not an XREF layer and has been ignored.
15478   The following layers were renamed:
15479   Existing layer
15480   New layer
15481   CP_LAYERMAN layer-name editor
15482   Enter new layer-name
15483   Error: Cannot rename more than one layer together. Please select only one layer name
15484   Error: Layer 0 cannot be renamed.
15485   Error: No layer selected. Please select only one layer name
15486   The Resolve-XREF operation renames *all* incoming XREF related layers by removing the <xref>$0$... prefix that appears in front of all such layers.
15487   For example, a layer <xref>$0$WINDOWS will get renamed to WINDOWS.
15488   If the layer WINDOWS already exists, then the contents are merged with the existing layer.
15489   Please be aware that we will not be able to change entities to the correct layer if such $0$ layers are in entities within blocks.
15490   If there are still <xref>$0$... layers remaining after running this operation, this could be the reason.
15491   All layers meeting the criteria of an XREF-resolved layer will be processed. Your specific selection of layers is not required in this case.
15492   layer names copied to clipboard. Control-V to paste it.
15493   Error: vlax-curve-getFirstDeriv function failed on this polyline.Please report bug to 'rakesh.rao@thedesignsense.com'
15494   Error: vlax-curve-getPointAtParam function failed on this polyline.Please report bug to 'rakesh.rao@thedesignsense.com'
15495   Error: vlax-curve-getParamAtDist function failed on this polyline.Please report bug to 'rakesh.rao@thedesignsense.com'
15496   Enter (or show) the profile interval distance
15497   Enter (or show) the annotation interval distance
15498   Enter (or show) the annotation text height
15499   Enter (or show) the height text distance below profile
15500   Enter (or show) the chainage text distance below profile
15501   Enter (or show) the names distance below profile
15502   Enter (or show) the X coordinates distance
15503   Enter (or show) the Y coordinates distance
15504   Enter (or show) the segment distance annotation below profile
15505   Enter (or show) the profile [swath] width
15506   GeoTools Source Profile Report
15507   Error: ade_odattachrecord failed.
15508   Error: ade_odnewrecord failed.
15509   The file format is chosen as 'Other'. In this mode, you must specify *ALL* the fields of the format, including the ones to be ignored (I)
15510   The file format is chosen as 'Other' and 'StackedCoords' is not enabled.
15511   In this mode, you need to specify only the relevant fields from the beginning to be read.
15512   For example, PIIIINEZ with read only the first 8 fields and ignore the rest, if present
15513   The file format is chosen as 'Other' and 'StackedCoords' is enabled.
15514   In this mode, you need to specify *ALL* the fields of the record.
15515   For example, PIIIINEZII must be specified if your stacked record has a total of 10 fields, stacked one below the other
15516   In the above example, even though the last two fields are to be ignored, they must be specified for the program to
15517   detect the end of the stacked record
15518   OSNAP-nea returned nil.
15519   Unit Volume
15520   Total Volume
15521   Unit Weight
15522   Additional Resources
15523   BlockName
15524   Perform multiple automatic offset in the same direction?
15525   The image selected for the block will appear in a tile block create new from now on. The existing tile block
15526   may or may not have image defined in it.
15527   Please verify and create a new block if required.
15528   Image option deselected. This will apply in a tile block create new from now on. The existing tile block
15529   may or may not have an image defined in it.
15530   Select TILE block
15531   Enter description
15532   Select tile blocks:
15533   CP_UNCLUTTER command has been changed back to its normal(dialog-box) driven mode.
15534   CP_UNCLUTTER command is operating is command-line mode. You can switch back using the CP_UNCLUTTERDLGMODE command.
15535   CP_UNCLUTTER is a time-consuming process,
15536   it is advisable to disable AUTOSAVE and UNDO logging.
15537   This will help reduce disk swapping activity and can improve performance.
15538   Do you want to apply these setting now?
15539   Yes-Disable UNDO/AUTOSave
15540   No-Continue with existing
15541   CP_UNCLUTTER Message
15542   Both UNDO logging and AUTOSAVE have been disabled for performance improvement.
15543   Please remember to reset and switch on these settings if there is a program crash while running.
15544   In the normal course of completing the program, these settings will be automatically reverted to original values.
15545   We have reached the maximum number of iterations [
15546   ] set for this entity.
15547   This enity will be skipped now.
15548   CP_UNCLUTTER command will operate in command-line mode during the next run. You can revert to the normal mode using the CP_UNCLUTTERDLGMODE command.
15549   Only entities from layer(s) specified here will be checked under the text for obstructions. Other layers will be ignored.
15550   No layer check applied. All entities under the text will be checked for obstructions.
15551   Select layer(s) for filtering
15552   The syntax of this section is as follows:
15553   An example listing of the current set of general parameter is shown below:
15554   This section shows all the fixture names and layers that are used by the program
15555   This section shows all the opening sizes used by program so far
15556   <Length> X <Height> [this is the <Horizontal x Vertical> dimension of the tile]
15557   This section shows all the floor names used by the program so far
15558   Selected floor:
15559   select objects from layer:
15560   Pick new location for copy:
15561   Old layer:
15562   New layer:
15563   Selected floor does not match the current floor prefix
15564   and name
15565   settings
15566   Please select a floor before you can exit from this dialog. Run the CP_BUILDWALLS command or choose a valid floor from the list above.
15567   Select 'SpacePlanner' parameters INI file
15568   Selected floor does not match the current floor prefix and name settings
15569   Select footprint layer
15570   Select fixtures layer
15571   Select lofts layer
15572   Select wall layer
15573   Select window layer
15574   Select doors layer
15575   Select ventilator layer
15576   Database to extract
15577   Error: Data definition file
15578   Please select a opening type.
15579   Type        :
15580   OpenType
15581   Area        :
15582   Description :
15583   Grand Total Net Wall Area:
15584   The other case.
15585   objects do not have extended data of application:
15586   objects do not have object data of table:
15587   Please select an extended entity data application name first
15588   Please select an object table name first
15589   Points selection mode
15590   Point elevation:
15591   transferred to polyline segment #
15592   1 point was beyond search tolerance and was ignored.
15593   transferred to polyline vertex #
15594   Elevation of polyline vertex:
15595   Enter or show search distance to look for points around the line
15596   Select elevation blocks
15597   Multiple objects selection mode?
15598   Pick a boundary point:
15599   A new boundary centroid POINT object was created in the layer:
15600   its area is:
15601   A new boundary centroid BLOCK object was created in the layer:
15602   Error: A valid boundary could not be found. Please check if your surrounding polygon edges are correct, and verify if they contain SPLINE or ELLIPSE objects.
15603   These may cause problems unless the correct options are chosen.
15604   Error: The CADPower Object Table name specified
15605   does not exist in the current drawing
15606   Please choose a different table name name.
15607   Select layer for boundary polygon
15608   Select layer(s) for points, blocks, text
15609   closed polygons were created.
15610   centroid objects were created.
15611   objects selected for boundary.
15612   polygon edge objects selected.
15613   No polygon edge objects in selected layer(s)
15614   Layer selection filter :
15615   Enter or show SCAN size window
15616   Select an object to specify polygon edge layer:
15617   added to the filter list.
15618   This layer
15619   Enter or show ZOOM size window
15620   No objects in selected layer(s)
15621   The CADPower Quick Image Insert command
15622   Pick point to place the image:
15623   Pick other corner of image:
15624   The CADPower QuickHatch command
15625   Pick point for hatch
15626   (or select entity or type 'S' for settings):
15627   Error: Selected entity is an open curve and cannot be hatched.
15628   Error: Invalid entity selected for hatch.
15629   Recent hatch patterns list reset.
15630   Error: please select a hatch pattern before you can exit from this dialog.
15631   Saved hatch pattern
15632   found in registry. Hatch angle set to
15633   and scale set to
15634   Error: Image file
15635   Error: please select an image to attach before you can exit from this dialog.
15636   Specify image file to attach
15637   CAD measured angle (2d-along XY plane) is:
15638   degs
15639   Geographic bearing between the two points is:
15640   The angle from XY plane (slope of the edge) is:
15641   degrees.
15642   Select a 3d polyline, 3DFACE or 3d block entity:
15643   3DSlope computation is possible only on polylines with 3 or 4 vertices. The polyline you selected has
15644   The rotation angle of the block about the X axis is:
15645   degs, Y:
15646   degs, Z:
15647   degs.
15648   Rotation mode?
15649   Rotation axis, relative to block insertion?
15650   Enter rotation angle
15651   Rotation angle about X axis is:
15652   Rotation angle about Y axis is:
15653   Rotation angle about Z axis is:
15654   Error: You must select a 3d polyline, 3dface or 3d block entity only. You selected a
15655   just now
15656   The slope of this
15657   degrees from the horizontal
15658   ****** Command Name:
15659           Started on    :
15660           Ended   on    :
15661           Elapsed time :
15662   Error...
15663   Select block to export into DWG:
15664   Error: Cannot find the block dwg:
15665   Pick nearest reference point to move:
15666   Pick new arrow-head point:
15667   Pick new dog-leg point:
15668   Pick new text point:
15669   Select MLEADER text:
15670   Pick first [arrow-head] point of MLEADER:
15671   Pick second [dog-leg] point of MLEADER:
15672   Select existing MULTILEADER objects:
15673   Specify INI file to read
15674   Error: Please select an INI section -or- select existing MLEADERs manually before you can exit from this dialog.
15675   Processing linear objects...
15676   Pick first text alignment point:
15677   Pick second text alignment point:
15678   Alignment direction set as:
15679   Create breakline symbol.
15680   Size:
15681   Dynamic size:
15682   Linear factor:
15683   Create-on-existing:
15684   Continuous:
15685   Size: (dynamic), Dynamic size mode: Yes , Linear factor:
15686   Block symbol:
15687   Specify first point for breakline or [B]lock/[S]ize]/se[T]tings:
15688   Block Size Ttings Dynamic
15689   Specify a block name to use (or . for none)
15690   Error: There is no block by name
15691   in the current drawing.
15692   Enter (or show) size of the breakline symbol
15693   Enter linear factor scale (along the break-line, relative to Size)
15694   Continue from last drawn breakline?
15695   Create breakline symbols with different size each time?
15696   Second point for breakline symbol:
15697   Pick breakpoint <ENTER for midpoint>:
15698   Enter (or show) breakline size
15699   Compute area of selected objects
15700   Select entity to add area, [S]ubtract: [ENTER to finish]
15701   Select entity to subtract area, [A]dd: [ENTER to finish]
15702   Error: Please pick a closed spline only.
15703   This entity area has already been picked and added.
15704   Since 'AllowAgain' option is enabled, the selected entity area will be added again.
15705   This entity area has already been picked and subtracted.
15706   Since 'AllowAgain' option is enabled, the selected entity area will be subtracted again.
15707   Selected entity area:
15708   cumulative area so far:
15709   [already selected, hence ignored.]
15710   Error: Please select a closed polyline, spline or circle entity only.
15711   Curve sampling distance (for approx. curve highlighting)
15712   Allow same entity to be selected again?
15713   Enter transparency percentage [0-100]
15714   *** D A T A    P R E P A R A T I O N   Tip
15715   CP_SHAPEMANAGER command requires topologically clean, closed polygon geometry for best results.
15716   Please ensure that your polyline is indeed closed (with the closed flag).
15717   Sometimes, it may visually appear closed but it could be an open polyline.
15718   Use the CP_MPEDIT command from CADPower, if necessary, to close multiple polylines.
15719   Also ensure that your polylines have no self-intersecting or overlapping segments.
15720   Such polylines can return wrong results.
15721   Ensure that your polylines have no collinear and duplicate vertices.
15722   You can use the GT_REM_LINVERTS command from GeoTools -or- the OVERKILL command to fix collinear vertices
15723   You can use the GT_DISTANGWEED from GeoTools -or- the OVERKILL command to fix duplicated vertices.
15724   For best results, please take a moment to check your data thoroughly before running the CP_SHAPEMANAGER command
15725   Do you want to continue (Yes) or re-check your data (Re-check)?
15726   Please select a source shape to replace.
15727   Please select a target shape to replace with.
15728   TableName =
15729   Data Source Location :
15730   Data Source :
15731   Database Table Name :
15732   DataSourceLoc=
15733   DataSource=
15734   DataSourceLocation
15735   DataSource
15736   Table
15737   Program END
15738   Layer Settings
15739   restored.
15740   Please try with a different internet connection, or switch to a wifi or mobile hotspot.
15741   A LAN cable connected internet can sometimes throw up errors.
15742   CADPower cloud license manager (CP_ACTIVATECLOUDLICENSE message)
15743   GeoTools cloud license manager (GT_ACTIVATECLOUDLICENSE message)
15744   You are trying to use a FREEWARE command
15745   from CADPower, whose trial has expired.
15746   You can be eligible for a FREEWARE license of CADPower at NO COST, if you have purchased the full version of CADPower
15747   -or- If you have purchased BricsCAD from us -or- from our authorized, designated partner.
15748   Please email 'rakesh.rao@thedesignsense.com' along with the appkey for this computer to determine your elibility to
15749   receive a CADPower FREEWARE mnodule license file.
15750   DESIGNSENSE reserves the right to issue or deny a FREEWARE module license to users based on the prevailing rules
15751   and policies as on date, and the decision of the company shall be final and binding.
15752   You can generate your computer appkeys by typing 'CP_APPKEY' on the command line -or- from the menu
15753   Please email 's.langer@mervisoft-gmbh.de' along with the appkey for this computer to determine your elibility to
15754   CAD Deutschland CDIC GmbH reserves the right to issue or deny a FREEWARE module license to users based on the prevailing rules
15755   The appkey of this computer is:
15756   Your license for this appkey has expired
15757   It had a validity from
15758   Please contact 'rakesh.rao@thedesignsense.com' to obtain a new license. Charges may apply!
15759   Please contact 'cs@cad-deutschland.de' to obtain a new license. Charges may apply!
15760   Error: Cannot find GT_CP_Utilities_BC.dll utilitity in the support file search path.
15761   utility in the support file search path.
15762   The CADPower license file you are using requires you to run the latest version which is
15763   Please upgrade to the required version in order to use CADPower with this license file.
15764   Please email 'rakesh.rao@thedesignsense.com' for more info, help and technical support.
15765   Please email 'cs@cad-deutschland.de' for more info, help and technical support.
15766   Error: Cannot find GT_CP_Utilities_BC.dll utility in the support file search path.
15767   Checking GeoTools license....
15768   Your GeoTools license for this appkey has expired
15769   GeoTools appkey information copied to clipboard. You can paste it in your email body and send it to 'cs@cad-deutschland.de'
15770   CADPower appkey information copied to clipboard. You can paste it in your email body and send it to 'cs@cad-deutschland.de'
15771   Polygon Number
15772   Centroid-X
15773   Centroid-Y
15774   Centroid-Z
15775   Full Area
15776   Exclusion Area
15777   Net Area
15778   Incl.Angle
15779   Direction
15780   Seg.Slope(%)
15781   Seg.Slope(degs)
15782   Direction(Bearing)
15783   Polyline Statistics Table
15784   Totals
15785   Converted output file
15786   Please be aware that only the fields mentioned as P, N, E, Z and D will be considered in the converted export. Other fields, if any,  will be ignored.
15787   Finished ground alignment coordinates file
15788   Warning: There are already
15789   objects in the layer
15790   specified for bore-hole sections.
15791   Do you want to continue? [new section lines will be created now]
15792   specified for bore-hole points.
15793   Do you want to continue? [new bore-hole points will be created now]
15794   created with
15795   attributes whose tag names are:
15796   CADPower Object Table:
15797   Error: CADPower Object Table:
15798   A bore-hole section with
15799   bore-hole drill points created.
15800   Bore-hole drill log file:
15801   Error: the temporary UCS could not be created.
15802   Block moved by
15803   1 block ignored. No XY values were found in attributes.
15804   SHAPE name(Count#)
15805   <Area>
15806   <Length>
15807   <Description>
15808   <Key Geometry Dimensions>
15809   Select MLEADER objects to update
15810   Select an MLEADER object (in order) to update [ENTER to finish]:
15811   The MLEADER object is already selected once.
15812   Error: Selected object is not an MLEADER.
15813   Select MLEADER object, after which to insert new MLEADER object:
15814   Select MLEADER object to delete:
15815   Error: Please select an MULTILEADER object only.
15816   Select MLEADERs [for update]
15817   Old MLEADER text:
15818   Ask for new text insertion point each time?
15819   Num-Objects
15820   Enter (or show) distance between two vertices
15821   Select entity to pick area from (or [S]ettings): [ENTER to specify area points]:
15822   Error: Please select a line, polyline, arc, circle or spline object only.
15823   Pick first point to measure area from:
15824   Pick next point to measure area to [ENTER to finish]:
15825   We need you to pick a minimum of 3 points to define an area.
15826   Pick first point to measure length from:
15827   Pick second point to measure length to:
15828   Original area=
15829   Area property cannot be obtained for this entity
15830   Pan -or- Zoom as required and press ENTER when done.
15831   Select an entity to slide / copy:
15832   Copy again? (or enter # of times to copy):
15833   Enter or show MLEADER length
15834   The [*RECORD] section defines the structure of the data that you are creating.
15835   This is the same format of INI file as used by the CP_DATAMAN command.
15836   You are defining a database here to store your linear material definition. Think of this as the database name.
15837   For example: FIELD=Weight per unit length,Real,110.0
15838   For example: FIELD=Supplier, String, Polycab
15839   For example: FIELD=Width, Real, 10.0
15840   CADPower Object table name
15841   created from parameter file:
15842   The CADPower Object table name
15843   already exists. A new table was not created.
15844   Select objects to attach linear quantities data [ENTER to select by layer]:
15845   Select objects to edit linear quantities data [ENTER to select by layer]:
15846   Select objects to compute linear quantities [ENTER to select by layer]:
15847   objects selected for editing.
15848   Quantities Table
15849   A new INI file
15850   containing the linear quantity info has been created.
15851   A new CADPower object table also will be created now.
15852   You can use the CP_ATTACHDATA command (CADPower -> Build -> Object data table -> Attach object data) to attach this object data to your linear entities.
15853   There is an 'Attach data' option provided in this dialog box also, which does the same.
15854   The generic CADPower Object table
15855   does not exist, and will be created now.
15856   Area of triangulated area [raw dwg units]:
15857   One triangle was completely outside the TIN boundary
15858   One triangle overlapped existing TIN boundary.
15859   Do you want to delete the
15860   wrongly created triangles.
15861   ** WARNING **: There is a mis-match between the original area of the polygon and the added up areas of the triangles.
15862   Original curve area:
15863   added up triangle areas:
15864   Some triangles *MAY NOT* be depicted correctly. They are shown in cyan color.
15865   Please correct them manually and run the CP_TRIANGULATE_MEA_MANUAL command to complete the annotations.
15866   CADPower Measurement Tools message
15867   Error: Selected polyline is open. Please select an closed polyline only.
15868   Error: Please select a closed polyline object only.
15869   SR.NO
15870   BASE
15871   Pick point to place triangulation table:
15872   Select a triangle to annotate:
15873   CP_SHAPEMANAGER Message
15874   Pick arrow-head location of MLEADER:
15875   Pick leader landing point of MLEADER:
15876   Specify statistics output file-name
15877   Text content
15878   Number of occurences
15879   X Scale factor
15880   Angle
15881   Table of angle orientations and their linear lengths
15882   HATCH patterns found in this drawing
15883   Number of HATCH patterns
15884   block INSERT objects
15885   block INSERTs
15886   anonymous INSERT objects
15887   Anonymous blocks
15888   <Pattern-Name>=Cost-Per-Sq-Unit,Time-Per-Sq-Unit
15889   Select polylines to align with the first-last vertex direction.
15890   vertices moved by an average distance of
15891   1 polyline with 2 vertices ignored.
15892   Error: Cannot find the map signoff block 'GT_DOC_SIGNOFF.dwg' in the search path.
15893   Place a map sign-off block:
15894   Place a map boundaries annotation block:
15895   Error: Cannot find the map signoff block 'GT_PROP_BOUNDARY.dwg' in the search path.
15896   Place a map scalebar block:
15897   Error: Cannot find the map scale-bar 'GTCP_SCALEBAR.dwg' in the search path.
15898   Roaming [root] Folder already exists.
15899   Volatile Registry does not exist, stitching from c:/Users
15900   Elevation
15901   X-coordinates
15902   Y-coordinates
15903   Segment distance
15904   Create L-Section profile from selected data from Excel.
15905   Please select from Excel or a text file the data that contains the chainage and elevation values.
15906   Click on 'Ok' when done.
15907   rows and
15908   Please specify the column number within your selection, where the cross section number is available.
15909   This column is NOT MANDATORY and can be left as 0 the data is not available in the selection.
15910   Please specify the column number within your selection, where the elevation (Z-level) information is is available.
15911   Atleast one column showing the elevation is MANDATORY. There are five such columns provided to show multiple heights, if available. The remaining four are optional.
15912   Please specify the column number within your selection, where the chainage information is available.
15913   This column is MANDATORY and cannot be left blank.
15914   Pick start point of L-section:
15915   Additional
15916   information dialog boxes showing floating license status will pop up each time your CAD application starts.
15917   information dialog boxes showing floating license status will NOT pop up each time your CAD application starts.
15918   A number of CADPower shortcut macros will be enabled after the next restart of your CAD application
15919   The currently defined CADPower shortcut macros will be disabled after the next restart of your CAD application
15920   This command is not relevant in GeoTools
15921   CUI/X files will be re-loaded each time your CAD application restarts [enables a reread/reload each time].
15922   CUI/X files will NOT be re-loaded each time your CAD application restarts [existing CUI/X load continues].
15923   will show not display any CUI/X user interface after the next re-start
15924   will show the normal CUI/X user interface after the next re-start
15925   Some of the
15926   commands have been enabled with voice-assist mode. This is an experimental feature.
15927   The voice-assist mode in
15928   commands have been disabled.
15929   When you save your drawing with Control-S, the .BAK file created will be moved to the specified folder
15930   Use CP_MOVEBAK command to configure further.
15931   When you save your drawing with Control-S, the .BAK file created will NOT be moved.
15932   It will stay in the DWG folder only [default behavior].
15933   This enables the right-click menu behavior on an empty screen or on entities.
15934   This disables the right-click menu behavior on an empty screen or on entities.
15935   This feature is enabled only in the English version of BricsCAD.
15936   This feature is enabled only in the English version of CADPower.
15937   AUTOSNAP system variable set to 127 (default), and all options turned on.
15938   BricsCAD only: The commandline miniframe will be disabled.
15939   BricsCAD only: The commandline miniframe will be enabled.
15940   Counter clock-wise angles will be measured positive [default behavior].
15941   Clock-wise angles will be measured positive [changed from default].
15942   During the next restart of your CAD application,
15943   will search for the first available license file on the support path, even if it is found in the USER/APPDATA folder [default location].
15944   This over-ride may be required in custom deployments, usually large, multi-user setups, in order to reduce the license management / administration tasks
15945   will search for the license file first from the USER/APPDATA folder, then the application installation folder, and then the support file search path.
15946   This is the default behavior and how
15947   works as per design.
15948   will not check for any updates from the server.
15949   will check for updates on the server during each restart of your CAD application -or- as per the frequency entered in the dialog box.
15950   installation folder name will be added to the top of the 'Support files search path' list [highest priority]
15951   installation folder name will be added to the bottom of the 'Support files search path' list [least priority]
15952   A two-line command prompt window will be displayed.
15953   May require BricsCAD to be restarted.
15954   Grips display within blocks enabled.
15955   Grips display within blocks disabled.
15956   Select template file to use
15957   Double clicking on a text will now edit the text in its own location, without a dialog box popping up.
15958   Double clicking on a text will now allow editing the text in a dialog box.
15959   Please be aware that this may make your DWG data look cluttered.
15960   A crash dump file will be created if BricsCAD crashes.
15961   You can view the crash report using the CP_CRASHREPORTMGR command in CADPower.
15962   A crash dump file will not be created [disabled]
15963   The CADPower installation path has been added to the default support file search path.
15964   The CADPower installation path has been removed from the default support file search path.
15965   The GeoTools installation path has been added to the default support file search path.
15966   The GeoTools installation path has been removed from the default support file search path.
15967   Unit Time/weight
15968   Total Time/weight
15969   Code
15970   Index
15971   Visibility Attribute Value
15972   BOQ Table
15973   ERP Drawing Name
15974   ERP Drawing Revision number
15975   ERP Date of Export
15976   ERP Time of Export
15977   The system variable
15978   The operating language of CADPower is:
15979   (not defined)
15980   The operating language of GeoTools is:
15981   Please select only the numeric values, please DO NOT select the title row, if any. This causes the program logic to fail.
15982   The GT_BUFFERPOLY_SPLIT command requires that all data be topologically as clean as possible
15983   This means that there must be no overlapping segments, duplicated vertices, kinks or knots in your polygon data.
15984   It is the responsibility of the user to ensure that these are fixed before using the buffer polygon split tool.
15985   There are several tools in GeoTools to ensure that your data can be cleaned up in multiple ways.
15986   Here is a recommended list of some of them which are useful for data preparation and cleanup:
15987   Use this tool to get rid of any duplicated objects. It will not only ensure you have successful
15988   processing, but will also speed up the processing operations, which can sometimes be time consuming
15989   This is a comprehensive angle and distance based vertex optimization tool (weed in GIS parlance)
15990   Use this tool to specify an optimal distance parameter so you can remove unecessarily too much data
15991   and keep only what is required.
15992   Use this tool to remove redundant vertices which are all in a straight line. They don't add any value
15993   to the polygons being procressed, except to increase processing time
15994   If you have knots in your polygon geometry, the GT_KINK command helps to identify them. You need to
15995   manually fix it thereafter.
15996   Select a buffer polygon boundary:
15997   Error: Please select a closed polyline for buffer polygon boundary.
15998   Select layer for splitted polygons outside the buffer
15999   Select layer for splitted polygons inside the buffer
16000   Specify CSV export file for split polygon info
16001   Error: Please select a valid CSV file for export.
16002   file
16003   file.
16004   Select layer to place polygons inside buffer poly
16005   Select layer to place polygons outside buffer poly
16006   Select layer where closed parcels exist
16007   Select layer for parcel name text
16008   polylines contained wholly inside the buffer polygon.
16009   Processing polygons along alignment intersections...
16010   intersections with the buffer polygon.
16011   A polygon with
16012   intersections ignored.
16013   1 open polyline in the base parcel layer found and ignored.
16014   Invalid entry, only +ve values permitted.
16015   Invalid entry, only -ve values permitted.
16016   Invalid entry, only zero or +ve values allowed.
16017   Invalid entry, only zero or -ve values allowed.
16018   Copied to clipboard
16019   records for editing
16020   Select a file to attach
16021   is already selected and will not be added.
16022   Select folder to browse
16023   PL_BreakX Message: Polyline break was NOT successful.
16024   Picked polyline is not on layer :
16025   Picked object is not a polyline.
16026   1 3d line found and ignored.
16027   Pre-processing polyline objects...
16028   1 3d polyline found and ignored.
16029   Joining POLYLINEs :
16030   Joining POLYLINEs: (100% over)
16031   Exploding polylines/3dfaces....
16032   Updating polyline with
16033   vertices, please wait...
16034   Processing vertices...
16035   distinct AutoCAD versions installed on this computer.
16036   AutoCAD installations of version
16037   versions installed on this computer.
16038   distinct BricsCAD versions installed on this computer.
16039   Error: There is no cloud enabled license available for this computer. Please contact 'rakesh.rao@thedesignsense.com' for a license.
16040   Error: Could not access
16041   cloud license. Maybe there is no active internet connection?
16042   A cloud license is specified, so
16043   cannot continue until you connect to the internet.
16044   Cannot find the file
16045   Error: Encryption NOT successful.
16046   Error: Could not open temporary file.
16047   Internal error: Windows TEMP directory has not been set. Please set this directory before resuming.
16048   is not a valid object type for centroid computation.
16049   There was an error in determining the object extents in the GE_GetObjectBoundingBox function.
16050   Please select a closed polyline only.
16051   Output: Splitted area file:
16052   created sucessfully.
16053   Polygon number, Inside buffer polygon area,Outside buffer polygon area,Undivided area,Inside area-%,Outside area-%,Village-Name
16054   Error: Custom format cannot contain an ignorable character 'I' when the 'Convert' option is chosen.
16055   Error: There cannot be more than one description field 'D' when the 'Convert' option is chosen.
16056   File not found:
16057   Choose language CUI to load
16058   Choose language CUI to unload / load [reset]
16059   GeoTools license has already expired on
16060   Error: Text Style
16061   is not defined.
16062   Text informatiomn from list saved as
16063   -Or- you don't have permission to create a files in this folder.
16064   Created file:
16065   Change
16066   operating language
16067   Specify a file name to save the listed information
16068   Enter or show interpolation distance
16069   Enter or show attribute height
16070   Enter or show distance to slide in X direction
16071   Enter or show distance to slide in Y direction
16072   Enter or show distance to elevation text near the contours
16073   Enter or show length of the rectangle
16074   Enter or show width (height) of the rectangle
16075   Invalid input. Please try again.
16076   Pick other corner (or type Height dimension):
16077   Draw a Rectangle
16078   Pick lower left corner:
16079   Show direction and lower right corner of rectangle (or D for dimensions):
16080   Draw a Rectangle, specifying the center and one edge
16081   Pick center point of the rectangle:
16082   Specify rotation angle.
16083   Rectangle with length:
16084   Specify a new center point for rectangle each time
16085   Drag-rotate the rectangle after it is placed
16086   Pick a corner of the rectangle
16087   Enter or show value for selected property
16088   Enter or show vertex movement distance in X direction
16089   Enter or show vertex movement distance in Y direction
16090   Enter or show vertex movement distance in Z direction
16091   Enter or show dynamic vertex movement distance in X direction
16092   Enter or show dynamic vertex movement distance in Y direction
16093   Enter or show dynamic vertex movement distance in Z direction
16094   Enter or show dynamic custom vertex movement distance
16095   Enter or show contour label text height
16096   Enter or show contour label spacing distance
16097   WIPEOUTs deleted from layer:
16098   Enter or show hatch line spacing
16099   Enter or show width of hatch line for vertical fronts
16100   Enter or show hatch width
16101   Enter or show offset distance for each iteration
16102   Success: Created a polygon with area
16103   Error: The boundary command has failed. Please make sure that there is a closed space enclosing the bounding objects and the movable guide line.
16104   Error: The movable guide line should be a LINE or polyline entity only.
16105   Enter offset distance from existing guide line
16106   Error: The movable guide line LINE or polyline entity only.
16107   Select a new guide line:
16108   New guideline: From point:
16109   Guideline specification?
16110   Pick direction for drawing the lots:
16111   Pick a start point inside the next probable polygon:
16112   Target area is LESS than than the EXISTSING area of bounded polygon. Lot size must decrease with each iteration.
16113   Target area is MORE than the EXISTING area of bounded polygon. Lot size must increase with each iteration.
16114   Enter target area of the lot to create
16115   Required lot area:
16116   Enclosing polygon area:
16117   Pick a start point inside the first probable polygon:
16118   Select movable guide line
16119   Select bounding polygon objects:
16120   Create new polygon(s) around picked point?
16121   Get text label settings from CP_CALCAREA command?
16122   Enter polygon name
16123   Layer for closed polygon labels:
16124   Select layer for closed polygon labels
16125   Enter layer for closed polygon labels (~ or ? for list)
16126   Error: There are no objects found matching boundary selection in layer(s):
16127   There are no polygons possible matching the specified criteria in layer(s):
16128   area:
16129   Area Units:
16130   items found.
16131   Pick label point:
16132   Currently visible entities will be considered for boundary detection. ZOOM in/out if necessary
16133   Layer for closed polygons:
16134   Select layer for closed polygons
16135   Enter layer for closed polygons (~ or ? for list)
16136   Layer(s) for polygon edges:
16137   Select layer(s) to process
16138   Enter layers to process (~ or ? for list)
16139   Search all layers for polygon edges?
16140   Enter detailed parameters setup?
16141   X Scale factor:
16142   Y Scale factor:
16143   Rotation angle:
16144   Z Scale factor:
16145   Pick point to place block:
16146   Enter X Scale factor:
16147   Enter Y Scale factor:
16148   Error : Cannot find block:
16149   .dwg in the support path
16150   *** P E R F O R M A N C E  Tip
16151   CP_DWGAUDIT is a time-consuming process,
16152   CP_DWGAUDIT Message
16153   Scanning blocks list....
16154   Sorting blocks list....
16155   This command does the following:
16156   All blocks named A$/ZW$ ... will be exploded automatically if there is exactly 1 insertion of such a block.
16157   If there are more than 1 insertions of such blocks, user will be asked before exploding the same, or alternatively,
16158   an option is provided to rename them
16159   Blocks without attributes will be ignored.
16160   *** Other important notes ***
16161   Text labels for parcels and village names must be as TEXT entities, not MTEXT.
16162   There must be only one TEXT entity in each parcel text layer or village name text layer.
16163   More than one TEXT may cause errors or cause the program to stop.
16164   You must correct the data before re-starting
16165   GT_BUFFERPOLY_SPLIT message
16166   GT_BUFFERPOLY_SPLIT can be a time-consuming process on large data-sets
16167   Select layer name for village (or county) name (text labels)
16168   Select layer name for village (or county) polygons
16169   <none>
16170   (not found)
16171   Error: There are
16172   TEXT objects found inside this polygon.
16173   The GT_BUFFERPOLY_SPLIT command expects only one text label to be present, which represents the county (or village) name.
16174   Please correct this mistake and re-run the GT_BUFFERPOLY_SPLIT command again.
16175   Error: There is no village name text found inside this polygon.
16176   GT_CCPOLY can be a time-consuming process on large data-sets
16177   GT_CCPOLY Message
16178   Scan size:
16179   column number
16180   There are no pre-selected points for processing.
16181   point objects selected for processing.
16182   Select layer(s) for points
16183   Once the point is processed, it will be moved to a layer with an '_PROCESSED' suffix
16184   This will help manage large data-sets to be processed in parts easily by segregating processed and to-be-processed points
16185   Automatic scanning will be made as per the specified scan window distance, and closed polygons will be created.
16186   This is a time-consuming and a lesser efficient method than selecting points for polygon creation
16187   Use this method only if you have no points data already as reference for polygon building.
16188   After clicking 'Ok', You will be asked to select points, blocks or text around which a closed polygon will be created.
16189   Processing village boundaries...
16190   1 open polyline in the village boundary layer was ignored.
16191   Points layer selection filter is not set.
16192   There are no INI sections in this file to edit.
16193   If you have made changes to the sections in your INI file, please click the 'Yes' button
16194   here to commit these changes to the INI file, and exit this dialog.
16195   Click 'No' to exit without saving.
16196   Have you saved your edits?
16197   Edit token values
16198   INI file name to save
16199   saved [on disk].
16200   Enter or show width of right-of-way
16201   Pick start point of clothoid curve:
16202   Selected object is:
16203   and slope at the point is:
16204   slope at picked point could not be determined.
16205   Deflection angle between each point [degrees]
16206   Length of the clothoid curve (L)
16207   Radius of the curve at exit (R)
16208   The computed value of the homothetic [flatness] parameter is:
16209   The clothoid curvature gradient is 1 in
16210   Clothoid parameter [sqrt (L*R)]
16211   Enter turn direction
16212   Yes, download ZIP
16213   download format
16214   will be downloaded via your default browser now. You must double-click and install the same yourself.
16215   will be dowloaded via your default browser now. You must extract the ZIP file and copy the contents to the desired folder.
16216   The EXE download is used for a standard, default installation.
16217   This will enable demand-loading of
16218   on all platforms where it is supported.
16219   The ZIP download is useful for a customized installation.
16220   Use this option when you want to prevent demand-loading during each update, -or- if you want to configure multiple plugins using the same startup LSP file.
16221   The CADPower license file you are using requires you to run CADPower V
16222   or higher.
16223   The GeoTools license file you are using requires you to run the latest version which is
16224   Please upgrade to the required version in order to use GeoTools with this license file.
